<?xml version="1.0" encoding="utf-8"?>
<datafile>
  <header>
    <name>Sega System 32</name>
    <description>Sega System 32 datafile extracted from mame</description>
    <category>MAME Arcade</category>
    <version>0.226</version>
    <date>20201109</date>
    <author>Eric Bole-Feysot</author>
    <homepage>Romcenter Home Page</homepage>
    <url>http://www.romcenter.com/</url>
    <comment>Datafile made with Romcenter rom manager</comment>
  </header>
  <machine name="alien3" sourcefile="segas32.cpp">
    <description>Alien3: The Gun (World)</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15943.ic17" size="262144" crc="ac4591aa" sha1="677155a3ebdac6602525e06adb25d287eaf9e089" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15942.ic8" size="262144" crc="a1e1d0ec" sha1="10d8d2235a67a4ba475fe98124c6a4a5311592b5" region="mainpcb:maincpu" offset="80000" />
    <rom name="mpr-15855.ic18" size="524288" crc="a6fadabe" sha1="328bbb54651eef197ba13f1bd9228f3f4de7ee5e" region="mainpcb:maincpu" offset="100000" />
    <rom name="mpr-15854.ic9" size="524288" crc="d1aec392" sha1="f48804fe0151e83ad45e912b55db8ae8ddebd2ad" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-15859a.ic36" size="262144" crc="91b55bd0" sha1="23b85a006a91c2a5eb1cee14172fd0d8b7732518" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15858.ic35" size="1048576" crc="2eb64c10" sha1="b2dbe86b82e889f4a9850cf4aa6596a139c1c3d6" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15857.ic34" size="1048576" crc="915c56df" sha1="7031f937c826af17caf7ec8cbb6155d0a55bd38a" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15856.ic24" size="1048576" crc="a5ef4f1f" sha1="e8da7a995955e80872a25bd75465c590b649cfab" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-15863.ic14" size="2097152" crc="9d36b645" sha1="2977047780b615b64c3b4aec78fef0643d40490e" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15862.ic5" size="2097152" crc="9e277d25" sha1="9f191484a42391268306a8d2d95c340ce8b2d6cd" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15864.ic32" size="2097152" crc="58207157" sha1="d1b0c7edac8b89b1322398d4cd3a976a88bc0b56" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15866.ic30" size="2097152" crc="9c53732c" sha1="9aa5103cc10b4927c16e0cf102b64a15dd038756" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15868.ic28" size="2097152" crc="62d556e8" sha1="d70cab0881784a3d4dd06d0c99587ca6054c2dc4" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15870.ic26" size="2097152" crc="d31c0400" sha1="44c1b2e5236d894d31ff72552a7ad50270dd2fad" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15865.ic31" size="2097152" crc="dd64f87b" sha1="cfa96c5f2b1221706552f5cef4aa7c61ebe21e39" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15867.ic29" size="2097152" crc="8cf9cb11" sha1="a77399fccee3f258a5716721edd69a33f94f8daf" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15869.ic27" size="2097152" crc="dd4b137f" sha1="7316dce32d35bf468defae5e6ed86910a37a2457" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15871.ic25" size="2097152" crc="58eb10ae" sha1="23f2a72dc7b2d7b5c8a979952f81608296805745" region="mainpcb:sprites" offset="800006" />
    <rom name="93c45_eeprom.ic76" size="128" crc="6e1d9df3" sha1="2fd818bc393fb96e945fa37a63c8a3c4aff2f79f" region="mainpcb:eeprom" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="stick" player="1" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
      <control type="stick" player="2" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="alien3j" sourcefile="segas32.cpp" cloneof="alien3" romof="alien3">
    <description>Alien3: The Gun (Japan)</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15861.ic17" size="262144" crc="e970603f" sha1="b67cf4cb5269d808ff8adc007202cb6e18d5b6a9" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15860.ic8" size="262144" crc="9af0d996" sha1="3fb06947712947da4830200db2382d9c433a18a9" region="mainpcb:maincpu" offset="80000" />
    <rom name="mpr-15855.ic18" merge="mpr-15855.ic18" size="524288" crc="a6fadabe" sha1="328bbb54651eef197ba13f1bd9228f3f4de7ee5e" region="mainpcb:maincpu" offset="100000" />
    <rom name="mpr-15854.ic9" merge="mpr-15854.ic9" size="524288" crc="d1aec392" sha1="f48804fe0151e83ad45e912b55db8ae8ddebd2ad" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-15859.ic36" size="262144" crc="7eeda800" sha1="d0599730a8a2adbed08fec4160b8b3963e8ac0f6" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15858.ic35" merge="mpr-15858.ic35" size="1048576" crc="2eb64c10" sha1="b2dbe86b82e889f4a9850cf4aa6596a139c1c3d6" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15857.ic34" merge="mpr-15857.ic34" size="1048576" crc="915c56df" sha1="7031f937c826af17caf7ec8cbb6155d0a55bd38a" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15856.ic24" merge="mpr-15856.ic24" size="1048576" crc="a5ef4f1f" sha1="e8da7a995955e80872a25bd75465c590b649cfab" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-15863.ic14" merge="mpr-15863.ic14" size="2097152" crc="9d36b645" sha1="2977047780b615b64c3b4aec78fef0643d40490e" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15862.ic5" merge="mpr-15862.ic5" size="2097152" crc="9e277d25" sha1="9f191484a42391268306a8d2d95c340ce8b2d6cd" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15864.ic32" merge="mpr-15864.ic32" size="2097152" crc="58207157" sha1="d1b0c7edac8b89b1322398d4cd3a976a88bc0b56" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15866.ic30" merge="mpr-15866.ic30" size="2097152" crc="9c53732c" sha1="9aa5103cc10b4927c16e0cf102b64a15dd038756" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15868.ic28" merge="mpr-15868.ic28" size="2097152" crc="62d556e8" sha1="d70cab0881784a3d4dd06d0c99587ca6054c2dc4" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15870.ic26" merge="mpr-15870.ic26" size="2097152" crc="d31c0400" sha1="44c1b2e5236d894d31ff72552a7ad50270dd2fad" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15865.ic31" merge="mpr-15865.ic31" size="2097152" crc="dd64f87b" sha1="cfa96c5f2b1221706552f5cef4aa7c61ebe21e39" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15867.ic29" merge="mpr-15867.ic29" size="2097152" crc="8cf9cb11" sha1="a77399fccee3f258a5716721edd69a33f94f8daf" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15869.ic27" merge="mpr-15869.ic27" size="2097152" crc="dd4b137f" sha1="7316dce32d35bf468defae5e6ed86910a37a2457" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15871.ic25" merge="mpr-15871.ic25" size="2097152" crc="58eb10ae" sha1="23f2a72dc7b2d7b5c8a979952f81608296805745" region="mainpcb:sprites" offset="800006" />
    <rom name="93c45_eeprom.ic76" merge="93c45_eeprom.ic76" size="128" crc="6e1d9df3" sha1="2fd818bc393fb96e945fa37a63c8a3c4aff2f79f" region="mainpcb:eeprom" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="stick" player="1" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
      <control type="stick" player="2" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="alien3u" sourcefile="segas32.cpp" cloneof="alien3" romof="alien3">
    <description>Alien3: The Gun (US, Rev A)</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15941.ic17" size="262144" crc="bf8c257f" sha1="d08b77d2e3f5af0da7e7d8727fbe7fc0eb1153ff" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15940a.ic8" size="262144" crc="8840b51e" sha1="0aa6945000676b1adc535b1557a1455d62aed9f5" region="mainpcb:maincpu" offset="80000" />
    <rom name="mpr-15855.ic18" merge="mpr-15855.ic18" size="524288" crc="a6fadabe" sha1="328bbb54651eef197ba13f1bd9228f3f4de7ee5e" region="mainpcb:maincpu" offset="100000" />
    <rom name="mpr-15854.ic9" merge="mpr-15854.ic9" size="524288" crc="d1aec392" sha1="f48804fe0151e83ad45e912b55db8ae8ddebd2ad" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-15859a.ic36" merge="epr-15859a.ic36" size="262144" crc="91b55bd0" sha1="23b85a006a91c2a5eb1cee14172fd0d8b7732518" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15858.ic35" merge="mpr-15858.ic35" size="1048576" crc="2eb64c10" sha1="b2dbe86b82e889f4a9850cf4aa6596a139c1c3d6" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15857.ic34" merge="mpr-15857.ic34" size="1048576" crc="915c56df" sha1="7031f937c826af17caf7ec8cbb6155d0a55bd38a" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15856.ic24" merge="mpr-15856.ic24" size="1048576" crc="a5ef4f1f" sha1="e8da7a995955e80872a25bd75465c590b649cfab" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-15863.ic14" merge="mpr-15863.ic14" size="2097152" crc="9d36b645" sha1="2977047780b615b64c3b4aec78fef0643d40490e" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15862.ic5" merge="mpr-15862.ic5" size="2097152" crc="9e277d25" sha1="9f191484a42391268306a8d2d95c340ce8b2d6cd" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15864.ic32" merge="mpr-15864.ic32" size="2097152" crc="58207157" sha1="d1b0c7edac8b89b1322398d4cd3a976a88bc0b56" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15866.ic30" merge="mpr-15866.ic30" size="2097152" crc="9c53732c" sha1="9aa5103cc10b4927c16e0cf102b64a15dd038756" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15868.ic28" merge="mpr-15868.ic28" size="2097152" crc="62d556e8" sha1="d70cab0881784a3d4dd06d0c99587ca6054c2dc4" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15870.ic26" merge="mpr-15870.ic26" size="2097152" crc="d31c0400" sha1="44c1b2e5236d894d31ff72552a7ad50270dd2fad" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15865.ic31" merge="mpr-15865.ic31" size="2097152" crc="dd64f87b" sha1="cfa96c5f2b1221706552f5cef4aa7c61ebe21e39" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15867.ic29" merge="mpr-15867.ic29" size="2097152" crc="8cf9cb11" sha1="a77399fccee3f258a5716721edd69a33f94f8daf" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15869.ic27" merge="mpr-15869.ic27" size="2097152" crc="dd4b137f" sha1="7316dce32d35bf468defae5e6ed86910a37a2457" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15871.ic25" merge="mpr-15871.ic25" size="2097152" crc="58eb10ae" sha1="23f2a72dc7b2d7b5c8a979952f81608296805745" region="mainpcb:sprites" offset="800006" />
    <rom name="93c45_eeprom.ic76" merge="93c45_eeprom.ic76" size="128" crc="6e1d9df3" sha1="2fd818bc393fb96e945fa37a63c8a3c4aff2f79f" region="mainpcb:eeprom" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="stick" player="1" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
      <control type="stick" player="2" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="arabfgt" sourcefile="segas32.cpp">
    <description>Arabian Fight (World)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14609.ic8" size="131072" crc="6a43c7fb" sha1="70e9f9fa5f867f0455d62ff2690ad19055d79363" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14592.ic18" size="262144" crc="f7dff316" sha1="338690a1404dde6e7e66067f23605a247c7d0f5b" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14591.ic9" size="262144" crc="bbd940fb" sha1="99c17aba890935eaf7ea468492da03103288eb1b" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14596.ic36" size="131072" crc="bd01faec" sha1="c909dcb8ef2672c4b0060d911d295e445ca311eb" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14595f.ic35" size="1048576" crc="5173d1af" sha1="dccda644488d0c561c8ff7fa9619bd9504d8d9c6" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14594f.ic34" size="1048576" crc="01777645" sha1="7bcbe7687bd80b94bd3b2b3099cdd036bf7e0cd3" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14593f.ic24" size="1048576" crc="aa037047" sha1="5cb1cfb235bbbf875d2b07ac4a9130ba13d47e57" region="mainpcb:soundcpu" offset="300000" />
    <rom name="epr-14468-01.u3" size="65536" crc="c3c591e4" sha1="53e48066e85b61d0c456618d14334a509b354cb3" region="mainpcb:mcu" offset="0" />
    <rom name="mpr-14599f.ic14" size="2097152" crc="94f1cf10" sha1="34ec86487bcb6726c025149c319f00a854eb7a1d" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14598f.ic5" size="2097152" crc="010656f3" sha1="31619c022cba4f250ce174f186d3e34444f60faf" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14600f.ic32" size="2097152" crc="e860988a" sha1="328581877c0890519c854f75f0976b0e9c4560f8" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14602.ic30" size="2097152" crc="64524e4d" sha1="86246185ab5ab638a73991c9e3aeb07c6d51be4f" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14604.ic28" size="2097152" crc="5f8d5167" sha1="1b08495e5a4cc2530c2895e47abd0e0b75496c68" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14606.ic26" size="2097152" crc="7047f437" sha1="e806a1cd73c96b33e8edc64e41d99bf7798103e0" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14601f.ic31" size="2097152" crc="a2f3bb32" sha1="1a60975dead5faf08ad4e9a96a00f98664d5e5ec" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-14603.ic29" size="2097152" crc="f6ce494b" sha1="b3117e34913e855c035ebe37fbfbe0f7466f94f0" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-14605.ic27" size="2097152" crc="aaf52697" sha1="b502a37ae68fc08b60cdf0e2b744898b3474d3b9" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-14607.ic25" size="2097152" crc="b70b0735" sha1="9ef2da6f710bc5c2c7ee30dc144409a61dbe6646" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_v25" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <device_ref name="mb8421" />
    <device_ref name="v25" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="mainpcb:mcu" name="NEC V25" clock="10000000" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="2" service="yes">
      <control type="joy" player="1" buttons="2" ways="8" />
      <control type="joy" player="2" buttons="2" ways="8" />
      <control type="joy" player="3" buttons="2" ways="8" />
      <control type="joy" player="4" buttons="2" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="arabfgtj" sourcefile="segas32.cpp" cloneof="arabfgt" romof="arabfgt">
    <description>Arabian Fight (Japan)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14597.ic8" size="131072" crc="7a6fe222" sha1="f730e9d44ad20dbaa59f6311a077c889e0aec8e4" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14592.ic18" merge="epr-14592.ic18" size="262144" crc="f7dff316" sha1="338690a1404dde6e7e66067f23605a247c7d0f5b" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14591.ic9" merge="epr-14591.ic9" size="262144" crc="bbd940fb" sha1="99c17aba890935eaf7ea468492da03103288eb1b" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14596.ic36" merge="epr-14596.ic36" size="131072" crc="bd01faec" sha1="c909dcb8ef2672c4b0060d911d295e445ca311eb" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14595f.ic35" merge="mpr-14595f.ic35" size="1048576" crc="5173d1af" sha1="dccda644488d0c561c8ff7fa9619bd9504d8d9c6" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14594f.ic34" merge="mpr-14594f.ic34" size="1048576" crc="01777645" sha1="7bcbe7687bd80b94bd3b2b3099cdd036bf7e0cd3" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14593f.ic24" merge="mpr-14593f.ic24" size="1048576" crc="aa037047" sha1="5cb1cfb235bbbf875d2b07ac4a9130ba13d47e57" region="mainpcb:soundcpu" offset="300000" />
    <rom name="epr-14468-01.u3" merge="epr-14468-01.u3" size="65536" crc="c3c591e4" sha1="53e48066e85b61d0c456618d14334a509b354cb3" region="mainpcb:mcu" offset="0" />
    <rom name="mpr-14599f.ic14" merge="mpr-14599f.ic14" size="2097152" crc="94f1cf10" sha1="34ec86487bcb6726c025149c319f00a854eb7a1d" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14598f.ic5" merge="mpr-14598f.ic5" size="2097152" crc="010656f3" sha1="31619c022cba4f250ce174f186d3e34444f60faf" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14600f.ic32" merge="mpr-14600f.ic32" size="2097152" crc="e860988a" sha1="328581877c0890519c854f75f0976b0e9c4560f8" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14602.ic30" merge="mpr-14602.ic30" size="2097152" crc="64524e4d" sha1="86246185ab5ab638a73991c9e3aeb07c6d51be4f" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14604.ic28" merge="mpr-14604.ic28" size="2097152" crc="5f8d5167" sha1="1b08495e5a4cc2530c2895e47abd0e0b75496c68" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14606.ic26" merge="mpr-14606.ic26" size="2097152" crc="7047f437" sha1="e806a1cd73c96b33e8edc64e41d99bf7798103e0" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14601f.ic31" merge="mpr-14601f.ic31" size="2097152" crc="a2f3bb32" sha1="1a60975dead5faf08ad4e9a96a00f98664d5e5ec" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-14603.ic29" merge="mpr-14603.ic29" size="2097152" crc="f6ce494b" sha1="b3117e34913e855c035ebe37fbfbe0f7466f94f0" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-14605.ic27" merge="mpr-14605.ic27" size="2097152" crc="aaf52697" sha1="b502a37ae68fc08b60cdf0e2b744898b3474d3b9" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-14607.ic25" merge="mpr-14607.ic25" size="2097152" crc="b70b0735" sha1="9ef2da6f710bc5c2c7ee30dc144409a61dbe6646" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_v25" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <device_ref name="mb8421" />
    <device_ref name="v25" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="mainpcb:mcu" name="NEC V25" clock="10000000" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="2" service="yes">
      <control type="joy" player="1" buttons="2" ways="8" />
      <control type="joy" player="2" buttons="2" ways="8" />
      <control type="joy" player="3" buttons="2" ways="8" />
      <control type="joy" player="4" buttons="2" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="arabfgtu" sourcefile="segas32.cpp" cloneof="arabfgt" romof="arabfgt">
    <description>Arabian Fight (US)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14608.ic8" size="131072" crc="cd5efba9" sha1="a7daf8e95d31359753c984c447e93d40f43a179d" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14592.ic18" merge="epr-14592.ic18" size="262144" crc="f7dff316" sha1="338690a1404dde6e7e66067f23605a247c7d0f5b" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14591.ic9" merge="epr-14591.ic9" size="262144" crc="bbd940fb" sha1="99c17aba890935eaf7ea468492da03103288eb1b" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14596.ic36" merge="epr-14596.ic36" size="131072" crc="bd01faec" sha1="c909dcb8ef2672c4b0060d911d295e445ca311eb" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14595f.ic35" merge="mpr-14595f.ic35" size="1048576" crc="5173d1af" sha1="dccda644488d0c561c8ff7fa9619bd9504d8d9c6" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14594f.ic34" merge="mpr-14594f.ic34" size="1048576" crc="01777645" sha1="7bcbe7687bd80b94bd3b2b3099cdd036bf7e0cd3" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14593f.ic24" merge="mpr-14593f.ic24" size="1048576" crc="aa037047" sha1="5cb1cfb235bbbf875d2b07ac4a9130ba13d47e57" region="mainpcb:soundcpu" offset="300000" />
    <rom name="epr-14468-01.u3" merge="epr-14468-01.u3" size="65536" crc="c3c591e4" sha1="53e48066e85b61d0c456618d14334a509b354cb3" region="mainpcb:mcu" offset="0" />
    <rom name="mpr-14599f.ic14" merge="mpr-14599f.ic14" size="2097152" crc="94f1cf10" sha1="34ec86487bcb6726c025149c319f00a854eb7a1d" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14598f.ic5" merge="mpr-14598f.ic5" size="2097152" crc="010656f3" sha1="31619c022cba4f250ce174f186d3e34444f60faf" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14600f.ic32" merge="mpr-14600f.ic32" size="2097152" crc="e860988a" sha1="328581877c0890519c854f75f0976b0e9c4560f8" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14602.ic30" merge="mpr-14602.ic30" size="2097152" crc="64524e4d" sha1="86246185ab5ab638a73991c9e3aeb07c6d51be4f" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14604.ic28" merge="mpr-14604.ic28" size="2097152" crc="5f8d5167" sha1="1b08495e5a4cc2530c2895e47abd0e0b75496c68" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14606.ic26" merge="mpr-14606.ic26" size="2097152" crc="7047f437" sha1="e806a1cd73c96b33e8edc64e41d99bf7798103e0" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14601f.ic31" merge="mpr-14601f.ic31" size="2097152" crc="a2f3bb32" sha1="1a60975dead5faf08ad4e9a96a00f98664d5e5ec" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-14603.ic29" merge="mpr-14603.ic29" size="2097152" crc="f6ce494b" sha1="b3117e34913e855c035ebe37fbfbe0f7466f94f0" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-14605.ic27" merge="mpr-14605.ic27" size="2097152" crc="aaf52697" sha1="b502a37ae68fc08b60cdf0e2b744898b3474d3b9" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-14607.ic25" merge="mpr-14607.ic25" size="2097152" crc="b70b0735" sha1="9ef2da6f710bc5c2c7ee30dc144409a61dbe6646" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_v25" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <device_ref name="mb8421" />
    <device_ref name="v25" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="mainpcb:mcu" name="NEC V25" clock="10000000" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="4" service="yes">
      <control type="joy" player="1" buttons="2" ways="8" />
      <control type="joy" player="2" buttons="2" ways="8" />
      <control type="joy" player="3" buttons="2" ways="8" />
      <control type="joy" player="4" buttons="2" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="arescue" sourcefile="segas32.cpp">
    <description>Air Rescue (World)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14542.ic13" size="131072" crc="6d39fc18" sha1="7fbddfb2605a020331e1e81a7bc4466196df17bd" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14541.ic6" size="131072" crc="5c3f2ec5" sha1="d11a24d12917e4c5ac9010ca6db0f1ac9d44475a" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-14509.ic14" size="524288" crc="daa5a356" sha1="ca87242c59de5ab5f9406635bee758a855fe20bc" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14508.ic7" size="524288" crc="6702c14d" sha1="dc9324f16a3e3238f5ccdade9451d6823a50b563" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14513.ic35" size="262144" crc="f9a884cd" sha1="73010fff5e0257355e08e78838c74af86ed364ce" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14512.ic31" size="524288" crc="9da48051" sha1="2d41148d089a75362ed0fde577eca919213ac666" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14511.ic26" size="524288" crc="074c53cc" sha1="9c89843bbe8058123c25b7f8f86de754ddbca2bb" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14510.ic22" size="524288" crc="5ea6d52d" sha1="d424082468940bb91ab424ac7812839792ed4e88" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14496.ic25" size="524288" crc="737da16c" sha1="52247d9bc2924e90d040bef484a541b1f4a9026f" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-14497.ic29" size="524288" crc="ebd7ed17" sha1="2307dc28501965432d2ff55a21698efdce014401" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14498.ic34" size="524288" crc="d4a764bd" sha1="8434a9225ed1e01e8b1cfe169268e42cd3ce6ee3" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-14499.ic38" size="524288" crc="fadc4b2b" sha1="01c02a4dfad1ab19bac8b81b61d37fdc035bc5c5" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14500.ic24" size="1048576" crc="0a064e9b" sha1="264761f4aacaeeac9426528caf180404cd7f6e18" region="mainpcb:sprites" offset="7" />
    <rom name="mpr-14501.ic28" size="1048576" crc="4662bb41" sha1="80774e680468e9ba9c5dd5eeaa4791fa3b3722fd" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14502.ic33" size="1048576" crc="988555a9" sha1="355e44319fd51358329cc7cd226e4c4725e045cb" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-14503.ic37" size="1048576" crc="90556aca" sha1="24df62af55048db66d50c7034c5460330d231bf5" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14504.ic23" size="1048576" crc="46dd038d" sha1="9530a52e2e7388437c20ebcb19bf84c8b3b5086b" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-14505.ic27" size="1048576" crc="be142c1f" sha1="224631e00c2458c39c6a2ef7978c2b1131fb4da2" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14506.ic32" size="1048576" crc="5dd8fb6b" sha1="7d21cacb2c9dba5db2547b6d8e89397e0424ee8e" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-14507.ic36" size="1048576" crc="db3f59ec" sha1="96dcb3827354773fc2911c62260a27e90dcbe96a" region="mainpcb:sprites" offset="0" />
    <rom name="d7725.01" size="10240" crc="a7ec5644" sha1="e9b05c70b639ee289e557dfd9a6c724b36338e2b" region="mainpcb:dsp" offset="0" />
    <rom name="epr-14542.ic13" size="131072" crc="6d39fc18" sha1="7fbddfb2605a020331e1e81a7bc4466196df17bd" region="slavepcb:maincpu" offset="0" />
    <rom name="epr-14541.ic6" size="131072" crc="5c3f2ec5" sha1="d11a24d12917e4c5ac9010ca6db0f1ac9d44475a" region="slavepcb:maincpu" offset="80000" />
    <rom name="epr-14509.ic14" size="524288" crc="daa5a356" sha1="ca87242c59de5ab5f9406635bee758a855fe20bc" region="slavepcb:maincpu" offset="100000" />
    <rom name="epr-14508.ic7" size="524288" crc="6702c14d" sha1="dc9324f16a3e3238f5ccdade9451d6823a50b563" region="slavepcb:maincpu" offset="100001" />
    <rom name="epr-14513.ic35" size="262144" crc="f9a884cd" sha1="73010fff5e0257355e08e78838c74af86ed364ce" region="slavepcb:soundcpu" offset="0" />
    <rom name="mpr-14512.ic31" size="524288" crc="9da48051" sha1="2d41148d089a75362ed0fde577eca919213ac666" region="slavepcb:soundcpu" offset="100000" />
    <rom name="mpr-14511.ic26" size="524288" crc="074c53cc" sha1="9c89843bbe8058123c25b7f8f86de754ddbca2bb" region="slavepcb:soundcpu" offset="200000" />
    <rom name="mpr-14510.ic22" size="524288" crc="5ea6d52d" sha1="d424082468940bb91ab424ac7812839792ed4e88" region="slavepcb:soundcpu" offset="300000" />
    <rom name="mpr-14496.ic25" size="524288" crc="737da16c" sha1="52247d9bc2924e90d040bef484a541b1f4a9026f" region="slavepcb:gfx1" offset="3" />
    <rom name="mpr-14497.ic29" size="524288" crc="ebd7ed17" sha1="2307dc28501965432d2ff55a21698efdce014401" region="slavepcb:gfx1" offset="1" />
    <rom name="mpr-14498.ic34" size="524288" crc="d4a764bd" sha1="8434a9225ed1e01e8b1cfe169268e42cd3ce6ee3" region="slavepcb:gfx1" offset="2" />
    <rom name="mpr-14499.ic38" size="524288" crc="fadc4b2b" sha1="01c02a4dfad1ab19bac8b81b61d37fdc035bc5c5" region="slavepcb:gfx1" offset="0" />
    <rom name="mpr-14500.ic24" size="1048576" crc="0a064e9b" sha1="264761f4aacaeeac9426528caf180404cd7f6e18" region="slavepcb:sprites" offset="7" />
    <rom name="mpr-14501.ic28" size="1048576" crc="4662bb41" sha1="80774e680468e9ba9c5dd5eeaa4791fa3b3722fd" region="slavepcb:sprites" offset="6" />
    <rom name="mpr-14502.ic33" size="1048576" crc="988555a9" sha1="355e44319fd51358329cc7cd226e4c4725e045cb" region="slavepcb:sprites" offset="5" />
    <rom name="mpr-14503.ic37" size="1048576" crc="90556aca" sha1="24df62af55048db66d50c7034c5460330d231bf5" region="slavepcb:sprites" offset="4" />
    <rom name="mpr-14504.ic23" size="1048576" crc="46dd038d" sha1="9530a52e2e7388437c20ebcb19bf84c8b3b5086b" region="slavepcb:sprites" offset="3" />
    <rom name="mpr-14505.ic27" size="1048576" crc="be142c1f" sha1="224631e00c2458c39c6a2ef7978c2b1131fb4da2" region="slavepcb:sprites" offset="2" />
    <rom name="mpr-14506.ic32" size="1048576" crc="5dd8fb6b" sha1="7d21cacb2c9dba5db2547b6d8e89397e0424ee8e" region="slavepcb:sprites" offset="1" />
    <rom name="mpr-14507.ic36" size="1048576" crc="db3f59ec" sha1="96dcb3827354773fc2911c62260a27e90dcbe96a" region="slavepcb:sprites" offset="0" />
    <device_ref name="segas32_pcb_upd7725" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <device_ref name="upd7725" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="mainpcb:dsp" name="NEC uPD7725" clock="8000000" />
    <chip type="cpu" tag="slavepcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="slavepcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <chip type="audio" tag="slavepcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="slavepcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="4" />
    <input players="2" coins="4" service="yes">
      <control type="stick" player="1" buttons="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
      <control type="stick" player="2" buttons="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="1">
      <diplocation name="slavepcb_SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="2">
      <diplocation name="slavepcb_SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="4">
      <diplocation name="slavepcb_SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="8">
      <diplocation name="slavepcb_SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":slavepcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:P1_A" />
    <port tag=":slavepcb:P2_A" />
    <port tag=":slavepcb:PORTC_A" />
    <port tag=":slavepcb:SERVICE12_A" />
    <port tag=":slavepcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="arescuej" sourcefile="segas32.cpp" cloneof="arescue" romof="arescue">
    <description>Air Rescue (Japan)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14515.ic13" size="131072" crc="fb5eefbd" sha1="f2739ad2e168843fe992d7fb546ffd859fa6c17a" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14514.ic6" size="131072" crc="ebf6dfc5" sha1="2146dc23f1268124b6ad3cd00416a71fc56130bf" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-14509.ic14" merge="epr-14509.ic14" size="524288" crc="daa5a356" sha1="ca87242c59de5ab5f9406635bee758a855fe20bc" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14508.ic7" merge="epr-14508.ic7" size="524288" crc="6702c14d" sha1="dc9324f16a3e3238f5ccdade9451d6823a50b563" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14513.ic35" merge="epr-14513.ic35" size="262144" crc="f9a884cd" sha1="73010fff5e0257355e08e78838c74af86ed364ce" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14512.ic31" merge="mpr-14512.ic31" size="524288" crc="9da48051" sha1="2d41148d089a75362ed0fde577eca919213ac666" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14511.ic26" merge="mpr-14511.ic26" size="524288" crc="074c53cc" sha1="9c89843bbe8058123c25b7f8f86de754ddbca2bb" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14510.ic22" merge="mpr-14510.ic22" size="524288" crc="5ea6d52d" sha1="d424082468940bb91ab424ac7812839792ed4e88" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14496.ic25" merge="mpr-14496.ic25" size="524288" crc="737da16c" sha1="52247d9bc2924e90d040bef484a541b1f4a9026f" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-14497.ic29" merge="mpr-14497.ic29" size="524288" crc="ebd7ed17" sha1="2307dc28501965432d2ff55a21698efdce014401" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14498.ic34" merge="mpr-14498.ic34" size="524288" crc="d4a764bd" sha1="8434a9225ed1e01e8b1cfe169268e42cd3ce6ee3" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-14499.ic38" merge="mpr-14499.ic38" size="524288" crc="fadc4b2b" sha1="01c02a4dfad1ab19bac8b81b61d37fdc035bc5c5" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14500.ic24" merge="mpr-14500.ic24" size="1048576" crc="0a064e9b" sha1="264761f4aacaeeac9426528caf180404cd7f6e18" region="mainpcb:sprites" offset="7" />
    <rom name="mpr-14501.ic28" merge="mpr-14501.ic28" size="1048576" crc="4662bb41" sha1="80774e680468e9ba9c5dd5eeaa4791fa3b3722fd" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14502.ic33" merge="mpr-14502.ic33" size="1048576" crc="988555a9" sha1="355e44319fd51358329cc7cd226e4c4725e045cb" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-14503.ic37" merge="mpr-14503.ic37" size="1048576" crc="90556aca" sha1="24df62af55048db66d50c7034c5460330d231bf5" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14504.ic23" merge="mpr-14504.ic23" size="1048576" crc="46dd038d" sha1="9530a52e2e7388437c20ebcb19bf84c8b3b5086b" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-14505.ic27" merge="mpr-14505.ic27" size="1048576" crc="be142c1f" sha1="224631e00c2458c39c6a2ef7978c2b1131fb4da2" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14506.ic32" merge="mpr-14506.ic32" size="1048576" crc="5dd8fb6b" sha1="7d21cacb2c9dba5db2547b6d8e89397e0424ee8e" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-14507.ic36" merge="mpr-14507.ic36" size="1048576" crc="db3f59ec" sha1="96dcb3827354773fc2911c62260a27e90dcbe96a" region="mainpcb:sprites" offset="0" />
    <rom name="d7725.01" merge="d7725.01" size="10240" crc="a7ec5644" sha1="e9b05c70b639ee289e557dfd9a6c724b36338e2b" region="mainpcb:dsp" offset="0" />
    <rom name="epr-14515.ic13" size="131072" crc="fb5eefbd" sha1="f2739ad2e168843fe992d7fb546ffd859fa6c17a" region="slavepcb:maincpu" offset="0" />
    <rom name="epr-14514.ic6" size="131072" crc="ebf6dfc5" sha1="2146dc23f1268124b6ad3cd00416a71fc56130bf" region="slavepcb:maincpu" offset="80000" />
    <rom name="epr-14509.ic14" merge="epr-14509.ic14" size="524288" crc="daa5a356" sha1="ca87242c59de5ab5f9406635bee758a855fe20bc" region="slavepcb:maincpu" offset="100000" />
    <rom name="epr-14508.ic7" merge="epr-14508.ic7" size="524288" crc="6702c14d" sha1="dc9324f16a3e3238f5ccdade9451d6823a50b563" region="slavepcb:maincpu" offset="100001" />
    <rom name="epr-14513.ic35" merge="epr-14513.ic35" size="262144" crc="f9a884cd" sha1="73010fff5e0257355e08e78838c74af86ed364ce" region="slavepcb:soundcpu" offset="0" />
    <rom name="mpr-14512.ic31" merge="mpr-14512.ic31" size="524288" crc="9da48051" sha1="2d41148d089a75362ed0fde577eca919213ac666" region="slavepcb:soundcpu" offset="100000" />
    <rom name="mpr-14511.ic26" merge="mpr-14511.ic26" size="524288" crc="074c53cc" sha1="9c89843bbe8058123c25b7f8f86de754ddbca2bb" region="slavepcb:soundcpu" offset="200000" />
    <rom name="mpr-14510.ic22" merge="mpr-14510.ic22" size="524288" crc="5ea6d52d" sha1="d424082468940bb91ab424ac7812839792ed4e88" region="slavepcb:soundcpu" offset="300000" />
    <rom name="mpr-14496.ic25" merge="mpr-14496.ic25" size="524288" crc="737da16c" sha1="52247d9bc2924e90d040bef484a541b1f4a9026f" region="slavepcb:gfx1" offset="3" />
    <rom name="mpr-14497.ic29" merge="mpr-14497.ic29" size="524288" crc="ebd7ed17" sha1="2307dc28501965432d2ff55a21698efdce014401" region="slavepcb:gfx1" offset="1" />
    <rom name="mpr-14498.ic34" merge="mpr-14498.ic34" size="524288" crc="d4a764bd" sha1="8434a9225ed1e01e8b1cfe169268e42cd3ce6ee3" region="slavepcb:gfx1" offset="2" />
    <rom name="mpr-14499.ic38" merge="mpr-14499.ic38" size="524288" crc="fadc4b2b" sha1="01c02a4dfad1ab19bac8b81b61d37fdc035bc5c5" region="slavepcb:gfx1" offset="0" />
    <rom name="mpr-14500.ic24" merge="mpr-14500.ic24" size="1048576" crc="0a064e9b" sha1="264761f4aacaeeac9426528caf180404cd7f6e18" region="slavepcb:sprites" offset="7" />
    <rom name="mpr-14501.ic28" merge="mpr-14501.ic28" size="1048576" crc="4662bb41" sha1="80774e680468e9ba9c5dd5eeaa4791fa3b3722fd" region="slavepcb:sprites" offset="6" />
    <rom name="mpr-14502.ic33" merge="mpr-14502.ic33" size="1048576" crc="988555a9" sha1="355e44319fd51358329cc7cd226e4c4725e045cb" region="slavepcb:sprites" offset="5" />
    <rom name="mpr-14503.ic37" merge="mpr-14503.ic37" size="1048576" crc="90556aca" sha1="24df62af55048db66d50c7034c5460330d231bf5" region="slavepcb:sprites" offset="4" />
    <rom name="mpr-14504.ic23" merge="mpr-14504.ic23" size="1048576" crc="46dd038d" sha1="9530a52e2e7388437c20ebcb19bf84c8b3b5086b" region="slavepcb:sprites" offset="3" />
    <rom name="mpr-14505.ic27" merge="mpr-14505.ic27" size="1048576" crc="be142c1f" sha1="224631e00c2458c39c6a2ef7978c2b1131fb4da2" region="slavepcb:sprites" offset="2" />
    <rom name="mpr-14506.ic32" merge="mpr-14506.ic32" size="1048576" crc="5dd8fb6b" sha1="7d21cacb2c9dba5db2547b6d8e89397e0424ee8e" region="slavepcb:sprites" offset="1" />
    <rom name="mpr-14507.ic36" merge="mpr-14507.ic36" size="1048576" crc="db3f59ec" sha1="96dcb3827354773fc2911c62260a27e90dcbe96a" region="slavepcb:sprites" offset="0" />
    <device_ref name="segas32_pcb_upd7725" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <device_ref name="upd7725" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="mainpcb:dsp" name="NEC uPD7725" clock="8000000" />
    <chip type="cpu" tag="slavepcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="slavepcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <chip type="audio" tag="slavepcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="slavepcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="4" />
    <input players="2" coins="4" service="yes">
      <control type="stick" player="1" buttons="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
      <control type="stick" player="2" buttons="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="1">
      <diplocation name="slavepcb_SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="2">
      <diplocation name="slavepcb_SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="4">
      <diplocation name="slavepcb_SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="8">
      <diplocation name="slavepcb_SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":slavepcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:P1_A" />
    <port tag=":slavepcb:P2_A" />
    <port tag=":slavepcb:PORTC_A" />
    <port tag=":slavepcb:SERVICE12_A" />
    <port tag=":slavepcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="arescueu" sourcefile="segas32.cpp" cloneof="arescue" romof="arescue">
    <description>Air Rescue (US)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14540.ic13" size="131072" crc="c2b4e5d0" sha1="69f8ddded5095df9012663d0ded61b78f1692a8d" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14539.ic6" size="131072" crc="1a1b5532" sha1="f3651470222036703b7ecedb6e91e4cdb3d20df7" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-14509.ic14" merge="epr-14509.ic14" size="524288" crc="daa5a356" sha1="ca87242c59de5ab5f9406635bee758a855fe20bc" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14508.ic7" merge="epr-14508.ic7" size="524288" crc="6702c14d" sha1="dc9324f16a3e3238f5ccdade9451d6823a50b563" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14513.ic35" merge="epr-14513.ic35" size="262144" crc="f9a884cd" sha1="73010fff5e0257355e08e78838c74af86ed364ce" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14512.ic31" merge="mpr-14512.ic31" size="524288" crc="9da48051" sha1="2d41148d089a75362ed0fde577eca919213ac666" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14511.ic26" merge="mpr-14511.ic26" size="524288" crc="074c53cc" sha1="9c89843bbe8058123c25b7f8f86de754ddbca2bb" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14510.ic22" merge="mpr-14510.ic22" size="524288" crc="5ea6d52d" sha1="d424082468940bb91ab424ac7812839792ed4e88" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14496.ic25" merge="mpr-14496.ic25" size="524288" crc="737da16c" sha1="52247d9bc2924e90d040bef484a541b1f4a9026f" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-14497.ic29" merge="mpr-14497.ic29" size="524288" crc="ebd7ed17" sha1="2307dc28501965432d2ff55a21698efdce014401" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14498.ic34" merge="mpr-14498.ic34" size="524288" crc="d4a764bd" sha1="8434a9225ed1e01e8b1cfe169268e42cd3ce6ee3" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-14499.ic38" merge="mpr-14499.ic38" size="524288" crc="fadc4b2b" sha1="01c02a4dfad1ab19bac8b81b61d37fdc035bc5c5" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14500.ic24" merge="mpr-14500.ic24" size="1048576" crc="0a064e9b" sha1="264761f4aacaeeac9426528caf180404cd7f6e18" region="mainpcb:sprites" offset="7" />
    <rom name="mpr-14501.ic28" merge="mpr-14501.ic28" size="1048576" crc="4662bb41" sha1="80774e680468e9ba9c5dd5eeaa4791fa3b3722fd" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14502.ic33" merge="mpr-14502.ic33" size="1048576" crc="988555a9" sha1="355e44319fd51358329cc7cd226e4c4725e045cb" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-14503.ic37" merge="mpr-14503.ic37" size="1048576" crc="90556aca" sha1="24df62af55048db66d50c7034c5460330d231bf5" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14504.ic23" merge="mpr-14504.ic23" size="1048576" crc="46dd038d" sha1="9530a52e2e7388437c20ebcb19bf84c8b3b5086b" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-14505.ic27" merge="mpr-14505.ic27" size="1048576" crc="be142c1f" sha1="224631e00c2458c39c6a2ef7978c2b1131fb4da2" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14506.ic32" merge="mpr-14506.ic32" size="1048576" crc="5dd8fb6b" sha1="7d21cacb2c9dba5db2547b6d8e89397e0424ee8e" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-14507.ic36" merge="mpr-14507.ic36" size="1048576" crc="db3f59ec" sha1="96dcb3827354773fc2911c62260a27e90dcbe96a" region="mainpcb:sprites" offset="0" />
    <rom name="d7725.01" merge="d7725.01" size="10240" crc="a7ec5644" sha1="e9b05c70b639ee289e557dfd9a6c724b36338e2b" region="mainpcb:dsp" offset="0" />
    <rom name="epr-14540.ic13" size="131072" crc="c2b4e5d0" sha1="69f8ddded5095df9012663d0ded61b78f1692a8d" region="slavepcb:maincpu" offset="0" />
    <rom name="epr-14539.ic6" size="131072" crc="1a1b5532" sha1="f3651470222036703b7ecedb6e91e4cdb3d20df7" region="slavepcb:maincpu" offset="80000" />
    <rom name="epr-14509.ic14" merge="epr-14509.ic14" size="524288" crc="daa5a356" sha1="ca87242c59de5ab5f9406635bee758a855fe20bc" region="slavepcb:maincpu" offset="100000" />
    <rom name="epr-14508.ic7" merge="epr-14508.ic7" size="524288" crc="6702c14d" sha1="dc9324f16a3e3238f5ccdade9451d6823a50b563" region="slavepcb:maincpu" offset="100001" />
    <rom name="epr-14513.ic35" merge="epr-14513.ic35" size="262144" crc="f9a884cd" sha1="73010fff5e0257355e08e78838c74af86ed364ce" region="slavepcb:soundcpu" offset="0" />
    <rom name="mpr-14512.ic31" merge="mpr-14512.ic31" size="524288" crc="9da48051" sha1="2d41148d089a75362ed0fde577eca919213ac666" region="slavepcb:soundcpu" offset="100000" />
    <rom name="mpr-14511.ic26" merge="mpr-14511.ic26" size="524288" crc="074c53cc" sha1="9c89843bbe8058123c25b7f8f86de754ddbca2bb" region="slavepcb:soundcpu" offset="200000" />
    <rom name="mpr-14510.ic22" merge="mpr-14510.ic22" size="524288" crc="5ea6d52d" sha1="d424082468940bb91ab424ac7812839792ed4e88" region="slavepcb:soundcpu" offset="300000" />
    <rom name="mpr-14496.ic25" merge="mpr-14496.ic25" size="524288" crc="737da16c" sha1="52247d9bc2924e90d040bef484a541b1f4a9026f" region="slavepcb:gfx1" offset="3" />
    <rom name="mpr-14497.ic29" merge="mpr-14497.ic29" size="524288" crc="ebd7ed17" sha1="2307dc28501965432d2ff55a21698efdce014401" region="slavepcb:gfx1" offset="1" />
    <rom name="mpr-14498.ic34" merge="mpr-14498.ic34" size="524288" crc="d4a764bd" sha1="8434a9225ed1e01e8b1cfe169268e42cd3ce6ee3" region="slavepcb:gfx1" offset="2" />
    <rom name="mpr-14499.ic38" merge="mpr-14499.ic38" size="524288" crc="fadc4b2b" sha1="01c02a4dfad1ab19bac8b81b61d37fdc035bc5c5" region="slavepcb:gfx1" offset="0" />
    <rom name="mpr-14500.ic24" merge="mpr-14500.ic24" size="1048576" crc="0a064e9b" sha1="264761f4aacaeeac9426528caf180404cd7f6e18" region="slavepcb:sprites" offset="7" />
    <rom name="mpr-14501.ic28" merge="mpr-14501.ic28" size="1048576" crc="4662bb41" sha1="80774e680468e9ba9c5dd5eeaa4791fa3b3722fd" region="slavepcb:sprites" offset="6" />
    <rom name="mpr-14502.ic33" merge="mpr-14502.ic33" size="1048576" crc="988555a9" sha1="355e44319fd51358329cc7cd226e4c4725e045cb" region="slavepcb:sprites" offset="5" />
    <rom name="mpr-14503.ic37" merge="mpr-14503.ic37" size="1048576" crc="90556aca" sha1="24df62af55048db66d50c7034c5460330d231bf5" region="slavepcb:sprites" offset="4" />
    <rom name="mpr-14504.ic23" merge="mpr-14504.ic23" size="1048576" crc="46dd038d" sha1="9530a52e2e7388437c20ebcb19bf84c8b3b5086b" region="slavepcb:sprites" offset="3" />
    <rom name="mpr-14505.ic27" merge="mpr-14505.ic27" size="1048576" crc="be142c1f" sha1="224631e00c2458c39c6a2ef7978c2b1131fb4da2" region="slavepcb:sprites" offset="2" />
    <rom name="mpr-14506.ic32" merge="mpr-14506.ic32" size="1048576" crc="5dd8fb6b" sha1="7d21cacb2c9dba5db2547b6d8e89397e0424ee8e" region="slavepcb:sprites" offset="1" />
    <rom name="mpr-14507.ic36" merge="mpr-14507.ic36" size="1048576" crc="db3f59ec" sha1="96dcb3827354773fc2911c62260a27e90dcbe96a" region="slavepcb:sprites" offset="0" />
    <device_ref name="segas32_pcb_upd7725" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <device_ref name="upd7725" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="mainpcb:dsp" name="NEC uPD7725" clock="8000000" />
    <chip type="cpu" tag="slavepcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="slavepcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <chip type="audio" tag="slavepcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="slavepcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="4" />
    <input players="2" coins="4" service="yes">
      <control type="stick" player="1" buttons="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
      <control type="stick" player="2" buttons="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="1">
      <diplocation name="slavepcb_SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="2">
      <diplocation name="slavepcb_SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="4">
      <diplocation name="slavepcb_SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="8">
      <diplocation name="slavepcb_SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":slavepcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:P1_A" />
    <port tag=":slavepcb:P2_A" />
    <port tag=":slavepcb:PORTC_A" />
    <port tag=":slavepcb:SERVICE12_A" />
    <port tag=":slavepcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="as1" sourcefile="segas32.cpp">
    <description>AS-1 Controller</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr15420.ic37" size="131072" crc="1f9747b0" sha1="51d1fbccf6960967d4458ba26fad42ac51978c67" region="mainpcb:maincpu" offset="0" />
    <rom name="epr15421.ic40" size="131072" crc="aa96422a" sha1="21cf327d102f5c7c4a4e41d889d9b4d10c44de35" region="mainpcb:maincpu" offset="2" />
    <rom name="epr15367.ic31" size="131072" crc="0220f078" sha1="9fab79fc91764ecf678bfa4d38d1b4054e258b76" region="mainpcb:soundcpu" offset="0" />
    <rom name="epr15422.ic3" size="524288" crc="6c61ba6d" sha1="b41237ced4a2e8741ae0339c333bea4221903690" region="mainpcb:gfx1" offset="0" />
    <rom name="epr15423.ic11" size="524288" crc="5178912a" sha1="b637451c28877ddc93c9920bea356888b4c8eea3" region="mainpcb:gfx1" offset="1" />
    <device_ref name="segas32_pcb_multi" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="3" ways="8" />
      <control type="joy" player="2" buttons="3" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="preliminary" emulation="preliminary" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
    <feature type="sound" status="imperfect" />
  </machine>
  <machine name="brival" sourcefile="segas32.cpp">
    <description>Burning Rival (World)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15722.ic8" size="131072" crc="138141c0" sha1="aca2a46ee1008e91c65a09e79c76d5175e7df5e8" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15723.ic18" size="524288" crc="4ff40d39" sha1="b33a656f976ec7a1a2268e7b9a81d5b84f3d9ca3" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15724.ic9" size="524288" crc="3ff8a052" sha1="f484a8e15a022f9ff290e662ab27f96f9f0ad24e" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-15725.ic36" size="131072" crc="ea1407d7" sha1="68b571341f032278e87a38739ba8084b7a6062d3" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15627.ic35" size="1048576" crc="8a8388c5" sha1="7ee03feb975cc576a3d8651fd41976ca87d60894" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15626.ic34" size="1048576" crc="83306d1e" sha1="feb08902b51c0013d9417832cdf198e36cdfc28c" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15625.ic24" size="1048576" crc="3ce82932" sha1="f2107bc2591f46a51c9f0d706933b1ae69db91f9" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-15629.ic14" size="2097152" crc="2c8dd96d" sha1="4a42a30485c19eb4f4a9d518a3dff3ae11911d01" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15628.ic5" size="2097152" crc="58d4ca40" sha1="b1633acc803bba7e8283a9663b49abeda662a74d" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15637.ic32" size="2097152" crc="b6cf2f05" sha1="a308d40ce5165e03fccf7fcd615ee111f7840fdc" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15635.ic30" size="2097152" crc="70f2eb2b" sha1="9868c8b0dd8ce810a0e32f51e702eee7e1c9a967" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15633.ic28" size="2097152" crc="005dfed5" sha1="f555620d75d3886a890307be9df9c0879bcda695" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15631.ic26" size="2097152" crc="c35e2f21" sha1="37935aa2eaa1769e57fb58f47f9797ae153d7496" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15636.ic31" size="2097152" crc="d81ca97b" sha1="a8e64e6cbe822f18ce20f50c8ddb8f1d5ed8b783" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15634.ic29" size="2097152" crc="b0c6c52a" sha1="04dd7344ca82e38f9d796a764c9e5a631a89aaac" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15632.ic27" size="2097152" crc="8476e52b" sha1="e89748d34febcaf362580cdae30a5c570e56899a" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15630.ic25" size="2097152" crc="bf7dd2f6" sha1="ab3fbe9e2b9b57424fb2a147f32b0f573c0b11b8" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_4player" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="6" ways="8" />
      <control type="joy" player="2" buttons="6" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="brivalj" sourcefile="segas32.cpp" cloneof="brival" romof="brival">
    <description>Burning Rival (Japan)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15720.ic8" size="131072" crc="0d182d78" sha1="53e9e5898869ea4a354dc3e9a78d8b8e9a7274c9" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15723.ic18" merge="epr-15723.ic18" size="524288" crc="4ff40d39" sha1="b33a656f976ec7a1a2268e7b9a81d5b84f3d9ca3" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15724.ic9" merge="epr-15724.ic9" size="524288" crc="3ff8a052" sha1="f484a8e15a022f9ff290e662ab27f96f9f0ad24e" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-15725.ic36" merge="epr-15725.ic36" size="131072" crc="ea1407d7" sha1="68b571341f032278e87a38739ba8084b7a6062d3" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15627.ic35" merge="mpr-15627.ic35" size="1048576" crc="8a8388c5" sha1="7ee03feb975cc576a3d8651fd41976ca87d60894" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15626.ic34" merge="mpr-15626.ic34" size="1048576" crc="83306d1e" sha1="feb08902b51c0013d9417832cdf198e36cdfc28c" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15625.ic24" merge="mpr-15625.ic24" size="1048576" crc="3ce82932" sha1="f2107bc2591f46a51c9f0d706933b1ae69db91f9" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14599f.ic14" size="2097152" crc="1de17e83" sha1="04ee14b863f93b42a5bd1b6da71cff54ef11d4b7" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14598f.ic5" size="2097152" crc="cafb0de9" sha1="94c6bfc7a4081dee373e9466a7b6f80889696087" region="mainpcb:gfx1" offset="1" />
    <rom name="brivalj_mp15637.32" size="2097152" crc="f39844c0" sha1="c48dc8cccdd9d3756cf99a983c6a89ed43fcda22" region="mainpcb:sprites" offset="0" />
    <rom name="brivalj_mp15635.30" size="2097152" crc="263cf6d1" sha1="7accd214502fd050edc0901c9929d6069dae4d00" region="mainpcb:sprites" offset="2" />
    <rom name="brivalj_mp15633.28" size="2097152" crc="44e9a88b" sha1="57a930b9c3b83c889df54de60c90f847c2dcb614" region="mainpcb:sprites" offset="4" />
    <rom name="brivalj_mp15631.26" size="2097152" crc="e93cf9c9" sha1="17786cd3ccaef613216db724e923861841c52b45" region="mainpcb:sprites" offset="6" />
    <rom name="brivalj_mp15636.31" size="2097152" crc="079ff77f" sha1="bdd41acef58c39ba58cf85d307229622877dbdf9" region="mainpcb:sprites" offset="800000" />
    <rom name="brivalj_mp15634.29" size="2097152" crc="1edc14cd" sha1="80a281c904560b364fe9f2b8987b7a254220a29f" region="mainpcb:sprites" offset="800002" />
    <rom name="brivalj_mp15632.27" size="2097152" crc="796215f2" sha1="d7b393781dbba59c9b1cd600d27e6d91e36ea771" region="mainpcb:sprites" offset="800004" />
    <rom name="brivalj_mp15630.25" size="2097152" crc="8dabb501" sha1="c5af2187d00e0b9732a82441f9758b303fecbb2c" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_4player" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="6" ways="8" />
      <control type="joy" player="2" buttons="6" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="darkedge" sourcefile="segas32.cpp">
    <description>Dark Edge (World)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15246.ic8" size="524288" crc="c0bdceeb" sha1="9cf670cf9a8691f259c75c1d9c6cb14e8a70bb72" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15243.ic36" size="131072" crc="08ca5f11" sha1="c2c48d2f02770941a93794f82cb407d6264904d2" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15242.ic35" size="1048576" crc="ffb7d917" sha1="bfeae1a2bd7250edb695b7034f6b1f851f6fd48a" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15241.ic34" size="1048576" crc="8eccc4fe" sha1="119724b9b6d2b51ad4f065ebf74d200960090e68" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15240.ic24" size="1048576" crc="867d59e8" sha1="fb1c0d26dbb1bde9d8bc86419cd911b8e37bf923" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-15248.ic14" size="524288" crc="185b308b" sha1="a49c1b752b3c4355560e0cd712fb9a096140e37b" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15247.ic5" size="524288" crc="be21548c" sha1="2e315aadc2a0b781c3ee3fe71c75eb1f43514eff" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15249.ic32" size="2097152" crc="2b4371a8" sha1="47f448bfbc068f2d0cdedd81bcd280823d5758a3" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15251.ic30" size="2097152" crc="efe2d689" sha1="af22153ea3afdde3732f881087c642170f91d745" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15253.ic28" size="2097152" crc="8356ed01" sha1="a28747813807361c7d0c722a94e194caea8bfab6" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15255.ic26" size="2097152" crc="ff04a5b0" sha1="d4548f9da014ba5249c2f75d654a2a88c095aaf8" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15250.ic31" size="2097152" crc="c5cab71a" sha1="111c69c40a39c3fceef38f5876e1dcf7ac2fbee2" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15252.ic29" size="2097152" crc="f8885fea" sha1="ef944df5f6fd64813734056ad2a150f518c75459" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15254.ic27" size="2097152" crc="7765424b" sha1="7cd4c275f6333beeea62dd65a769e11650c68923" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15256.ic25" size="2097152" crc="44c36b62" sha1="4c7f2cc4347ef2126dcbf43e8dce8500e52b5f8e" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_4player" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="5" ways="8" />
      <control type="joy" player="2" buttons="5" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="darkedgej" sourcefile="segas32.cpp" cloneof="darkedge" romof="darkedge">
    <description>Dark Edge (Japan)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15244.ic8" size="524288" crc="0db138cb" sha1="79ccb754e0d816b395b536a6d9c5a6e93168a913" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15243.ic36" merge="epr-15243.ic36" size="131072" crc="08ca5f11" sha1="c2c48d2f02770941a93794f82cb407d6264904d2" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15242.ic35" merge="mpr-15242.ic35" size="1048576" crc="ffb7d917" sha1="bfeae1a2bd7250edb695b7034f6b1f851f6fd48a" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15241.ic34" merge="mpr-15241.ic34" size="1048576" crc="8eccc4fe" sha1="119724b9b6d2b51ad4f065ebf74d200960090e68" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15240.ic24" merge="mpr-15240.ic24" size="1048576" crc="867d59e8" sha1="fb1c0d26dbb1bde9d8bc86419cd911b8e37bf923" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-15248.ic14" merge="mpr-15248.ic14" size="524288" crc="185b308b" sha1="a49c1b752b3c4355560e0cd712fb9a096140e37b" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15247.ic5" merge="mpr-15247.ic5" size="524288" crc="be21548c" sha1="2e315aadc2a0b781c3ee3fe71c75eb1f43514eff" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15249.ic32" merge="mpr-15249.ic32" size="2097152" crc="2b4371a8" sha1="47f448bfbc068f2d0cdedd81bcd280823d5758a3" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15251.ic30" merge="mpr-15251.ic30" size="2097152" crc="efe2d689" sha1="af22153ea3afdde3732f881087c642170f91d745" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15253.ic28" merge="mpr-15253.ic28" size="2097152" crc="8356ed01" sha1="a28747813807361c7d0c722a94e194caea8bfab6" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15255.ic26" merge="mpr-15255.ic26" size="2097152" crc="ff04a5b0" sha1="d4548f9da014ba5249c2f75d654a2a88c095aaf8" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15250.ic31" merge="mpr-15250.ic31" size="2097152" crc="c5cab71a" sha1="111c69c40a39c3fceef38f5876e1dcf7ac2fbee2" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15252.ic29" merge="mpr-15252.ic29" size="2097152" crc="f8885fea" sha1="ef944df5f6fd64813734056ad2a150f518c75459" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15254.ic27" merge="mpr-15254.ic27" size="2097152" crc="7765424b" sha1="7cd4c275f6333beeea62dd65a769e11650c68923" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15256.ic25" merge="mpr-15256.ic25" size="2097152" crc="44c36b62" sha1="4c7f2cc4347ef2126dcbf43e8dce8500e52b5f8e" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_4player" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="5" ways="8" />
      <control type="joy" player="2" buttons="5" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="dbzvrvs" sourcefile="segas32.cpp">
    <description>Dragon Ball Z V.R.V.S. (Japan, Rev A)</description>
    <year>1994</year>
    <manufacturer>Sega / Banpresto</manufacturer>
    <rom name="epr-16543" size="524288" crc="7b9bc6f5" sha1="556fd8471bf471e41fc6a50471c2be1bd6b98697" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16542a" size="524288" crc="6449ab22" sha1="03e6cdacf77f2ff80dd6798094deac5486f2c840" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-16541" size="262144" crc="1d61d836" sha1="c6b1b54d41d2650abeaf69a31aa76c4462531880" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16540" size="1048576" crc="b6f9bb43" sha1="823f29a2fc4b9315e8c58616dbd095d45d366c8b" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16539" size="1048576" crc="38c26418" sha1="2442933e13c83209e904c1dec677aeda91b75290" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-16538" size="1048576" crc="4d402c31" sha1="2df160fd7e70f3d7b52fef2a2082e68966fd1535" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-16545" size="1048576" crc="51748bac" sha1="b1cae16b62a8d29117c0adb140eb09c1092f6c37" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16544" size="1048576" crc="f6c93dfc" sha1="a006cedb7d0151ccc8d22e6588b1c39e099da182" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16546" size="2097152" crc="96f4be31" sha1="ce3281630180d91de7850e9b1062382817fe0b1d" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16548" size="2097152" crc="00377f59" sha1="cf0f808d7730f334c5ac80d3171fa457be9ac88e" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16550" size="2097152" crc="168e8966" sha1="a18ec30f1358b09bcde6d8d2dbe0a82bea3bdae9" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16552" size="2097152" crc="a31dae31" sha1="2da2c391f29b5fdb87e3f95d9dabd50370fafa5a" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16547" size="2097152" crc="50d328ed" sha1="c4795299f5d7c9f3a847d684d8cde7012d4486f0" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16549" size="2097152" crc="a5802e9f" sha1="4cec3ed85a21aaf99b73013795721f212019e619" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16551" size="2097152" crc="dede05fc" sha1="51e092579e2b81fb68a9cc54165f80026fe71796" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16553" size="2097152" crc="c0a43009" sha1="e4f73768de512046b3e25c4238da811dcc2dde0b" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="3" ways="8" />
      <control type="joy" player="2" buttons="3" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1" />
    <port tag=":mainpcb:ANALOG2" />
    <port tag=":mainpcb:ANALOG3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="f1en" sourcefile="segas32.cpp">
    <description>F1 Exhaust Note (World, Rev A)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14452a.ic6" size="131072" crc="b5b4a9d9" sha1="6699c15dc1155c3cee33a06d320acbff0ab5ad11" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14445.ic14" size="262144" crc="d06261ab" sha1="6e1c4ce4e49a142fd5b1ecac98145960d7afd567" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14444.ic7" size="262144" crc="07724354" sha1="9d7f64a80553c4ae0e9cf716478fd5c4b8277470" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14449.ic35" size="131072" crc="2d29699c" sha1="cae02e5533a0edd3b3b4a54a1a43321285e06416" region="mainpcb:soundcpu" offset="0" />
    <rom name="epr-14448.ic31" size="524288" crc="87ca1e8d" sha1="739274171c13983a60d061176095645419dade49" region="mainpcb:soundcpu" offset="100000" />
    <rom name="epr-14447.ic26" size="524288" crc="db1cfcbd" sha1="c76eb2ced5571a548ad00709097dd272747127a2" region="mainpcb:soundcpu" offset="200000" />
    <rom name="epr-14446.ic22" size="524288" crc="646ec2cb" sha1="67e453f128ae227e22c68f55d0d3f5831fbeb2f9" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14362.ic38" size="262144" crc="fb1c4e79" sha1="38ee23763b9e5bb62bbc54cab95041415404f0c4" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14361.ic34" size="262144" crc="e3204bda" sha1="34157e80edd6d685bd5a5e23b1e0130a5f3d138a" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-14360.ic29" size="262144" crc="c5e8da79" sha1="662a6c146fe3d0b8763d845379c06d0ee6ced1ed" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14359.ic25" size="262144" crc="70305c68" sha1="7a6a1bf7381eba8cc1c3897497b32ca63316972a" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-14370.ic36" size="524288" crc="fda78289" sha1="3740affdcc738c50d07ff3e5b592bdf8a8b6be15" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14369.ic32" size="524288" crc="7765116d" sha1="9493148aa84adc90143cf638265d4c55bfb43990" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-14368.ic27" size="524288" crc="5744a30e" sha1="98544fb234a8e93716e951d5414a490845e213c5" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14367.ic23" size="524288" crc="77bb9003" sha1="6370fdeab4967976840d752577cd860b9ce8efca" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-14366.ic37" size="524288" crc="21078e83" sha1="f35f643c28aad3bf18cb9906b114c4f49b7b4cd1" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14365.ic33" size="524288" crc="36913790" sha1="4a447cffb44b023fe1441277db1e411d4cd119eb" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-14364.ic28" size="524288" crc="0fa12ecd" sha1="6a34c7718edffbeddded8786e11cac181b485ebd" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14363.ic24" size="524288" crc="f3427a56" sha1="6a99d7432dfff35470ddcca5cfde36689a77e706" region="mainpcb:sprites" offset="7" />
    <rom name="epr-14452a.ic6" size="131072" crc="b5b4a9d9" sha1="6699c15dc1155c3cee33a06d320acbff0ab5ad11" region="slavepcb:maincpu" offset="0" />
    <rom name="epr-14445.ic14" size="262144" crc="d06261ab" sha1="6e1c4ce4e49a142fd5b1ecac98145960d7afd567" region="slavepcb:maincpu" offset="100000" />
    <rom name="epr-14444.ic7" size="262144" crc="07724354" sha1="9d7f64a80553c4ae0e9cf716478fd5c4b8277470" region="slavepcb:maincpu" offset="100001" />
    <rom name="epr-14449.ic35" size="131072" crc="2d29699c" sha1="cae02e5533a0edd3b3b4a54a1a43321285e06416" region="slavepcb:soundcpu" offset="0" />
    <rom name="epr-14448.ic31" size="524288" crc="87ca1e8d" sha1="739274171c13983a60d061176095645419dade49" region="slavepcb:soundcpu" offset="100000" />
    <rom name="epr-14447.ic26" size="524288" crc="db1cfcbd" sha1="c76eb2ced5571a548ad00709097dd272747127a2" region="slavepcb:soundcpu" offset="200000" />
    <rom name="epr-14446.ic22" size="524288" crc="646ec2cb" sha1="67e453f128ae227e22c68f55d0d3f5831fbeb2f9" region="slavepcb:soundcpu" offset="300000" />
    <rom name="mpr-14362.ic38" size="262144" crc="fb1c4e79" sha1="38ee23763b9e5bb62bbc54cab95041415404f0c4" region="slavepcb:gfx1" offset="0" />
    <rom name="mpr-14361.ic34" size="262144" crc="e3204bda" sha1="34157e80edd6d685bd5a5e23b1e0130a5f3d138a" region="slavepcb:gfx1" offset="2" />
    <rom name="mpr-14360.ic29" size="262144" crc="c5e8da79" sha1="662a6c146fe3d0b8763d845379c06d0ee6ced1ed" region="slavepcb:gfx1" offset="1" />
    <rom name="mpr-14359.ic25" size="262144" crc="70305c68" sha1="7a6a1bf7381eba8cc1c3897497b32ca63316972a" region="slavepcb:gfx1" offset="3" />
    <rom name="mpr-14370.ic36" size="524288" crc="fda78289" sha1="3740affdcc738c50d07ff3e5b592bdf8a8b6be15" region="slavepcb:sprites" offset="0" />
    <rom name="mpr-14369.ic32" size="524288" crc="7765116d" sha1="9493148aa84adc90143cf638265d4c55bfb43990" region="slavepcb:sprites" offset="1" />
    <rom name="mpr-14368.ic27" size="524288" crc="5744a30e" sha1="98544fb234a8e93716e951d5414a490845e213c5" region="slavepcb:sprites" offset="2" />
    <rom name="mpr-14367.ic23" size="524288" crc="77bb9003" sha1="6370fdeab4967976840d752577cd860b9ce8efca" region="slavepcb:sprites" offset="3" />
    <rom name="mpr-14366.ic37" size="524288" crc="21078e83" sha1="f35f643c28aad3bf18cb9906b114c4f49b7b4cd1" region="slavepcb:sprites" offset="4" />
    <rom name="mpr-14365.ic33" size="524288" crc="36913790" sha1="4a447cffb44b023fe1441277db1e411d4cd119eb" region="slavepcb:sprites" offset="5" />
    <rom name="mpr-14364.ic28" size="524288" crc="0fa12ecd" sha1="6a34c7718edffbeddded8786e11cac181b485ebd" region="slavepcb:sprites" offset="6" />
    <rom name="mpr-14363.ic24" size="524288" crc="f3427a56" sha1="6a99d7432dfff35470ddcca5cfde36689a77e706" region="slavepcb:sprites" offset="7" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="slavepcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="slavepcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <chip type="audio" tag="slavepcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="slavepcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="4" />
    <input players="2" coins="3" service="yes">
      <control type="paddle" player="1" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
      <control type="pedal" player="1" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
      <control type="paddle" player="2" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
      <control type="pedal" player="2" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="1">
      <diplocation name="slavepcb_SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="2">
      <diplocation name="slavepcb_SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="4">
      <diplocation name="slavepcb_SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="8">
      <diplocation name="slavepcb_SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":slavepcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:P1_A" />
    <port tag=":slavepcb:P2_A" />
    <port tag=":slavepcb:PORTC_A" />
    <port tag=":slavepcb:SERVICE12_A" />
    <port tag=":slavepcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="f1enj" sourcefile="segas32.cpp" cloneof="f1en" romof="f1en">
    <description>F1 Exhaust Note (Japan, Rev A)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14450a.ic6" size="131072" crc="10f62723" sha1="68fcd6655798f348678e3cc8857c6d1cb46e0987" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14445.ic14" merge="epr-14445.ic14" size="262144" crc="d06261ab" sha1="6e1c4ce4e49a142fd5b1ecac98145960d7afd567" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14444.ic7" merge="epr-14444.ic7" size="262144" crc="07724354" sha1="9d7f64a80553c4ae0e9cf716478fd5c4b8277470" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14449.ic35" merge="epr-14449.ic35" size="131072" crc="2d29699c" sha1="cae02e5533a0edd3b3b4a54a1a43321285e06416" region="mainpcb:soundcpu" offset="0" />
    <rom name="epr-14448.ic31" merge="epr-14448.ic31" size="524288" crc="87ca1e8d" sha1="739274171c13983a60d061176095645419dade49" region="mainpcb:soundcpu" offset="100000" />
    <rom name="epr-14447.ic26" merge="epr-14447.ic26" size="524288" crc="db1cfcbd" sha1="c76eb2ced5571a548ad00709097dd272747127a2" region="mainpcb:soundcpu" offset="200000" />
    <rom name="epr-14446.ic22" merge="epr-14446.ic22" size="524288" crc="646ec2cb" sha1="67e453f128ae227e22c68f55d0d3f5831fbeb2f9" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14362.ic38" merge="mpr-14362.ic38" size="262144" crc="fb1c4e79" sha1="38ee23763b9e5bb62bbc54cab95041415404f0c4" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14361.ic34" merge="mpr-14361.ic34" size="262144" crc="e3204bda" sha1="34157e80edd6d685bd5a5e23b1e0130a5f3d138a" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-14360.ic29" merge="mpr-14360.ic29" size="262144" crc="c5e8da79" sha1="662a6c146fe3d0b8763d845379c06d0ee6ced1ed" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14359.ic25" merge="mpr-14359.ic25" size="262144" crc="70305c68" sha1="7a6a1bf7381eba8cc1c3897497b32ca63316972a" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-14370.ic36" merge="mpr-14370.ic36" size="524288" crc="fda78289" sha1="3740affdcc738c50d07ff3e5b592bdf8a8b6be15" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14369.ic32" merge="mpr-14369.ic32" size="524288" crc="7765116d" sha1="9493148aa84adc90143cf638265d4c55bfb43990" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-14368.ic27" merge="mpr-14368.ic27" size="524288" crc="5744a30e" sha1="98544fb234a8e93716e951d5414a490845e213c5" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14367.ic23" merge="mpr-14367.ic23" size="524288" crc="77bb9003" sha1="6370fdeab4967976840d752577cd860b9ce8efca" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-14366.ic37" merge="mpr-14366.ic37" size="524288" crc="21078e83" sha1="f35f643c28aad3bf18cb9906b114c4f49b7b4cd1" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14365.ic33" merge="mpr-14365.ic33" size="524288" crc="36913790" sha1="4a447cffb44b023fe1441277db1e411d4cd119eb" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-14364.ic28" merge="mpr-14364.ic28" size="524288" crc="0fa12ecd" sha1="6a34c7718edffbeddded8786e11cac181b485ebd" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14363.ic24" merge="mpr-14363.ic24" size="524288" crc="f3427a56" sha1="6a99d7432dfff35470ddcca5cfde36689a77e706" region="mainpcb:sprites" offset="7" />
    <rom name="epr-14450a.ic6" size="131072" crc="10f62723" sha1="68fcd6655798f348678e3cc8857c6d1cb46e0987" region="slavepcb:maincpu" offset="0" />
    <rom name="epr-14445.ic14" merge="epr-14445.ic14" size="262144" crc="d06261ab" sha1="6e1c4ce4e49a142fd5b1ecac98145960d7afd567" region="slavepcb:maincpu" offset="100000" />
    <rom name="epr-14444.ic7" merge="epr-14444.ic7" size="262144" crc="07724354" sha1="9d7f64a80553c4ae0e9cf716478fd5c4b8277470" region="slavepcb:maincpu" offset="100001" />
    <rom name="epr-14449.ic35" merge="epr-14449.ic35" size="131072" crc="2d29699c" sha1="cae02e5533a0edd3b3b4a54a1a43321285e06416" region="slavepcb:soundcpu" offset="0" />
    <rom name="epr-14448.ic31" merge="epr-14448.ic31" size="524288" crc="87ca1e8d" sha1="739274171c13983a60d061176095645419dade49" region="slavepcb:soundcpu" offset="100000" />
    <rom name="epr-14447.ic26" merge="epr-14447.ic26" size="524288" crc="db1cfcbd" sha1="c76eb2ced5571a548ad00709097dd272747127a2" region="slavepcb:soundcpu" offset="200000" />
    <rom name="epr-14446.ic22" merge="epr-14446.ic22" size="524288" crc="646ec2cb" sha1="67e453f128ae227e22c68f55d0d3f5831fbeb2f9" region="slavepcb:soundcpu" offset="300000" />
    <rom name="mpr-14362.ic38" merge="mpr-14362.ic38" size="262144" crc="fb1c4e79" sha1="38ee23763b9e5bb62bbc54cab95041415404f0c4" region="slavepcb:gfx1" offset="0" />
    <rom name="mpr-14361.ic34" merge="mpr-14361.ic34" size="262144" crc="e3204bda" sha1="34157e80edd6d685bd5a5e23b1e0130a5f3d138a" region="slavepcb:gfx1" offset="2" />
    <rom name="mpr-14360.ic29" merge="mpr-14360.ic29" size="262144" crc="c5e8da79" sha1="662a6c146fe3d0b8763d845379c06d0ee6ced1ed" region="slavepcb:gfx1" offset="1" />
    <rom name="mpr-14359.ic25" merge="mpr-14359.ic25" size="262144" crc="70305c68" sha1="7a6a1bf7381eba8cc1c3897497b32ca63316972a" region="slavepcb:gfx1" offset="3" />
    <rom name="mpr-14370.ic36" merge="mpr-14370.ic36" size="524288" crc="fda78289" sha1="3740affdcc738c50d07ff3e5b592bdf8a8b6be15" region="slavepcb:sprites" offset="0" />
    <rom name="mpr-14369.ic32" merge="mpr-14369.ic32" size="524288" crc="7765116d" sha1="9493148aa84adc90143cf638265d4c55bfb43990" region="slavepcb:sprites" offset="1" />
    <rom name="mpr-14368.ic27" merge="mpr-14368.ic27" size="524288" crc="5744a30e" sha1="98544fb234a8e93716e951d5414a490845e213c5" region="slavepcb:sprites" offset="2" />
    <rom name="mpr-14367.ic23" merge="mpr-14367.ic23" size="524288" crc="77bb9003" sha1="6370fdeab4967976840d752577cd860b9ce8efca" region="slavepcb:sprites" offset="3" />
    <rom name="mpr-14366.ic37" merge="mpr-14366.ic37" size="524288" crc="21078e83" sha1="f35f643c28aad3bf18cb9906b114c4f49b7b4cd1" region="slavepcb:sprites" offset="4" />
    <rom name="mpr-14365.ic33" merge="mpr-14365.ic33" size="524288" crc="36913790" sha1="4a447cffb44b023fe1441277db1e411d4cd119eb" region="slavepcb:sprites" offset="5" />
    <rom name="mpr-14364.ic28" merge="mpr-14364.ic28" size="524288" crc="0fa12ecd" sha1="6a34c7718edffbeddded8786e11cac181b485ebd" region="slavepcb:sprites" offset="6" />
    <rom name="mpr-14363.ic24" merge="mpr-14363.ic24" size="524288" crc="f3427a56" sha1="6a99d7432dfff35470ddcca5cfde36689a77e706" region="slavepcb:sprites" offset="7" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="slavepcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="slavepcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <chip type="audio" tag="slavepcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="slavepcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="4" />
    <input players="2" coins="3" service="yes">
      <control type="paddle" player="1" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
      <control type="pedal" player="1" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
      <control type="paddle" player="2" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
      <control type="pedal" player="2" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="1">
      <diplocation name="slavepcb_SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="2">
      <diplocation name="slavepcb_SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="4">
      <diplocation name="slavepcb_SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="8">
      <diplocation name="slavepcb_SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":slavepcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:P1_A" />
    <port tag=":slavepcb:P2_A" />
    <port tag=":slavepcb:PORTC_A" />
    <port tag=":slavepcb:SERVICE12_A" />
    <port tag=":slavepcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="f1enu" sourcefile="segas32.cpp" cloneof="f1en" romof="f1en">
    <description>F1 Exhaust Note (US, Rev A)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14451a.ic6" size="131072" crc="e17259c9" sha1="be789b7630b7265e19ea2c80f603caff9cec37f8" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14445.ic14" merge="epr-14445.ic14" size="262144" crc="d06261ab" sha1="6e1c4ce4e49a142fd5b1ecac98145960d7afd567" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14444.ic7" merge="epr-14444.ic7" size="262144" crc="07724354" sha1="9d7f64a80553c4ae0e9cf716478fd5c4b8277470" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14449.ic35" merge="epr-14449.ic35" size="131072" crc="2d29699c" sha1="cae02e5533a0edd3b3b4a54a1a43321285e06416" region="mainpcb:soundcpu" offset="0" />
    <rom name="epr-14448.ic31" merge="epr-14448.ic31" size="524288" crc="87ca1e8d" sha1="739274171c13983a60d061176095645419dade49" region="mainpcb:soundcpu" offset="100000" />
    <rom name="epr-14447.ic26" merge="epr-14447.ic26" size="524288" crc="db1cfcbd" sha1="c76eb2ced5571a548ad00709097dd272747127a2" region="mainpcb:soundcpu" offset="200000" />
    <rom name="epr-14446.ic22" merge="epr-14446.ic22" size="524288" crc="646ec2cb" sha1="67e453f128ae227e22c68f55d0d3f5831fbeb2f9" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14362.ic38" merge="mpr-14362.ic38" size="262144" crc="fb1c4e79" sha1="38ee23763b9e5bb62bbc54cab95041415404f0c4" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14361.ic34" merge="mpr-14361.ic34" size="262144" crc="e3204bda" sha1="34157e80edd6d685bd5a5e23b1e0130a5f3d138a" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-14360.ic29" merge="mpr-14360.ic29" size="262144" crc="c5e8da79" sha1="662a6c146fe3d0b8763d845379c06d0ee6ced1ed" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14359.ic25" merge="mpr-14359.ic25" size="262144" crc="70305c68" sha1="7a6a1bf7381eba8cc1c3897497b32ca63316972a" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-14370.ic36" merge="mpr-14370.ic36" size="524288" crc="fda78289" sha1="3740affdcc738c50d07ff3e5b592bdf8a8b6be15" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14369.ic32" merge="mpr-14369.ic32" size="524288" crc="7765116d" sha1="9493148aa84adc90143cf638265d4c55bfb43990" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-14368.ic27" merge="mpr-14368.ic27" size="524288" crc="5744a30e" sha1="98544fb234a8e93716e951d5414a490845e213c5" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14367.ic23" merge="mpr-14367.ic23" size="524288" crc="77bb9003" sha1="6370fdeab4967976840d752577cd860b9ce8efca" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-14366.ic37" merge="mpr-14366.ic37" size="524288" crc="21078e83" sha1="f35f643c28aad3bf18cb9906b114c4f49b7b4cd1" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14365.ic33" merge="mpr-14365.ic33" size="524288" crc="36913790" sha1="4a447cffb44b023fe1441277db1e411d4cd119eb" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-14364.ic28" merge="mpr-14364.ic28" size="524288" crc="0fa12ecd" sha1="6a34c7718edffbeddded8786e11cac181b485ebd" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14363.ic24" merge="mpr-14363.ic24" size="524288" crc="f3427a56" sha1="6a99d7432dfff35470ddcca5cfde36689a77e706" region="mainpcb:sprites" offset="7" />
    <rom name="epr-14451a.ic6" size="131072" crc="e17259c9" sha1="be789b7630b7265e19ea2c80f603caff9cec37f8" region="slavepcb:maincpu" offset="0" />
    <rom name="epr-14445.ic14" merge="epr-14445.ic14" size="262144" crc="d06261ab" sha1="6e1c4ce4e49a142fd5b1ecac98145960d7afd567" region="slavepcb:maincpu" offset="100000" />
    <rom name="epr-14444.ic7" merge="epr-14444.ic7" size="262144" crc="07724354" sha1="9d7f64a80553c4ae0e9cf716478fd5c4b8277470" region="slavepcb:maincpu" offset="100001" />
    <rom name="epr-14449.ic35" merge="epr-14449.ic35" size="131072" crc="2d29699c" sha1="cae02e5533a0edd3b3b4a54a1a43321285e06416" region="slavepcb:soundcpu" offset="0" />
    <rom name="epr-14448.ic31" merge="epr-14448.ic31" size="524288" crc="87ca1e8d" sha1="739274171c13983a60d061176095645419dade49" region="slavepcb:soundcpu" offset="100000" />
    <rom name="epr-14447.ic26" merge="epr-14447.ic26" size="524288" crc="db1cfcbd" sha1="c76eb2ced5571a548ad00709097dd272747127a2" region="slavepcb:soundcpu" offset="200000" />
    <rom name="epr-14446.ic22" merge="epr-14446.ic22" size="524288" crc="646ec2cb" sha1="67e453f128ae227e22c68f55d0d3f5831fbeb2f9" region="slavepcb:soundcpu" offset="300000" />
    <rom name="mpr-14362.ic38" merge="mpr-14362.ic38" size="262144" crc="fb1c4e79" sha1="38ee23763b9e5bb62bbc54cab95041415404f0c4" region="slavepcb:gfx1" offset="0" />
    <rom name="mpr-14361.ic34" merge="mpr-14361.ic34" size="262144" crc="e3204bda" sha1="34157e80edd6d685bd5a5e23b1e0130a5f3d138a" region="slavepcb:gfx1" offset="2" />
    <rom name="mpr-14360.ic29" merge="mpr-14360.ic29" size="262144" crc="c5e8da79" sha1="662a6c146fe3d0b8763d845379c06d0ee6ced1ed" region="slavepcb:gfx1" offset="1" />
    <rom name="mpr-14359.ic25" merge="mpr-14359.ic25" size="262144" crc="70305c68" sha1="7a6a1bf7381eba8cc1c3897497b32ca63316972a" region="slavepcb:gfx1" offset="3" />
    <rom name="mpr-14370.ic36" merge="mpr-14370.ic36" size="524288" crc="fda78289" sha1="3740affdcc738c50d07ff3e5b592bdf8a8b6be15" region="slavepcb:sprites" offset="0" />
    <rom name="mpr-14369.ic32" merge="mpr-14369.ic32" size="524288" crc="7765116d" sha1="9493148aa84adc90143cf638265d4c55bfb43990" region="slavepcb:sprites" offset="1" />
    <rom name="mpr-14368.ic27" merge="mpr-14368.ic27" size="524288" crc="5744a30e" sha1="98544fb234a8e93716e951d5414a490845e213c5" region="slavepcb:sprites" offset="2" />
    <rom name="mpr-14367.ic23" merge="mpr-14367.ic23" size="524288" crc="77bb9003" sha1="6370fdeab4967976840d752577cd860b9ce8efca" region="slavepcb:sprites" offset="3" />
    <rom name="mpr-14366.ic37" merge="mpr-14366.ic37" size="524288" crc="21078e83" sha1="f35f643c28aad3bf18cb9906b114c4f49b7b4cd1" region="slavepcb:sprites" offset="4" />
    <rom name="mpr-14365.ic33" merge="mpr-14365.ic33" size="524288" crc="36913790" sha1="4a447cffb44b023fe1441277db1e411d4cd119eb" region="slavepcb:sprites" offset="5" />
    <rom name="mpr-14364.ic28" merge="mpr-14364.ic28" size="524288" crc="0fa12ecd" sha1="6a34c7718edffbeddded8786e11cac181b485ebd" region="slavepcb:sprites" offset="6" />
    <rom name="mpr-14363.ic24" merge="mpr-14363.ic24" size="524288" crc="f3427a56" sha1="6a99d7432dfff35470ddcca5cfde36689a77e706" region="slavepcb:sprites" offset="7" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="slavepcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="slavepcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <chip type="audio" tag="slavepcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="slavepcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="slavepcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="slavepcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="4" />
    <input players="2" coins="3" service="yes">
      <control type="paddle" player="1" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
      <control type="pedal" player="1" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
      <control type="paddle" player="2" buttons="2" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
      <control type="pedal" player="2" minimum="0" maximum="255" sensitivity="50" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="1">
      <diplocation name="slavepcb_SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="2">
      <diplocation name="slavepcb_SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="4">
      <diplocation name="slavepcb_SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="slavepcb:SERVICE34_A" mask="8">
      <diplocation name="slavepcb_SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":slavepcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":slavepcb:P1_A" />
    <port tag=":slavepcb:P2_A" />
    <port tag=":slavepcb:PORTC_A" />
    <port tag=":slavepcb:SERVICE12_A" />
    <port tag=":slavepcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="f1lap" sourcefile="segas32.cpp">
    <description>F1 Super Lap (World)</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15598.ic17" size="131072" crc="9feab7cd" sha1="2a14c0df39e7bdae12a34679fabc6abb7618e27d" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15611.ic8" size="131072" crc="0d8c97c2" sha1="863c606c58faddc2bdaeb69f9079266155ff9a96" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-15596.ic18" size="262144" crc="20e92909" sha1="b974c79e11bfbd1cee61f9041cf79971fd96db3a" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15597.ic9" size="262144" crc="cd1ccddb" sha1="ff0371a8010141d1ab81b5eba555ae7c64e5da37" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-15592.ic36" size="131072" crc="7c055cc8" sha1="169beb83dfae86dd408aa92b3c214b8f607825fc" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15593.ic35" size="1048576" crc="e7300441" sha1="33c264f0e6326689ba75026932c0932868e83b25" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15594.ic34" size="1048576" crc="7f4ca3bb" sha1="dc53a1857d619e574acb4c0587a6ba844df2d283" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15595.ic24" size="1048576" crc="3fbdad9a" sha1="573ea2242f79c7d3b6bf0e6745f6b07a621834ac" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-15608.ic14" size="2097152" crc="64462c69" sha1="9501e83c52e3e16f73b94cef975b5a31b2ee5476" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15609.ic5" size="2097152" crc="d586e455" sha1="aea190d31c590216eb19766ba749b1e9b710bdce" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15600.ic32" size="2097152" crc="d2698d23" sha1="996fbcc1d0814e6f14fa7e4870ece077ecda54e6" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15602.ic30" size="2097152" crc="1674764d" sha1="bc39757a5d25df1a088f874ca2442854eb551e48" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15604.ic28" size="2097152" crc="1552bbb9" sha1="77edd3f9d8dec87fa0445d264309e6164eba9313" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15606.ic26" size="2097152" crc="2b4f5265" sha1="48b4ccdedb52fbf80661ff380e5a273201fc0a12" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15601.ic31" size="2097152" crc="31a8f40a" sha1="62798346750dea87e43c8a8b01c33bf886bb50f4" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15603.ic29" size="2097152" crc="3805ecbc" sha1="54d29250441160f282c70adfd515adb21d2cda33" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15605.ic27" size="2097152" crc="cbdbf35e" sha1="a1c0900ac3210e72f5848561a6c4a77c804782c6" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15607.ic25" size="2097152" crc="6c8817c9" sha1="f5d493ed4237caf5042e95373bf9abd1fd16f873" region="mainpcb:sprites" offset="800006" />
    <rom name="15612" size="131072" crc="9d204617" sha1="8db57121065f5d1ac52fcfb88459bdbdc30e645b" region="user2" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="1" coins="2" service="yes">
      <control type="paddle" buttons="3" minimum="0" maximum="255" sensitivity="50" keydelta="20" />
      <control type="pedal" minimum="0" maximum="255" sensitivity="50" keydelta="20" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="f1lapj" sourcefile="segas32.cpp" cloneof="f1lap" romof="f1lap">
    <description>F1 Super Lap (Japan)</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15598.ic17" merge="epr-15598.ic17" size="131072" crc="9feab7cd" sha1="2a14c0df39e7bdae12a34679fabc6abb7618e27d" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15599.ic8" size="131072" crc="5c5ac112" sha1="2c071946e33f0700a832c7aad36f639acd35f555" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-15596.ic18" merge="epr-15596.ic18" size="262144" crc="20e92909" sha1="b974c79e11bfbd1cee61f9041cf79971fd96db3a" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15597.ic9" merge="epr-15597.ic9" size="262144" crc="cd1ccddb" sha1="ff0371a8010141d1ab81b5eba555ae7c64e5da37" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-15592.ic36" merge="epr-15592.ic36" size="131072" crc="7c055cc8" sha1="169beb83dfae86dd408aa92b3c214b8f607825fc" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15593.ic35" merge="mpr-15593.ic35" size="1048576" crc="e7300441" sha1="33c264f0e6326689ba75026932c0932868e83b25" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15594.ic34" merge="mpr-15594.ic34" size="1048576" crc="7f4ca3bb" sha1="dc53a1857d619e574acb4c0587a6ba844df2d283" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15595.ic24" merge="mpr-15595.ic24" size="1048576" crc="3fbdad9a" sha1="573ea2242f79c7d3b6bf0e6745f6b07a621834ac" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-15608.ic14" merge="mpr-15608.ic14" size="2097152" crc="64462c69" sha1="9501e83c52e3e16f73b94cef975b5a31b2ee5476" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15609.ic5" merge="mpr-15609.ic5" size="2097152" crc="d586e455" sha1="aea190d31c590216eb19766ba749b1e9b710bdce" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15600.ic32" merge="mpr-15600.ic32" size="2097152" crc="d2698d23" sha1="996fbcc1d0814e6f14fa7e4870ece077ecda54e6" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15602.ic30" merge="mpr-15602.ic30" size="2097152" crc="1674764d" sha1="bc39757a5d25df1a088f874ca2442854eb551e48" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15604.ic28" merge="mpr-15604.ic28" size="2097152" crc="1552bbb9" sha1="77edd3f9d8dec87fa0445d264309e6164eba9313" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15606.ic26" merge="mpr-15606.ic26" size="2097152" crc="2b4f5265" sha1="48b4ccdedb52fbf80661ff380e5a273201fc0a12" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15601.ic31" merge="mpr-15601.ic31" size="2097152" crc="31a8f40a" sha1="62798346750dea87e43c8a8b01c33bf886bb50f4" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15603.ic29" merge="mpr-15603.ic29" size="2097152" crc="3805ecbc" sha1="54d29250441160f282c70adfd515adb21d2cda33" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15605.ic27" merge="mpr-15605.ic27" size="2097152" crc="cbdbf35e" sha1="a1c0900ac3210e72f5848561a6c4a77c804782c6" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15607.ic25" merge="mpr-15607.ic25" size="2097152" crc="6c8817c9" sha1="f5d493ed4237caf5042e95373bf9abd1fd16f873" region="mainpcb:sprites" offset="800006" />
    <rom name="15612" merge="15612" size="131072" crc="9d204617" sha1="8db57121065f5d1ac52fcfb88459bdbdc30e645b" region="user2" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="1" coins="2" service="yes">
      <control type="paddle" buttons="3" minimum="0" maximum="255" sensitivity="50" keydelta="20" />
      <control type="pedal" minimum="0" maximum="255" sensitivity="50" keydelta="20" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="f1lapt" sourcefile="segas32.cpp" cloneof="f1lap" romof="f1lap">
    <description>F1 Super Lap (World, Unprotected)</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15598.ic17" merge="epr-15598.ic17" size="131072" crc="9feab7cd" sha1="2a14c0df39e7bdae12a34679fabc6abb7618e27d" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15611t.ic8" size="131072" crc="7a57b792" sha1="77c96c841e90e9292182875822c85a2014d2d125" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-15596t.ic18" merge="epr-15596.ic18" size="262144" crc="20e92909" sha1="b974c79e11bfbd1cee61f9041cf79971fd96db3a" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15597t.ic9" merge="epr-15597.ic9" size="262144" crc="cd1ccddb" sha1="ff0371a8010141d1ab81b5eba555ae7c64e5da37" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-15592.ic36" merge="epr-15592.ic36" size="131072" crc="7c055cc8" sha1="169beb83dfae86dd408aa92b3c214b8f607825fc" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15593.ic35" merge="mpr-15593.ic35" size="1048576" crc="e7300441" sha1="33c264f0e6326689ba75026932c0932868e83b25" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15594.ic34" merge="mpr-15594.ic34" size="1048576" crc="7f4ca3bb" sha1="dc53a1857d619e574acb4c0587a6ba844df2d283" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15595.ic24" merge="mpr-15595.ic24" size="1048576" crc="3fbdad9a" sha1="573ea2242f79c7d3b6bf0e6745f6b07a621834ac" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-15608.ic14" merge="mpr-15608.ic14" size="2097152" crc="64462c69" sha1="9501e83c52e3e16f73b94cef975b5a31b2ee5476" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15609.ic5" merge="mpr-15609.ic5" size="2097152" crc="d586e455" sha1="aea190d31c590216eb19766ba749b1e9b710bdce" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15600.ic32" merge="mpr-15600.ic32" size="2097152" crc="d2698d23" sha1="996fbcc1d0814e6f14fa7e4870ece077ecda54e6" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15602.ic30" merge="mpr-15602.ic30" size="2097152" crc="1674764d" sha1="bc39757a5d25df1a088f874ca2442854eb551e48" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15604.ic28" merge="mpr-15604.ic28" size="2097152" crc="1552bbb9" sha1="77edd3f9d8dec87fa0445d264309e6164eba9313" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15606.ic26" merge="mpr-15606.ic26" size="2097152" crc="2b4f5265" sha1="48b4ccdedb52fbf80661ff380e5a273201fc0a12" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15601.ic31" merge="mpr-15601.ic31" size="2097152" crc="31a8f40a" sha1="62798346750dea87e43c8a8b01c33bf886bb50f4" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15603.ic29" merge="mpr-15603.ic29" size="2097152" crc="3805ecbc" sha1="54d29250441160f282c70adfd515adb21d2cda33" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15605.ic27" merge="mpr-15605.ic27" size="2097152" crc="cbdbf35e" sha1="a1c0900ac3210e72f5848561a6c4a77c804782c6" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15607.ic25" merge="mpr-15607.ic25" size="2097152" crc="6c8817c9" sha1="f5d493ed4237caf5042e95373bf9abd1fd16f873" region="mainpcb:sprites" offset="800006" />
    <rom name="15612" merge="15612" size="131072" crc="9d204617" sha1="8db57121065f5d1ac52fcfb88459bdbdc30e645b" region="user2" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="1" coins="2" service="yes">
      <control type="paddle" buttons="3" minimum="0" maximum="255" sensitivity="50" keydelta="20" />
      <control type="pedal" minimum="0" maximum="255" sensitivity="50" keydelta="20" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="ga2" sourcefile="segas32.cpp">
    <description>Golden Axe: The Revenge of Death Adder (World, Rev B)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14961b.ic17" size="131072" crc="d9cd8885" sha1="dc9d1f01770bd23ba5959e300badbc5093a149bc" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14958b.ic8" size="131072" crc="0be324a3" sha1="5e5f457548906453eaa8d326c353b47353eab73d" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-15148b.ic18" size="262144" crc="c477a9fd" sha1="a9d60f801c12fd067e5ad1801a92c84edd13bd08" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15147b.ic9" size="262144" crc="1bb676ea" sha1="125ffd13204f48be23e20b281c42c2307888c40b" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14945.ic36" size="65536" crc="4781d4cb" sha1="bd1b774b3cd0c3e0290c55e426f66d6820d21d0f" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14944.ic35" size="1048576" crc="fd4d4b86" sha1="e14b9cd6004bf9ecd902e37b433b828241361b46" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14943.ic34" size="1048576" crc="24d40333" sha1="38faf8f3eac317a163e93bd2247fe98189b13d2d" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14942.ic24" size="1048576" crc="a89b0e90" sha1="e14c62418eb7f9a2deb2a6dcf635bedc1c73c253" region="mainpcb:soundcpu" offset="300000" />
    <rom name="epr-14468-02.u3" size="65536" crc="77634daa" sha1="339169d164b9ed7dc3787b084d33effdc8e9efc1" region="mainpcb:mcu" offset="0" />
    <rom name="mpr-14948.ic14" size="2097152" crc="75050d4a" sha1="51d6bc9935abcf30af438e69c2cf4e09f57a803f" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14947.ic5" size="2097152" crc="b53e62f4" sha1="5aa0f198e6eb070b77b0d180d30c0228a9bc691e" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14949.ic32" size="2097152" crc="152c716c" sha1="448d16ea036b66e886119c00af543dfa5e53fd84" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14951.ic30" size="2097152" crc="fdb1a534" sha1="3126b595bf69bf9952fedf8f9c6743eb10489dc6" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14953.ic28" size="2097152" crc="33bd1c15" sha1="4e16562e3357d4db54b20543073e8f1fd6f74b1f" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14955.ic26" size="2097152" crc="e42684aa" sha1="12e0f18a11edb46f09e2e8c5c4ba14170d0cf00d" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14950.ic31" size="2097152" crc="15fd0026" sha1="e918984bd60ad63172fe273b31cc9019100228c8" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-14952.ic29" size="2097152" crc="96f96613" sha1="4c9808866032dab0401de322c28242e8a8775457" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-14954.ic27" size="2097152" crc="39b2ac9e" sha1="74f4c81d85ab9b4c5e8ae4b4d2c6dff766c482ca" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-14956.ic25" size="2097152" crc="298fca50" sha1="16e09b19cc7be3dfc8e82b45348e6d1cf2ed5621" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_v25" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <device_ref name="mb8421" />
    <device_ref name="v25" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="mainpcb:mcu" name="NEC V25" clock="10000000" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="2" service="yes">
      <control type="joy" player="1" buttons="3" ways="8" />
      <control type="joy" player="2" buttons="3" ways="8" />
      <control type="joy" player="3" buttons="3" ways="8" />
      <control type="joy" player="4" buttons="3" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="ga2j" sourcefile="segas32.cpp" cloneof="ga2" romof="ga2">
    <description>Golden Axe: The Revenge of Death Adder (Japan)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14959.ic17" size="131072" crc="f1929177" sha1="7dc39c40eff9fb46c2e51d1e83478cd6970e3951" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14946.ic8" size="131072" crc="eacafe94" sha1="d41a7e1ee2df9e053b559be0a1a6d2ae520fd3e4" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-14941.ic18" size="262144" crc="0ffb8203" sha1="b27dce634d203af8abb6ddfb656d4c48eb54af01" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14940.ic9" size="262144" crc="3b5b3084" sha1="ea17f6b7fd413fe3808f822cec84c993c9b75aa2" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14945.ic36" merge="epr-14945.ic36" size="65536" crc="4781d4cb" sha1="bd1b774b3cd0c3e0290c55e426f66d6820d21d0f" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14944.ic35" merge="mpr-14944.ic35" size="1048576" crc="fd4d4b86" sha1="e14b9cd6004bf9ecd902e37b433b828241361b46" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14943.ic34" merge="mpr-14943.ic34" size="1048576" crc="24d40333" sha1="38faf8f3eac317a163e93bd2247fe98189b13d2d" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14942.ic24" merge="mpr-14942.ic24" size="1048576" crc="a89b0e90" sha1="e14c62418eb7f9a2deb2a6dcf635bedc1c73c253" region="mainpcb:soundcpu" offset="300000" />
    <rom name="epr-14468-02.u3" merge="epr-14468-02.u3" size="65536" crc="77634daa" sha1="339169d164b9ed7dc3787b084d33effdc8e9efc1" region="mainpcb:mcu" offset="0" />
    <rom name="mpr-14948.ic14" merge="mpr-14948.ic14" size="2097152" crc="75050d4a" sha1="51d6bc9935abcf30af438e69c2cf4e09f57a803f" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14947.ic5" merge="mpr-14947.ic5" size="2097152" crc="b53e62f4" sha1="5aa0f198e6eb070b77b0d180d30c0228a9bc691e" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14949.ic32" merge="mpr-14949.ic32" size="2097152" crc="152c716c" sha1="448d16ea036b66e886119c00af543dfa5e53fd84" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14951.ic30" merge="mpr-14951.ic30" size="2097152" crc="fdb1a534" sha1="3126b595bf69bf9952fedf8f9c6743eb10489dc6" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14953.ic28" merge="mpr-14953.ic28" size="2097152" crc="33bd1c15" sha1="4e16562e3357d4db54b20543073e8f1fd6f74b1f" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14955.ic26" merge="mpr-14955.ic26" size="2097152" crc="e42684aa" sha1="12e0f18a11edb46f09e2e8c5c4ba14170d0cf00d" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14950.ic31" merge="mpr-14950.ic31" size="2097152" crc="15fd0026" sha1="e918984bd60ad63172fe273b31cc9019100228c8" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-14952.ic29" merge="mpr-14952.ic29" size="2097152" crc="96f96613" sha1="4c9808866032dab0401de322c28242e8a8775457" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-14954.ic27" merge="mpr-14954.ic27" size="2097152" crc="39b2ac9e" sha1="74f4c81d85ab9b4c5e8ae4b4d2c6dff766c482ca" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-14956.ic25" merge="mpr-14956.ic25" size="2097152" crc="298fca50" sha1="16e09b19cc7be3dfc8e82b45348e6d1cf2ed5621" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_v25" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <device_ref name="mb8421" />
    <device_ref name="v25" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="mainpcb:mcu" name="NEC V25" clock="10000000" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="2" service="yes">
      <control type="joy" player="1" buttons="3" ways="8" />
      <control type="joy" player="2" buttons="3" ways="8" />
      <control type="joy" player="3" buttons="3" ways="8" />
      <control type="joy" player="4" buttons="3" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="ga2u" sourcefile="segas32.cpp" cloneof="ga2" romof="ga2">
    <description>Golden Axe: The Revenge of Death Adder (US, Rev A)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14960a.ic17" size="131072" crc="87182fea" sha1="bb669ea7091f1ea34589a565490effa934ca44a3" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14957a.ic8" size="131072" crc="ab787cf4" sha1="7e19bb3e5d587b5009efc9f9fa52aecaef0eedc4" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-15146a.ic18" size="262144" crc="7293d5c3" sha1="535a8b4b4a05546b321cee8de6733edfc1f71589" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15145a.ic9" size="262144" crc="0da61782" sha1="f0302d747e5d55663095bb38732af423104c33ea" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14945.ic36" merge="epr-14945.ic36" size="65536" crc="4781d4cb" sha1="bd1b774b3cd0c3e0290c55e426f66d6820d21d0f" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14944.ic35" merge="mpr-14944.ic35" size="1048576" crc="fd4d4b86" sha1="e14b9cd6004bf9ecd902e37b433b828241361b46" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14943.ic34" merge="mpr-14943.ic34" size="1048576" crc="24d40333" sha1="38faf8f3eac317a163e93bd2247fe98189b13d2d" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14942.ic24" merge="mpr-14942.ic24" size="1048576" crc="a89b0e90" sha1="e14c62418eb7f9a2deb2a6dcf635bedc1c73c253" region="mainpcb:soundcpu" offset="300000" />
    <rom name="epr-14468-02.u3" merge="epr-14468-02.u3" size="65536" crc="77634daa" sha1="339169d164b9ed7dc3787b084d33effdc8e9efc1" region="mainpcb:mcu" offset="0" />
    <rom name="mpr-14948.ic14" merge="mpr-14948.ic14" size="2097152" crc="75050d4a" sha1="51d6bc9935abcf30af438e69c2cf4e09f57a803f" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14947.ic5" merge="mpr-14947.ic5" size="2097152" crc="b53e62f4" sha1="5aa0f198e6eb070b77b0d180d30c0228a9bc691e" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14949.ic32" merge="mpr-14949.ic32" size="2097152" crc="152c716c" sha1="448d16ea036b66e886119c00af543dfa5e53fd84" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14951.ic30" merge="mpr-14951.ic30" size="2097152" crc="fdb1a534" sha1="3126b595bf69bf9952fedf8f9c6743eb10489dc6" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14953.ic28" merge="mpr-14953.ic28" size="2097152" crc="33bd1c15" sha1="4e16562e3357d4db54b20543073e8f1fd6f74b1f" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14955.ic26" merge="mpr-14955.ic26" size="2097152" crc="e42684aa" sha1="12e0f18a11edb46f09e2e8c5c4ba14170d0cf00d" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14950.ic31" merge="mpr-14950.ic31" size="2097152" crc="15fd0026" sha1="e918984bd60ad63172fe273b31cc9019100228c8" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-14952.ic29" merge="mpr-14952.ic29" size="2097152" crc="96f96613" sha1="4c9808866032dab0401de322c28242e8a8775457" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-14954.ic27" merge="mpr-14954.ic27" size="2097152" crc="39b2ac9e" sha1="74f4c81d85ab9b4c5e8ae4b4d2c6dff766c482ca" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-14956.ic25" merge="mpr-14956.ic25" size="2097152" crc="298fca50" sha1="16e09b19cc7be3dfc8e82b45348e6d1cf2ed5621" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_v25" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <device_ref name="mb8421" />
    <device_ref name="v25" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="cpu" tag="mainpcb:mcu" name="NEC V25" clock="10000000" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="4" service="yes">
      <control type="joy" player="1" buttons="3" ways="8" />
      <control type="joy" player="2" buttons="3" ways="8" />
      <control type="joy" player="3" buttons="3" ways="8" />
      <control type="joy" player="4" buttons="3" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="harddunk" sourcefile="segas32.cpp">
    <description>Hard Dunk (World)</description>
    <year>1994</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16512.ic37" size="262144" crc="1a7de085" sha1="2e0dac1f7715089b7f6b1035c859ffe2d674932f" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16513.ic40" size="262144" crc="603dee75" sha1="32ae964a4b57d470b4900cca6e06329f1a75a6e6" region="mainpcb:maincpu" offset="2" />
    <rom name="epr-16505.ic31" size="131072" crc="eeb90a07" sha1="d1c2132897994b2e85fd5a97222b9fcd61bc421e" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16503.ic3" size="524288" crc="ac1b6f1a" sha1="56482931adf7fe551acf796b74cd8af3773d4fef" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16504.ic11" size="524288" crc="7c61fcd8" sha1="ca4354f90fada752bf11ee22a7798a8aa22b1c61" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16495.ic14" size="2097152" crc="6e5f26be" sha1="146761072bbed08f4a9df8a474b34fab61afaa4f" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16497.ic15" size="2097152" crc="42ab5859" sha1="f50c51eb81186aec5f747ecab4c5c928f8701afc" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16499.ic10" size="2097152" crc="a290ea36" sha1="2503b44174f23a9d323caab86553977d1d6d9c94" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16501.ic38" size="2097152" crc="f1566620" sha1="bcf31d11ee669d5afc7dc22c42fa59f4e48c1f50" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16496.ic22" size="2097152" crc="d9d27247" sha1="d211623478516ed1b89ab16a7fc7969954c5e353" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16498.ic23" size="2097152" crc="c022a991" sha1="a660a20692f4d9ba7be73577328f69f109be5e47" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16500.ic18" size="2097152" crc="452c0be3" sha1="af87ce4618bae2d791c1baed34ba7f853af664ff" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16502.ic41" size="2097152" crc="ffc3147e" sha1="12d882dec3098674d27058a8009e8778555f477a" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-16506.1" size="2097152" crc="e779f5ed" sha1="462d1bbe8bb12a0c5a6d6c613c720b26ec21cb25" region="mainpcb:sega" offset="0" />
    <rom name="mpr-16507.2" size="2097152" crc="31e068d3" sha1="9ac88b15af441fb3b31ce759c565b60a09039571" region="mainpcb:sega" offset="200000" />
    <device_ref name="segas32_pcb_multi_6player" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="6" coins="2" service="yes">
      <control type="joy" player="1" buttons="4" ways="8" />
      <control type="joy" player="2" buttons="4" ways="8" />
      <control type="joy" player="3" buttons="4" ways="8" />
      <control type="joy" player="4" buttons="4" ways="8" />
      <control type="joy" player="5" buttons="4" ways="8" />
      <control type="joy" player="6" buttons="4" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="harddunkj" sourcefile="segas32.cpp" cloneof="harddunk" romof="harddunk">
    <description>Hard Dunk (Japan)</description>
    <year>1994</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16508.ic37" size="262144" crc="b3713be5" sha1="8123638a838e41fcc0d32e14382421b521eff94f" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16509.ic40" merge="epr-16513.ic40" size="262144" crc="603dee75" sha1="32ae964a4b57d470b4900cca6e06329f1a75a6e6" region="mainpcb:maincpu" offset="2" />
    <rom name="epr-16505.ic31" merge="epr-16505.ic31" size="131072" crc="eeb90a07" sha1="d1c2132897994b2e85fd5a97222b9fcd61bc421e" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16503.ic3" merge="mpr-16503.ic3" size="524288" crc="ac1b6f1a" sha1="56482931adf7fe551acf796b74cd8af3773d4fef" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16504.ic11" merge="mpr-16504.ic11" size="524288" crc="7c61fcd8" sha1="ca4354f90fada752bf11ee22a7798a8aa22b1c61" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16495.ic14" merge="mpr-16495.ic14" size="2097152" crc="6e5f26be" sha1="146761072bbed08f4a9df8a474b34fab61afaa4f" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16497.ic15" merge="mpr-16497.ic15" size="2097152" crc="42ab5859" sha1="f50c51eb81186aec5f747ecab4c5c928f8701afc" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16499.ic10" merge="mpr-16499.ic10" size="2097152" crc="a290ea36" sha1="2503b44174f23a9d323caab86553977d1d6d9c94" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16501.ic38" merge="mpr-16501.ic38" size="2097152" crc="f1566620" sha1="bcf31d11ee669d5afc7dc22c42fa59f4e48c1f50" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16496.ic22" merge="mpr-16496.ic22" size="2097152" crc="d9d27247" sha1="d211623478516ed1b89ab16a7fc7969954c5e353" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16498.ic23" merge="mpr-16498.ic23" size="2097152" crc="c022a991" sha1="a660a20692f4d9ba7be73577328f69f109be5e47" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16500.ic18" merge="mpr-16500.ic18" size="2097152" crc="452c0be3" sha1="af87ce4618bae2d791c1baed34ba7f853af664ff" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16502.ic41" merge="mpr-16502.ic41" size="2097152" crc="ffc3147e" sha1="12d882dec3098674d27058a8009e8778555f477a" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-16506.ic1" merge="mpr-16506.1" size="2097152" crc="e779f5ed" sha1="462d1bbe8bb12a0c5a6d6c613c720b26ec21cb25" region="mainpcb:sega" offset="0" />
    <rom name="mpr-16507.ic2" merge="mpr-16507.2" size="2097152" crc="31e068d3" sha1="9ac88b15af441fb3b31ce759c565b60a09039571" region="mainpcb:sega" offset="200000" />
    <device_ref name="segas32_pcb_multi_6player" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="6" coins="2" service="yes">
      <control type="joy" player="1" buttons="4" ways="8" />
      <control type="joy" player="2" buttons="4" ways="8" />
      <control type="joy" player="3" buttons="4" ways="8" />
      <control type="joy" player="4" buttons="4" ways="8" />
      <control type="joy" player="5" buttons="4" ways="8" />
      <control type="joy" player="6" buttons="4" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="holo" sourcefile="segas32.cpp">
    <description>Holosseum (US, Rev A)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14977a" size="131072" crc="e0d7e288" sha1="3126041ba73f21fac0207bf5c63230c61180f564" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14976a" size="131072" crc="e56f13be" sha1="3d9e7add8feaa35c4c2e8bda84ae251087bd5e40" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-15011" size="131072" crc="b9f59f59" sha1="f8c91fa877cf53153bec3d7850eab38227cc18ba" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15010" size="131072" crc="0c09c57b" sha1="028a9fe1c625be218ba90906308d25d69d4de4c4" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14965" size="131072" crc="3a918cfe" sha1="f43ecbc9e774873e868bc921321541b308ea1a3c" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14964" size="1048576" crc="7ff581d5" sha1="ab81bd70937319e4edc8924bdb493d5ef1ec096a" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14963" size="1048576" crc="0974a60e" sha1="87d770edcee9c9e8f37d36ab28c5aa5d685ea849" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14962" size="1048576" crc="6b2e694e" sha1="7874bdfd534231c7756e0e0d9fc7a3d5bdba74d3" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14973" size="1048576" crc="b3c3ff6b" sha1="94e8dbfae37a5b122ee3d471aad1f758e4a39b9e" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14972" size="1048576" crc="0c161374" sha1="413ab45deb687ecdbdc06ae98aa32ad8a0d80e0c" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-14971" size="1048576" crc="dfcf6fdf" sha1="417291b54010be20dd6738a70d372b580615a8bb" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14970" size="1048576" crc="cae3a745" sha1="b6cc1f4abb460cda4714967e880928dc727ecf0a" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-14969" size="1048576" crc="c06b7c15" sha1="8b97a899e6eacf798b9f55af8df95e12ccacadec" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14968" size="1048576" crc="f413894a" sha1="d65f57b1e55199e901c7c2f701589c46eeab739a" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-14967" size="1048576" crc="5377fce0" sha1="baf8f82ab851b24202938fc7213d72324b9b92c0" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14966" size="1048576" crc="dffba2e9" sha1="b97e47e78abb8302bc2c87681643382203bd76eb" region="mainpcb:sprites" offset="7" />
    <device_ref name="segas32_pcb_regular" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="180" flipx="yes" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="2" ways="8" />
      <control type="joy" player="2" buttons="2" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="jleague" sourcefile="segas32.cpp" cloneof="svf" romof="svf">
    <description>The J.League 1994 (Japan, Rev A)</description>
    <year>1994</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16782a.ic17" size="131072" crc="b399ac47" sha1="b7a2bfaf6ea2f98e177e3f4542f5b37ec9b00c8a" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16781a.ic8" size="131072" crc="e6d80225" sha1="bc9fd6b9e4019e01b9a496064e3b3209f31590e4" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-16776.ic18" size="524288" crc="e8694626" sha1="d4318a9a6b1cc5c719bff9c25b7398dd2ea1e18b" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-16775.ic9" size="524288" crc="e81e2c3d" sha1="2900710f1dec6cf71875c82a56584ba45ed3a545" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-16780.ic36" size="262144" crc="47aa4ec7" sha1="baea18aaac0314f769f1e36fdbe8aedf62862544" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16779.ic35" merge="mpr-16779.ic35" size="1048576" crc="7055e859" sha1="cde27fa4aaf0ee54063ee68794e9a6075581fff5" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16778.ic34" merge="mpr-16778.ic34" size="1048576" crc="feedaecf" sha1="25c14ccb85c467dc0c8e85b61f8f86f4396c0cc7" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-16777.ic24" merge="mpr-16777.ic24" size="1048576" crc="14b5d5df" sha1="1b0b0a31294b1bbc16d2046b374d584a1b00a78c" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-16784.ic14" merge="mpr-16784.ic14" size="1048576" crc="4608efe2" sha1="9b41aa28f50af770e854ef9fdff1a55da7b7b131" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16783.ic5" merge="mpr-16783.ic5" size="1048576" crc="042eabe7" sha1="a11df5c21d85f0c96dbdcaf57be37a79658ad648" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16785.ic32" merge="mpr-16785.ic32" size="2097152" crc="51f775ce" sha1="125b40bf47304d37b92e81df5081c81d9af6c8a2" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16787.ic30" merge="mpr-16787.ic30" size="2097152" crc="dee7a204" sha1="29acff4d5dd68609ac46853860788206d18262ab" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16789.ic28" merge="mpr-16789.ic28" size="2097152" crc="6b6c8ad3" sha1="97b0078c851845c31dcf0fe4b2a88393dcdf8988" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16791.ic26" merge="mpr-16791.ic26" size="2097152" crc="4f7236da" sha1="d1c29f6aa82d60a626217f1430bc8a76ef012007" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16786.ic31" size="2097152" crc="d08a2d32" sha1="baac63cbacbe38e057684174040384a7152eb523" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16788.ic29" size="2097152" crc="cd9d3605" sha1="7c4402be1a1ddde6766cfdd5fe7e2a088c4a59e8" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16790.ic27" size="2097152" crc="2ea75746" sha1="c91e5d678917886cc23fbef7a577c5a70665c7b2" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16792.ic25" size="2097152" crc="9f416072" sha1="18107cf64f918888aa5a54432f8e9137910101b8" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_regular" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="3" ways="8" />
      <control type="joy" player="2" buttons="3" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="jleagueo" sourcefile="segas32.cpp" cloneof="svf" romof="svf">
    <description>The J.League 1994 (Japan)</description>
    <year>1994</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16782.ic17" size="131072" crc="f0278944" sha1="49e3842231ee5abdd6205b598309153d6b4ddc02" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16781.ic8" size="131072" crc="7df9529b" sha1="de3633f4941ff3877c4cb8b53e080eccea19f22e" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-16776.ic18" size="524288" crc="e8694626" sha1="d4318a9a6b1cc5c719bff9c25b7398dd2ea1e18b" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-16775.ic9" size="524288" crc="e81e2c3d" sha1="2900710f1dec6cf71875c82a56584ba45ed3a545" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-16780.ic36" size="262144" crc="47aa4ec7" sha1="baea18aaac0314f769f1e36fdbe8aedf62862544" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16779.ic35" merge="mpr-16779.ic35" size="1048576" crc="7055e859" sha1="cde27fa4aaf0ee54063ee68794e9a6075581fff5" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16778.ic34" merge="mpr-16778.ic34" size="1048576" crc="feedaecf" sha1="25c14ccb85c467dc0c8e85b61f8f86f4396c0cc7" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-16777.ic24" merge="mpr-16777.ic24" size="1048576" crc="14b5d5df" sha1="1b0b0a31294b1bbc16d2046b374d584a1b00a78c" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-16784.ic14" merge="mpr-16784.ic14" size="1048576" crc="4608efe2" sha1="9b41aa28f50af770e854ef9fdff1a55da7b7b131" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16783.ic5" merge="mpr-16783.ic5" size="1048576" crc="042eabe7" sha1="a11df5c21d85f0c96dbdcaf57be37a79658ad648" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16785.ic32" merge="mpr-16785.ic32" size="2097152" crc="51f775ce" sha1="125b40bf47304d37b92e81df5081c81d9af6c8a2" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16787.ic30" merge="mpr-16787.ic30" size="2097152" crc="dee7a204" sha1="29acff4d5dd68609ac46853860788206d18262ab" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16789.ic28" merge="mpr-16789.ic28" size="2097152" crc="6b6c8ad3" sha1="97b0078c851845c31dcf0fe4b2a88393dcdf8988" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16791.ic26" merge="mpr-16791.ic26" size="2097152" crc="4f7236da" sha1="d1c29f6aa82d60a626217f1430bc8a76ef012007" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16786.ic31" size="2097152" crc="d08a2d32" sha1="baac63cbacbe38e057684174040384a7152eb523" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16788.ic29" size="2097152" crc="cd9d3605" sha1="7c4402be1a1ddde6766cfdd5fe7e2a088c4a59e8" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16790.ic27" size="2097152" crc="2ea75746" sha1="c91e5d678917886cc23fbef7a577c5a70665c7b2" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16792.ic25" size="2097152" crc="9f416072" sha1="18107cf64f918888aa5a54432f8e9137910101b8" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_regular" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="3" ways="8" />
      <control type="joy" player="2" buttons="3" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="jpark" sourcefile="segas32.cpp">
    <description>Jurassic Park (World, Rev A)</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16402a.ic8" size="524288" crc="c70db239" sha1="fd79dfd1ce194fcc8ccb58117bc845cdfe9943b1" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16395.ic18" size="524288" crc="ac5a01d6" sha1="df6bffdf5723cb8790a9c1c0ab271989a758bdd8" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-16394.ic9" size="524288" crc="c08c3a8a" sha1="923cf256d863656336401fa75103b42298cb3822" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-16399.ic36" size="262144" crc="b09b2fe3" sha1="bf8d646bab65fcc4ece8c2bd9a3df389e5860ed6" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16398.ic35" size="1048576" crc="fa710ca6" sha1="1fd625070eef5f99d7be07606aeeff9282e32532" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16397.ic34" size="1048576" crc="6e96e0be" sha1="422b783b72127b80a23043b2dd1c04f5772f436e" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-16396.ic24" size="1048576" crc="f69a2dc4" sha1="3f02b10976852916c58e852f3161a857784fe36b" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-16404.ic14" size="2097152" crc="11283807" sha1="99e465c3fc31e640740b8257a349e203f026754a" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16403.ic5" size="2097152" crc="02530a9b" sha1="b43e1b47f74c801bfc599cbe893fb8dc13453dd0" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16405.ic32" size="2097152" crc="b425f182" sha1="66c6bd29dd3450db816b895c4c9c5208a66aae67" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16407.ic30" size="2097152" crc="bc49ffd9" sha1="a50ba7ddccfdfd7638c4041978b39c1559afbbb4" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16409.ic28" size="2097152" crc="fe73660d" sha1="ec1a3ea5303d2ccb9e327da18476969953626e1c" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16411.ic26" size="2097152" crc="71cabbc5" sha1="9760f57ef43eb251488dadd37711d5682d902434" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16406.ic31" size="2097152" crc="b9ed73d6" sha1="0dd22e7a21e95d84fc91acd742c737f96529f515" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16408.ic29" size="2097152" crc="7b2f476b" sha1="da99a9911982ba8aaef8c9aecc2977c9fd6da094" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16410.ic27" size="2097152" crc="49c8f952" sha1="f26b818711910b10bf520e5f849a1478a6b1d6e6" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16412.ic25" size="2097152" crc="105dc26e" sha1="fd2ef8c9fe1a78b4f9cc891a6fbd060184e58a1f" region="mainpcb:sprites" offset="800006" />
    <rom name="epr-13908.xx" size="32768" crc="6228c1d2" sha1="bd37fe775534fb94c9af80546948ce5f9c47bbf5" region="cpu2" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes" tilt="yes">
      <control type="stick" player="1" buttons="1" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
      <control type="stick" player="2" buttons="1" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="jparkj" sourcefile="segas32.cpp" cloneof="jpark" romof="jpark">
    <description>Jurassic Park (Japan, Rev A, Deluxe)</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16400a.ic8" size="524288" crc="1e03dbfe" sha1="b7c274769ff483e687749ff20b1dc0fc38e8ef82" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16395.ic18" merge="epr-16395.ic18" size="524288" crc="ac5a01d6" sha1="df6bffdf5723cb8790a9c1c0ab271989a758bdd8" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-16394.ic9" merge="epr-16394.ic9" size="524288" crc="c08c3a8a" sha1="923cf256d863656336401fa75103b42298cb3822" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-16399.ic36" merge="epr-16399.ic36" size="262144" crc="b09b2fe3" sha1="bf8d646bab65fcc4ece8c2bd9a3df389e5860ed6" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16398.ic35" merge="mpr-16398.ic35" size="1048576" crc="fa710ca6" sha1="1fd625070eef5f99d7be07606aeeff9282e32532" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16397.ic34" merge="mpr-16397.ic34" size="1048576" crc="6e96e0be" sha1="422b783b72127b80a23043b2dd1c04f5772f436e" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-16396.ic24" merge="mpr-16396.ic24" size="1048576" crc="f69a2dc4" sha1="3f02b10976852916c58e852f3161a857784fe36b" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-16404.ic14" merge="mpr-16404.ic14" size="2097152" crc="11283807" sha1="99e465c3fc31e640740b8257a349e203f026754a" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16403.ic5" merge="mpr-16403.ic5" size="2097152" crc="02530a9b" sha1="b43e1b47f74c801bfc599cbe893fb8dc13453dd0" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16405.ic32" merge="mpr-16405.ic32" size="2097152" crc="b425f182" sha1="66c6bd29dd3450db816b895c4c9c5208a66aae67" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16407.ic30" merge="mpr-16407.ic30" size="2097152" crc="bc49ffd9" sha1="a50ba7ddccfdfd7638c4041978b39c1559afbbb4" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16409.ic28" merge="mpr-16409.ic28" size="2097152" crc="fe73660d" sha1="ec1a3ea5303d2ccb9e327da18476969953626e1c" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16411.ic26" merge="mpr-16411.ic26" size="2097152" crc="71cabbc5" sha1="9760f57ef43eb251488dadd37711d5682d902434" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16406.ic31" merge="mpr-16406.ic31" size="2097152" crc="b9ed73d6" sha1="0dd22e7a21e95d84fc91acd742c737f96529f515" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16408.ic29" merge="mpr-16408.ic29" size="2097152" crc="7b2f476b" sha1="da99a9911982ba8aaef8c9aecc2977c9fd6da094" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16410.ic27" merge="mpr-16410.ic27" size="2097152" crc="49c8f952" sha1="f26b818711910b10bf520e5f849a1478a6b1d6e6" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16412.ic25" merge="mpr-16412.ic25" size="2097152" crc="105dc26e" sha1="fd2ef8c9fe1a78b4f9cc891a6fbd060184e58a1f" region="mainpcb:sprites" offset="800006" />
    <rom name="epr-13908.xx" merge="epr-13908.xx" size="32768" crc="6228c1d2" sha1="bd37fe775534fb94c9af80546948ce5f9c47bbf5" region="cpu2" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes" tilt="yes">
      <control type="stick" player="1" buttons="1" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
      <control type="stick" player="2" buttons="1" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="jparkja" sourcefile="segas32.cpp" cloneof="jpark" romof="jpark">
    <description>Jurassic Park (Japan, Deluxe)</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16400.ic8" size="524288" crc="321c3411" sha1="c53e7ed5f2e523741a521c9cd271123ab557cc4a" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16395.ic18" merge="epr-16395.ic18" size="524288" crc="ac5a01d6" sha1="df6bffdf5723cb8790a9c1c0ab271989a758bdd8" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-16394.ic9" merge="epr-16394.ic9" size="524288" crc="c08c3a8a" sha1="923cf256d863656336401fa75103b42298cb3822" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-16399.ic36" merge="epr-16399.ic36" size="262144" crc="b09b2fe3" sha1="bf8d646bab65fcc4ece8c2bd9a3df389e5860ed6" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16398.ic35" merge="mpr-16398.ic35" size="1048576" crc="fa710ca6" sha1="1fd625070eef5f99d7be07606aeeff9282e32532" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16397.ic34" merge="mpr-16397.ic34" size="1048576" crc="6e96e0be" sha1="422b783b72127b80a23043b2dd1c04f5772f436e" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-16396.ic24" merge="mpr-16396.ic24" size="1048576" crc="f69a2dc4" sha1="3f02b10976852916c58e852f3161a857784fe36b" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-16404.ic14" merge="mpr-16404.ic14" size="2097152" crc="11283807" sha1="99e465c3fc31e640740b8257a349e203f026754a" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16403.ic5" merge="mpr-16403.ic5" size="2097152" crc="02530a9b" sha1="b43e1b47f74c801bfc599cbe893fb8dc13453dd0" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16405.ic32" merge="mpr-16405.ic32" size="2097152" crc="b425f182" sha1="66c6bd29dd3450db816b895c4c9c5208a66aae67" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16407.ic30" merge="mpr-16407.ic30" size="2097152" crc="bc49ffd9" sha1="a50ba7ddccfdfd7638c4041978b39c1559afbbb4" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16409.ic28" merge="mpr-16409.ic28" size="2097152" crc="fe73660d" sha1="ec1a3ea5303d2ccb9e327da18476969953626e1c" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16411.ic26" merge="mpr-16411.ic26" size="2097152" crc="71cabbc5" sha1="9760f57ef43eb251488dadd37711d5682d902434" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16406.ic31" merge="mpr-16406.ic31" size="2097152" crc="b9ed73d6" sha1="0dd22e7a21e95d84fc91acd742c737f96529f515" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16408.ic29" merge="mpr-16408.ic29" size="2097152" crc="7b2f476b" sha1="da99a9911982ba8aaef8c9aecc2977c9fd6da094" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16410.ic27" merge="mpr-16410.ic27" size="2097152" crc="49c8f952" sha1="f26b818711910b10bf520e5f849a1478a6b1d6e6" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16412.ic25" merge="mpr-16412.ic25" size="2097152" crc="105dc26e" sha1="fd2ef8c9fe1a78b4f9cc891a6fbd060184e58a1f" region="mainpcb:sprites" offset="800006" />
    <rom name="epr-13908.xx" merge="epr-13908.xx" size="32768" crc="6228c1d2" sha1="bd37fe775534fb94c9af80546948ce5f9c47bbf5" region="cpu2" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes" tilt="yes">
      <control type="stick" player="1" buttons="1" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
      <control type="stick" player="2" buttons="1" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="jparkjc" sourcefile="segas32.cpp" cloneof="jpark" romof="jpark">
    <description>Jurassic Park (Japan, Rev A, Conversion)</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16400a.ic8" size="524288" crc="1e03dbfe" sha1="b7c274769ff483e687749ff20b1dc0fc38e8ef82" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16395.ic18" merge="epr-16395.ic18" size="524288" crc="ac5a01d6" sha1="df6bffdf5723cb8790a9c1c0ab271989a758bdd8" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-16394.ic9" merge="epr-16394.ic9" size="524288" crc="c08c3a8a" sha1="923cf256d863656336401fa75103b42298cb3822" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-16630.ic36" size="262144" crc="955855eb" sha1="c7a325ba0009139c2cc263cd457dbc0d527c7582" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16398.ic35" merge="mpr-16398.ic35" size="1048576" crc="fa710ca6" sha1="1fd625070eef5f99d7be07606aeeff9282e32532" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16397.ic34" merge="mpr-16397.ic34" size="1048576" crc="6e96e0be" sha1="422b783b72127b80a23043b2dd1c04f5772f436e" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-16396.ic24" merge="mpr-16396.ic24" size="1048576" crc="f69a2dc4" sha1="3f02b10976852916c58e852f3161a857784fe36b" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-16404.ic14" merge="mpr-16404.ic14" size="2097152" crc="11283807" sha1="99e465c3fc31e640740b8257a349e203f026754a" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16403.ic5" merge="mpr-16403.ic5" size="2097152" crc="02530a9b" sha1="b43e1b47f74c801bfc599cbe893fb8dc13453dd0" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16405.ic32" merge="mpr-16405.ic32" size="2097152" crc="b425f182" sha1="66c6bd29dd3450db816b895c4c9c5208a66aae67" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16407.ic30" merge="mpr-16407.ic30" size="2097152" crc="bc49ffd9" sha1="a50ba7ddccfdfd7638c4041978b39c1559afbbb4" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16409.ic28" merge="mpr-16409.ic28" size="2097152" crc="fe73660d" sha1="ec1a3ea5303d2ccb9e327da18476969953626e1c" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16411.ic26" merge="mpr-16411.ic26" size="2097152" crc="71cabbc5" sha1="9760f57ef43eb251488dadd37711d5682d902434" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16406.ic31" merge="mpr-16406.ic31" size="2097152" crc="b9ed73d6" sha1="0dd22e7a21e95d84fc91acd742c737f96529f515" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16408.ic29" merge="mpr-16408.ic29" size="2097152" crc="7b2f476b" sha1="da99a9911982ba8aaef8c9aecc2977c9fd6da094" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16410.ic27" merge="mpr-16410.ic27" size="2097152" crc="49c8f952" sha1="f26b818711910b10bf520e5f849a1478a6b1d6e6" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16412.ic25" merge="mpr-16412.ic25" size="2097152" crc="105dc26e" sha1="fd2ef8c9fe1a78b4f9cc891a6fbd060184e58a1f" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes" tilt="yes">
      <control type="stick" player="1" buttons="1" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
      <control type="stick" player="2" buttons="1" minimum="0" maximum="255" sensitivity="50" keydelta="5" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="kokoroj" sourcefile="segas32.cpp">
    <description>Soreike Kokology (Rev A)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15524a.ic8" size="131072" crc="3b4cc0cf" sha1="2536c67ac4255cdb6988d37f48f91ad272aebb4f" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15521a.ic18" size="524288" crc="24c02cf9" sha1="d2ab8a47ff6541d2a6be7ce50784b8c9a3a215be" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15520a.ic9" size="524288" crc="bfbae875" sha1="340c1e07eeb8e15448f82b87cc749d66086130ab" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-15523.ic36" size="131072" crc="b3b9d29c" sha1="22acd747540e8c4558ec5eaeda1aaab68f84a6e2" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15522.ic35" size="524288" crc="fb68a351" sha1="f307c0e4f33786630e8baddbb8c0a5e0f956de76" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15526.ic14" size="1048576" crc="f6907c13" sha1="d3f65dd02d7cee0fd2f422ba6a54164b2a2b8303" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15525.ic5" size="1048576" crc="8c0c876f" sha1="e5335fa7a3e4a0e1d79fc7612bf4aaa50224f4ca" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15527.ic32" size="2097152" crc="132f91c6" sha1="0f854b173bdebfb642dba3b58a307d0e3a157c85" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15529.ic30" size="2097152" crc="c1b826f7" sha1="00051762074cdcf62b07cea6c744244b11ebf1b1" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15531.ic28" size="2097152" crc="d624e05f" sha1="f19f173aaeb04a59ab7fe89a3490d1d7c13c77a0" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15533.ic26" size="2097152" crc="aff0e9a8" sha1="5ced176cfef65426e2b4a3b990a319fdceaa9162" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15528.ic31" size="2097152" crc="2e4bc090" sha1="67d464ea078a19ae303b2b60f4ab0abd71aea85c" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15530.ic29" size="2097152" crc="307877a8" sha1="0104a51349f745a9fb7cc238a832ef6abeec2025" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15532.ic27" size="2097152" crc="923ba3e5" sha1="d26c55e7021c81b5fdaa9fadee20db30f6677981" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15534.ic25" size="2097152" crc="4fa5c56d" sha1="52926bef0f21ef17dc9d49e3137712bf6d8c29af" region="mainpcb:sprites" offset="800006" />
    <disk name="kokoroj" status="nodump" region="mainpcb:scsi:1:cdrom" index="0" writable="no" />
    <device_ref name="segas32_pcb_cd" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="mb89352" />
    <device_ref name="scsi" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsicd" />
    <device_ref name="cdrom_image" />
    <device_ref name="cdda" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsi_slot" />
    <device_ref name="cxd1095" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <chip type="audio" tag="mainpcb:scsi:1:cdrom:cdda" name="CD/DA" clock="44100" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="2" service="yes">
      <control type="only_buttons" player="1" buttons="4" />
      <control type="only_buttons" player="2" buttons="4" />
      <control type="only_buttons" player="3" buttons="4" />
      <control type="only_buttons" player="4" buttons="4" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="CD &amp; Printer" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="0" default="yes" />
      <dipvalue name="On" value="8" />
    </dipswitch>
    <configuration name="SCSI ID" tag="mainpcb:scsi:1:cdrom:SCSI_ID" mask="7">
      <confsetting name="0" value="0" default="yes" />
      <confsetting name="1" value="1" />
      <confsetting name="2" value="2" />
      <confsetting name="3" value="3" />
      <confsetting name="4" value="4" />
      <confsetting name="5" value="5" />
      <confsetting name="6" value="6" />
      <confsetting name="7" value="7" />
    </configuration>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:scsi:1:cdrom:SCSI_ID" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
    <feature type="sound" status="imperfect" />
    <feature type="printer" status="unemulated" />
    <device type="cdrom" tag="mainpcb:scsi:1:cdrom:image" interface="cdrom">
      <instance name="cdrom" briefname="cdrm" />
      <extension name="chd" />
      <extension name="cue" />
      <extension name="toc" />
      <extension name="nrg" />
      <extension name="gdi" />
      <extension name="iso" />
      <extension name="cdr" />
    </device>
    <slot name="mainpcb:scsi:1">
      <slotoption name="cdrom" devname="scsicd" default="yes" />
    </slot>
    <slot name="mainpcb:scsi:2" />
    <slot name="mainpcb:scsi:3" />
    <slot name="mainpcb:scsi:4" />
    <slot name="mainpcb:scsi:5" />
    <slot name="mainpcb:scsi:6" />
    <slot name="mainpcb:scsi:7" />
  </machine>
  <machine name="kokoroj2" sourcefile="segas32.cpp">
    <description>Soreike Kokology Vol. 2 - Kokoro no Tanteikyoku</description>
    <year>1993</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16186.ic8" size="131072" crc="8c3afb6e" sha1="68c3c066a943b1ea8e3bee06c7c8279b5a12e7f7" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16183.ic18" size="524288" crc="4844432f" sha1="b127169d0f108e0b99ec81814a5c3c45bb82e0b1" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-16182.ic9" size="524288" crc="a27f5f5f" sha1="c2bbd1632bce0851cf8ab45d3ccbec1076e67f5e" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-16185.ic36" size="131072" crc="afb97c4d" sha1="f6e77d932824f93d89559a9cb3b2d678d5fc6940" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16184.ic35" size="1048576" crc="d7a19751" sha1="8ae9f13689c8f9851e1eea995c51285972bed4a2" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16188.ic14" size="2097152" crc="83a450ab" sha1="1d0b45512d784ed1d82135b84c7c540f92d789f7" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16187.ic5" size="2097152" crc="98b62f8b" sha1="eaf98efd9eac7b7c385138a8a4dbc94b0ca38df5" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16189.ic32" size="2097152" crc="0937f713" sha1="4b2b09ec8ed97794ad3824d1c57eae7f7e01379c" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16191.ic30" size="2097152" crc="cfef4aaa" sha1="bc8a252dcbdb8facdd91eda7aed0f56fe7529d15" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16193.ic28" size="2097152" crc="a0706e4e" sha1="1f36d952971c05db4190b229aa4957db3e5224f1" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16195.ic26" size="2097152" crc="a4ddcd61" sha1="90ef40f1fc84d1e4d4f78c33b8f0d1f56e04bf90" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16190.ic31" size="2097152" crc="528d408e" sha1="89f8a2cfc8b59377d6a65555c3172e457b131502" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16192.ic29" size="2097152" crc="efaa93d1" sha1="2947eaf7fc358ced1c04e7abe7a3f3066c73f2d0" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16194.ic27" size="2097152" crc="39b5efe7" sha1="2039909a2dd46951d442f1b6377f365525f9f2f1" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16196.ic25" size="2097152" crc="b8e22e05" sha1="dd667e2c5d421cba356421825e6aca9b5ca0af45" region="mainpcb:sprites" offset="800006" />
    <disk name="cdp-00146" sha1="0b37e0ea2380ecd9abef2ccd6a8096d76d2ba344" region="mainpcb:scsi:1:cdrom" index="0" writable="no" />
    <device_ref name="segas32_pcb_cd" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="mb89352" />
    <device_ref name="scsi" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsicd" />
    <device_ref name="cdrom_image" />
    <device_ref name="cdda" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsi_slot" />
    <device_ref name="scsi_slot" />
    <device_ref name="cxd1095" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <chip type="audio" tag="mainpcb:scsi:1:cdrom:cdda" name="CD/DA" clock="44100" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="2" service="yes">
      <control type="only_buttons" player="1" buttons="4" />
      <control type="only_buttons" player="2" buttons="4" />
      <control type="only_buttons" player="3" buttons="4" />
      <control type="only_buttons" player="4" buttons="4" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="CD &amp; Printer" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="0" default="yes" />
      <dipvalue name="On" value="8" />
    </dipswitch>
    <configuration name="SCSI ID" tag="mainpcb:scsi:1:cdrom:SCSI_ID" mask="7">
      <confsetting name="0" value="0" default="yes" />
      <confsetting name="1" value="1" />
      <confsetting name="2" value="2" />
      <confsetting name="3" value="3" />
      <confsetting name="4" value="4" />
      <confsetting name="5" value="5" />
      <confsetting name="6" value="6" />
      <confsetting name="7" value="7" />
    </configuration>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:scsi:1:cdrom:SCSI_ID" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
    <feature type="sound" status="imperfect" />
    <feature type="printer" status="unemulated" />
    <device type="cdrom" tag="mainpcb:scsi:1:cdrom:image" interface="cdrom">
      <instance name="cdrom" briefname="cdrm" />
      <extension name="chd" />
      <extension name="cue" />
      <extension name="toc" />
      <extension name="nrg" />
      <extension name="gdi" />
      <extension name="iso" />
      <extension name="cdr" />
    </device>
    <slot name="mainpcb:scsi:1">
      <slotoption name="cdrom" devname="scsicd" default="yes" />
    </slot>
    <slot name="mainpcb:scsi:2" />
    <slot name="mainpcb:scsi:3" />
    <slot name="mainpcb:scsi:4" />
    <slot name="mainpcb:scsi:5" />
    <slot name="mainpcb:scsi:6" />
    <slot name="mainpcb:scsi:7" />
  </machine>
  <machine name="orunners" sourcefile="segas32.cpp">
    <description>OutRunners (World)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15620.ic37" size="131072" crc="84f5ad92" sha1="1f9cb04b42b2d450be93400d9979a7910eaf05d1" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15621.ic40" size="131072" crc="d98b765a" sha1="b58567e976228267a86af53de2135bc0b247a44a" region="mainpcb:maincpu" offset="2" />
    <rom name="mpr-15538.ic36" size="524288" crc="93958820" sha1="e19b6f18a5707dbb64ae009d63c05eac5bac4a81" region="mainpcb:maincpu" offset="100000" />
    <rom name="mpr-15539.ic39" size="524288" crc="219760fa" sha1="bd62a83de9c9542f6da454a87dc4947492f65c52" region="mainpcb:maincpu" offset="100002" />
    <rom name="epr-15550.ic31" size="524288" crc="0205d2ed" sha1="3475479e1a45fe96eefbe53842758898db7accbf" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15548.ic3" size="2097152" crc="b6470a66" sha1="e1544590c02d41f62f82a4d771b893fb0f2734c7" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15549.ic11" size="2097152" crc="81d12520" sha1="1555893941e832f00ad3d0b3ad0c34a0d3a1c58a" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15540.ic14" size="2097152" crc="a10d72b4" sha1="6d9d5e20be6721b53ce49df4d5a1bbd91f5b3aed" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15542.ic15" size="2097152" crc="40952374" sha1="c669ef52508bc2f49cf812dc86ac98fb535471fa" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15544.ic10" size="2097152" crc="39e3df45" sha1="38a7b21617b45613b05509dda388f8f7770b186c" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15546.ic38" size="2097152" crc="e3fcc12c" sha1="1cf7e05c7873f68789a27a91cddf471df40d7907" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15541.ic22" size="2097152" crc="a2003c2d" sha1="200a2c7d78d3f5f28909267fdcdbddd58c5f5fa2" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15543.ic23" size="2097152" crc="933e8e7b" sha1="0d53286f524f47851a483569dc37e9f6d34cc5f4" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15545.ic18" size="2097152" crc="53dd0235" sha1="4aee5ae1820ff933b6bd8a54bdbf989c0bc95c1a" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15547.ic41" size="2097152" crc="edcb2a43" sha1="f0bcfcc749ca0267f85bf9838164869912944d00" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-15551.ic1" size="2097152" crc="4894bc73" sha1="351f5c03fb430fd87df915dfe3a377b5ada622c4" region="mainpcb:sega" offset="0" />
    <rom name="mpr-15552.ic2" size="2097152" crc="1c4b5e73" sha1="50a8e9a200575a3522a51bf094aa0e87b90bb0a3" region="mainpcb:sega" offset="200000" />
    <device_ref name="segas32_pcb_multi_analog" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="paddle" player="1" buttons="5" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" player="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="paddle" player="2" buttons="5" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" player="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG7">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG8">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="orunnersj" sourcefile="segas32.cpp" cloneof="orunners" romof="orunners">
    <description>OutRunners (Japan)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15616.ic37" size="131072" crc="fb550545" sha1="2f2c36843b115f5417e1f2ccd4a34ebf91265190" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15617.ic40" size="131072" crc="6bb741e0" sha1="d92087a2c0b6de4287e569eecf9758615a85d1eb" region="mainpcb:maincpu" offset="2" />
    <rom name="mpr-15538.ic36" merge="mpr-15538.ic36" size="524288" crc="93958820" sha1="e19b6f18a5707dbb64ae009d63c05eac5bac4a81" region="mainpcb:maincpu" offset="100000" />
    <rom name="mpr-15539.ic39" merge="mpr-15539.ic39" size="524288" crc="219760fa" sha1="bd62a83de9c9542f6da454a87dc4947492f65c52" region="mainpcb:maincpu" offset="100002" />
    <rom name="epr-15550.ic31" merge="epr-15550.ic31" size="524288" crc="0205d2ed" sha1="3475479e1a45fe96eefbe53842758898db7accbf" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15548.ic3" merge="mpr-15548.ic3" size="2097152" crc="b6470a66" sha1="e1544590c02d41f62f82a4d771b893fb0f2734c7" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15549.ic11" merge="mpr-15549.ic11" size="2097152" crc="81d12520" sha1="1555893941e832f00ad3d0b3ad0c34a0d3a1c58a" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15540.ic14" merge="mpr-15540.ic14" size="2097152" crc="a10d72b4" sha1="6d9d5e20be6721b53ce49df4d5a1bbd91f5b3aed" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15542.ic15" merge="mpr-15542.ic15" size="2097152" crc="40952374" sha1="c669ef52508bc2f49cf812dc86ac98fb535471fa" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15544.ic10" merge="mpr-15544.ic10" size="2097152" crc="39e3df45" sha1="38a7b21617b45613b05509dda388f8f7770b186c" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15546.ic38" merge="mpr-15546.ic38" size="2097152" crc="e3fcc12c" sha1="1cf7e05c7873f68789a27a91cddf471df40d7907" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15541.ic22" merge="mpr-15541.ic22" size="2097152" crc="a2003c2d" sha1="200a2c7d78d3f5f28909267fdcdbddd58c5f5fa2" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15543.ic23" merge="mpr-15543.ic23" size="2097152" crc="933e8e7b" sha1="0d53286f524f47851a483569dc37e9f6d34cc5f4" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15545.ic18" merge="mpr-15545.ic18" size="2097152" crc="53dd0235" sha1="4aee5ae1820ff933b6bd8a54bdbf989c0bc95c1a" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15547.ic41" merge="mpr-15547.ic41" size="2097152" crc="edcb2a43" sha1="f0bcfcc749ca0267f85bf9838164869912944d00" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-15551.ic1" merge="mpr-15551.ic1" size="2097152" crc="4894bc73" sha1="351f5c03fb430fd87df915dfe3a377b5ada622c4" region="mainpcb:sega" offset="0" />
    <rom name="mpr-15552.ic2" merge="mpr-15552.ic2" size="2097152" crc="1c4b5e73" sha1="50a8e9a200575a3522a51bf094aa0e87b90bb0a3" region="mainpcb:sega" offset="200000" />
    <device_ref name="segas32_pcb_multi_analog" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="paddle" player="1" buttons="5" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" player="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="paddle" player="2" buttons="5" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" player="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG7">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG8">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="orunnersu" sourcefile="segas32.cpp" cloneof="orunners" romof="orunners">
    <description>OutRunners (US)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15618.ic37" size="131072" crc="25647f76" sha1="9f882921ebb2f078350295c322b263f75812c053" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15619.ic40" size="131072" crc="2a558f95" sha1="616ec0a7b251da61a49b933c58895b1a4d39417a" region="mainpcb:maincpu" offset="2" />
    <rom name="mpr-15538.ic36" merge="mpr-15538.ic36" size="524288" crc="93958820" sha1="e19b6f18a5707dbb64ae009d63c05eac5bac4a81" region="mainpcb:maincpu" offset="100000" />
    <rom name="mpr-15539.ic39" merge="mpr-15539.ic39" size="524288" crc="219760fa" sha1="bd62a83de9c9542f6da454a87dc4947492f65c52" region="mainpcb:maincpu" offset="100002" />
    <rom name="epr-15550.ic31" merge="epr-15550.ic31" size="524288" crc="0205d2ed" sha1="3475479e1a45fe96eefbe53842758898db7accbf" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15548.ic3" merge="mpr-15548.ic3" size="2097152" crc="b6470a66" sha1="e1544590c02d41f62f82a4d771b893fb0f2734c7" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15549.ic11" merge="mpr-15549.ic11" size="2097152" crc="81d12520" sha1="1555893941e832f00ad3d0b3ad0c34a0d3a1c58a" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15540.ic14" merge="mpr-15540.ic14" size="2097152" crc="a10d72b4" sha1="6d9d5e20be6721b53ce49df4d5a1bbd91f5b3aed" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15542.ic15" merge="mpr-15542.ic15" size="2097152" crc="40952374" sha1="c669ef52508bc2f49cf812dc86ac98fb535471fa" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15544.ic10" merge="mpr-15544.ic10" size="2097152" crc="39e3df45" sha1="38a7b21617b45613b05509dda388f8f7770b186c" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15546.ic38" merge="mpr-15546.ic38" size="2097152" crc="e3fcc12c" sha1="1cf7e05c7873f68789a27a91cddf471df40d7907" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15541.ic22" merge="mpr-15541.ic22" size="2097152" crc="a2003c2d" sha1="200a2c7d78d3f5f28909267fdcdbddd58c5f5fa2" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15543.ic23" merge="mpr-15543.ic23" size="2097152" crc="933e8e7b" sha1="0d53286f524f47851a483569dc37e9f6d34cc5f4" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15545.ic18" merge="mpr-15545.ic18" size="2097152" crc="53dd0235" sha1="4aee5ae1820ff933b6bd8a54bdbf989c0bc95c1a" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15547.ic41" merge="mpr-15547.ic41" size="2097152" crc="edcb2a43" sha1="f0bcfcc749ca0267f85bf9838164869912944d00" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-15551.ic1" merge="mpr-15551.ic1" size="2097152" crc="4894bc73" sha1="351f5c03fb430fd87df915dfe3a377b5ada622c4" region="mainpcb:sega" offset="0" />
    <rom name="mpr-15552.ic2" merge="mpr-15552.ic2" size="2097152" crc="1c4b5e73" sha1="50a8e9a200575a3522a51bf094aa0e87b90bb0a3" region="mainpcb:sega" offset="200000" />
    <device_ref name="segas32_pcb_multi_analog" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="paddle" player="1" buttons="5" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" player="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="paddle" player="2" buttons="5" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" player="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG7">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG8">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="radm" sourcefile="segas32.cpp">
    <description>Rad Mobile (World)</description>
    <year>1990</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-13693.ic21" size="131072" crc="3f09a211" sha1="e0e011d7069745e9bf0395bc1375d0f8b9c46dab" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-13525.ic37" size="524288" crc="62ad83a0" sha1="b537176ebca15d91db04d5d7ab36aa967d41288e" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-13526.ic38" size="524288" crc="59ea372a" sha1="e7a5d59586652c59c23e07e0a99ecc740fb6144d" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-13527.ic9" size="131072" crc="a2e3fbbe" sha1="2787bbef696ab3f2b7855ac991867837d3de54cd" region="mainpcb:soundcpu" offset="0" />
    <rom name="epr-13523.ic14" size="524288" crc="d5563697" sha1="eb3fd3dbfea383ac1bb5d2e1552723994cb4693d" region="mainpcb:soundcpu" offset="100000" />
    <rom name="epr-13699.ic20" size="524288" crc="33fd2913" sha1="60b664559b4989446b1c7d875432e53a36fe27df" region="mainpcb:soundcpu" offset="200000" />
    <rom name="epr-13523.ic22" size="524288" crc="d5563697" sha1="eb3fd3dbfea383ac1bb5d2e1552723994cb4693d" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-13519.ic3" size="524288" crc="bedc9534" sha1="7b3f7a47b6c0ca6707dc3c1167f3564d43adb32f" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-13520.ic7" size="524288" crc="3532e91a" sha1="669c8d27b4b48e1ab9d6d30b0994f5a4e5169118" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-13521.ic12" size="524288" crc="e9bca903" sha1="18a73c830b9755262a1c525e3ad5ae084117b64d" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-13522.ic18" size="524288" crc="25e04648" sha1="617e794e8f7aa2a435bac917b8968699fe88dafb" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-13511.ic1" size="1048576" crc="f8f15b11" sha1="da6c2b8c3a94c4c263583f046823eaea818aff7c" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-13512.ic5" size="1048576" crc="d0be34a6" sha1="b42a63e30f0f7a94de8a825ca93cf8efdb7a7648" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-13513.ic10" size="1048576" crc="feef1982" sha1="bdf906317079a12c48ef4fca5bef0d437e9bf050" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-13514.ic16" size="1048576" crc="d0f9ebd1" sha1="510ebd3d7a52bcab2debea61591770d1dff172a1" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-13515.ic2" size="1048576" crc="77bf2387" sha1="7215dde5618e238edbe16b3007ede790785fe25f" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-13516.ic6" size="1048576" crc="8c4bc62d" sha1="3206f623ec0b7558413d063404103b183f26b488" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-13517.ic11" size="1048576" crc="1d7d84a7" sha1="954cfccfc7250a5bead2eeba42e655d5ac82955f" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-13518.ic17" size="1048576" crc="9ea4b15d" sha1="7dcfd6d42bb945beca8344cf92e7bd53903a824b" region="mainpcb:sprites" offset="7" />
    <rom name="epr-13686.bin" size="32768" crc="317a2857" sha1="e0788dc7a7d214d9c4d26b24e44c1a0dc9ae477c" region="user2" offset="0" />
    <rom name="eeprom-radm.ic76" size="128" crc="b1737c06" sha1="29448a6effeb53322a93158feb9a62bc6ad31f21" region="mainpcb:eeprom" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="1" coins="2" service="yes">
      <control type="paddle" buttons="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="radmu" sourcefile="segas32.cpp" cloneof="radm" romof="radm">
    <description>Rad Mobile (US)</description>
    <year>1990</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-13690.ic21" size="131072" crc="21637dec" sha1="b9921effb10a72f3bdca4d540149c7f46662b716" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-13525.ic37" merge="epr-13525.ic37" size="524288" crc="62ad83a0" sha1="b537176ebca15d91db04d5d7ab36aa967d41288e" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-13526.ic38" merge="epr-13526.ic38" size="524288" crc="59ea372a" sha1="e7a5d59586652c59c23e07e0a99ecc740fb6144d" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-13527.ic9" merge="epr-13527.ic9" size="131072" crc="a2e3fbbe" sha1="2787bbef696ab3f2b7855ac991867837d3de54cd" region="mainpcb:soundcpu" offset="0" />
    <rom name="epr-13523.ic14" merge="epr-13523.ic14" size="524288" crc="d5563697" sha1="eb3fd3dbfea383ac1bb5d2e1552723994cb4693d" region="mainpcb:soundcpu" offset="100000" />
    <rom name="epr-13699.ic20" merge="epr-13699.ic20" size="524288" crc="33fd2913" sha1="60b664559b4989446b1c7d875432e53a36fe27df" region="mainpcb:soundcpu" offset="200000" />
    <rom name="epr-13523.ic22" merge="epr-13523.ic14" size="524288" crc="d5563697" sha1="eb3fd3dbfea383ac1bb5d2e1552723994cb4693d" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-13519.ic3" merge="mpr-13519.ic3" size="524288" crc="bedc9534" sha1="7b3f7a47b6c0ca6707dc3c1167f3564d43adb32f" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-13520.ic7" merge="mpr-13520.ic7" size="524288" crc="3532e91a" sha1="669c8d27b4b48e1ab9d6d30b0994f5a4e5169118" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-13521.ic12" merge="mpr-13521.ic12" size="524288" crc="e9bca903" sha1="18a73c830b9755262a1c525e3ad5ae084117b64d" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-13522.ic18" merge="mpr-13522.ic18" size="524288" crc="25e04648" sha1="617e794e8f7aa2a435bac917b8968699fe88dafb" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-13511.ic1" merge="mpr-13511.ic1" size="1048576" crc="f8f15b11" sha1="da6c2b8c3a94c4c263583f046823eaea818aff7c" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-13512.ic5" merge="mpr-13512.ic5" size="1048576" crc="d0be34a6" sha1="b42a63e30f0f7a94de8a825ca93cf8efdb7a7648" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-13513.ic10" merge="mpr-13513.ic10" size="1048576" crc="feef1982" sha1="bdf906317079a12c48ef4fca5bef0d437e9bf050" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-13514.ic16" merge="mpr-13514.ic16" size="1048576" crc="d0f9ebd1" sha1="510ebd3d7a52bcab2debea61591770d1dff172a1" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-13515.ic2" merge="mpr-13515.ic2" size="1048576" crc="77bf2387" sha1="7215dde5618e238edbe16b3007ede790785fe25f" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-13516.ic6" merge="mpr-13516.ic6" size="1048576" crc="8c4bc62d" sha1="3206f623ec0b7558413d063404103b183f26b488" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-13517.ic11" merge="mpr-13517.ic11" size="1048576" crc="1d7d84a7" sha1="954cfccfc7250a5bead2eeba42e655d5ac82955f" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-13518.ic17" merge="mpr-13518.ic17" size="1048576" crc="9ea4b15d" sha1="7dcfd6d42bb945beca8344cf92e7bd53903a824b" region="mainpcb:sprites" offset="7" />
    <rom name="epr-13686.bin" merge="epr-13686.bin" size="32768" crc="317a2857" sha1="e0788dc7a7d214d9c4d26b24e44c1a0dc9ae477c" region="user2" offset="0" />
    <rom name="eeprom-radm.ic76" merge="eeprom-radm.ic76" size="128" crc="b1737c06" sha1="29448a6effeb53322a93158feb9a62bc6ad31f21" region="mainpcb:eeprom" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="1" coins="2" service="yes">
      <control type="paddle" buttons="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="radr" sourcefile="segas32.cpp">
    <description>Rad Rally (World)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14241.ic21" size="131072" crc="59a5f63d" sha1="325a26a09475ddc828de71e71a1d3043f3959cec" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14106.ic37" size="524288" crc="e73c63bf" sha1="30fb68eaa7d02a232c873bd7751cac7d0fa08e44" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14107.ic38" size="524288" crc="832f797a" sha1="b0c16ef7bd8d37f592975052ba9da3da70a2fc79" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14108.ic9" size="131072" crc="38a99b4d" sha1="b6455e6b29bfef41c5e0ebe3a8064889b7e5f5fd" region="mainpcb:soundcpu" offset="0" />
    <rom name="epr-14109.ic14" size="524288" crc="d5563697" sha1="eb3fd3dbfea383ac1bb5d2e1552723994cb4693d" region="mainpcb:soundcpu" offset="100000" />
    <rom name="epr-14110.ic20" size="524288" crc="33fd2913" sha1="60b664559b4989446b1c7d875432e53a36fe27df" region="mainpcb:soundcpu" offset="200000" />
    <rom name="epr-14237.ic22" size="524288" crc="0a4b4b29" sha1="98447a587f903ba03e17d6a145b7c8bfddf25c4d" region="mainpcb:soundcpu" offset="300000" />
    <rom name="epr-14102.ic3" size="262144" crc="5626e80f" sha1="9844817295a8cd8a9b09da6681b0c1fbfe82618e" region="mainpcb:gfx1" offset="0" />
    <rom name="epr-14103.ic7" size="262144" crc="08c7e804" sha1="cf45b1934edc43cb3a0ed72159949cb0dd00d701" region="mainpcb:gfx1" offset="2" />
    <rom name="epr-14104.ic12" size="262144" crc="b0173646" sha1="1ba4edc033e0e4f5a1e02987e9f6b8b1650b46d7" region="mainpcb:gfx1" offset="1" />
    <rom name="epr-14105.ic18" size="262144" crc="614843b6" sha1="d4f2cd3b024f7152d6e89237f0da06adea2efe57" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-13511.ic1" size="1048576" crc="f8f15b11" sha1="da6c2b8c3a94c4c263583f046823eaea818aff7c" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-13512.ic5" size="1048576" crc="d0be34a6" sha1="b42a63e30f0f7a94de8a825ca93cf8efdb7a7648" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-13513.ic10" size="1048576" crc="feef1982" sha1="bdf906317079a12c48ef4fca5bef0d437e9bf050" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-13514.ic16" size="1048576" crc="d0f9ebd1" sha1="510ebd3d7a52bcab2debea61591770d1dff172a1" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-13515.ic2" size="1048576" crc="77bf2387" sha1="7215dde5618e238edbe16b3007ede790785fe25f" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-13516.ic6" size="1048576" crc="8c4bc62d" sha1="3206f623ec0b7558413d063404103b183f26b488" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-13517.ic11" size="1048576" crc="1d7d84a7" sha1="954cfccfc7250a5bead2eeba42e655d5ac82955f" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-13518.ic17" size="1048576" crc="9ea4b15d" sha1="7dcfd6d42bb945beca8344cf92e7bd53903a824b" region="mainpcb:sprites" offset="7" />
    <rom name="epr-14084.17" size="32768" crc="f14ed074" sha1="e1bb23eac85e3236046527c5c7688f6f23d43aef" region="user2" offset="0" />
    <rom name="eeprom-radr.ic76" size="128" crc="602032c6" sha1="fecf14017e537fe870457d2a8d4f86ec6d442b90" region="mainpcb:eeprom" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="1" coins="2" service="yes">
      <control type="paddle" buttons="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Transmission" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Manual" value="8" default="yes" />
      <dipvalue name="Automatic" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="radrj" sourcefile="segas32.cpp" cloneof="radr" romof="radr">
    <description>Rad Rally (Japan)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14111.ic21" size="131072" crc="7adc6d17" sha1="fc312a30b077ba060b6d98ab6ecccd2e16b32fc2" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14106.ic37" merge="epr-14106.ic37" size="524288" crc="e73c63bf" sha1="30fb68eaa7d02a232c873bd7751cac7d0fa08e44" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14107.ic38" merge="epr-14107.ic38" size="524288" crc="832f797a" sha1="b0c16ef7bd8d37f592975052ba9da3da70a2fc79" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14108.ic9" merge="epr-14108.ic9" size="131072" crc="38a99b4d" sha1="b6455e6b29bfef41c5e0ebe3a8064889b7e5f5fd" region="mainpcb:soundcpu" offset="0" />
    <rom name="epr-14109.ic14" merge="epr-14109.ic14" size="524288" crc="d5563697" sha1="eb3fd3dbfea383ac1bb5d2e1552723994cb4693d" region="mainpcb:soundcpu" offset="100000" />
    <rom name="epr-14110.ic20" merge="epr-14110.ic20" size="524288" crc="33fd2913" sha1="60b664559b4989446b1c7d875432e53a36fe27df" region="mainpcb:soundcpu" offset="200000" />
    <rom name="epr-14237.ic22" merge="epr-14237.ic22" size="524288" crc="0a4b4b29" sha1="98447a587f903ba03e17d6a145b7c8bfddf25c4d" region="mainpcb:soundcpu" offset="300000" />
    <rom name="epr-14102.ic3" merge="epr-14102.ic3" size="262144" crc="5626e80f" sha1="9844817295a8cd8a9b09da6681b0c1fbfe82618e" region="mainpcb:gfx1" offset="0" />
    <rom name="epr-14103.ic7" merge="epr-14103.ic7" size="262144" crc="08c7e804" sha1="cf45b1934edc43cb3a0ed72159949cb0dd00d701" region="mainpcb:gfx1" offset="2" />
    <rom name="epr-14104.ic12" merge="epr-14104.ic12" size="262144" crc="b0173646" sha1="1ba4edc033e0e4f5a1e02987e9f6b8b1650b46d7" region="mainpcb:gfx1" offset="1" />
    <rom name="epr-14105.ic16" merge="epr-14105.ic18" size="262144" crc="614843b6" sha1="d4f2cd3b024f7152d6e89237f0da06adea2efe57" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-13511.ic1" merge="mpr-13511.ic1" size="1048576" crc="f8f15b11" sha1="da6c2b8c3a94c4c263583f046823eaea818aff7c" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-13512.ic5" merge="mpr-13512.ic5" size="1048576" crc="d0be34a6" sha1="b42a63e30f0f7a94de8a825ca93cf8efdb7a7648" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-13513.ic10" merge="mpr-13513.ic10" size="1048576" crc="feef1982" sha1="bdf906317079a12c48ef4fca5bef0d437e9bf050" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-13514.ic16" merge="mpr-13514.ic16" size="1048576" crc="d0f9ebd1" sha1="510ebd3d7a52bcab2debea61591770d1dff172a1" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-13515.ic2" merge="mpr-13515.ic2" size="1048576" crc="77bf2387" sha1="7215dde5618e238edbe16b3007ede790785fe25f" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-13516.ic6" merge="mpr-13516.ic6" size="1048576" crc="8c4bc62d" sha1="3206f623ec0b7558413d063404103b183f26b488" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-13517.ic11" merge="mpr-13517.ic11" size="1048576" crc="1d7d84a7" sha1="954cfccfc7250a5bead2eeba42e655d5ac82955f" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-13518.ic17" merge="mpr-13518.ic17" size="1048576" crc="9ea4b15d" sha1="7dcfd6d42bb945beca8344cf92e7bd53903a824b" region="mainpcb:sprites" offset="7" />
    <rom name="epr-14084.17" merge="epr-14084.17" size="32768" crc="f14ed074" sha1="e1bb23eac85e3236046527c5c7688f6f23d43aef" region="user2" offset="0" />
    <rom name="eeprom-radr.ic76" merge="eeprom-radr.ic76" size="128" crc="602032c6" sha1="fecf14017e537fe870457d2a8d4f86ec6d442b90" region="mainpcb:eeprom" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="1" coins="2" service="yes">
      <control type="paddle" buttons="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Transmission" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Manual" value="8" default="yes" />
      <dipvalue name="Automatic" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="radru" sourcefile="segas32.cpp" cloneof="radr" romof="radr">
    <description>Rad Rally (US)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14240.ic21" size="131072" crc="8473e7ab" sha1="fbd883dc804d7de6ce239b68c6e6ae3a54e9e03c" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14106.ic37" merge="epr-14106.ic37" size="524288" crc="e73c63bf" sha1="30fb68eaa7d02a232c873bd7751cac7d0fa08e44" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14107.ic38" merge="epr-14107.ic38" size="524288" crc="832f797a" sha1="b0c16ef7bd8d37f592975052ba9da3da70a2fc79" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14108.ic9" merge="epr-14108.ic9" size="131072" crc="38a99b4d" sha1="b6455e6b29bfef41c5e0ebe3a8064889b7e5f5fd" region="mainpcb:soundcpu" offset="0" />
    <rom name="epr-14109.ic14" merge="epr-14109.ic14" size="524288" crc="d5563697" sha1="eb3fd3dbfea383ac1bb5d2e1552723994cb4693d" region="mainpcb:soundcpu" offset="100000" />
    <rom name="epr-14110.ic20" merge="epr-14110.ic20" size="524288" crc="33fd2913" sha1="60b664559b4989446b1c7d875432e53a36fe27df" region="mainpcb:soundcpu" offset="200000" />
    <rom name="epr-14237.ic22" merge="epr-14237.ic22" size="524288" crc="0a4b4b29" sha1="98447a587f903ba03e17d6a145b7c8bfddf25c4d" region="mainpcb:soundcpu" offset="300000" />
    <rom name="epr-14102.ic3" merge="epr-14102.ic3" size="262144" crc="5626e80f" sha1="9844817295a8cd8a9b09da6681b0c1fbfe82618e" region="mainpcb:gfx1" offset="0" />
    <rom name="epr-14103.ic7" merge="epr-14103.ic7" size="262144" crc="08c7e804" sha1="cf45b1934edc43cb3a0ed72159949cb0dd00d701" region="mainpcb:gfx1" offset="2" />
    <rom name="epr-14104.ic12" merge="epr-14104.ic12" size="262144" crc="b0173646" sha1="1ba4edc033e0e4f5a1e02987e9f6b8b1650b46d7" region="mainpcb:gfx1" offset="1" />
    <rom name="epr-14105.ic16" merge="epr-14105.ic18" size="262144" crc="614843b6" sha1="d4f2cd3b024f7152d6e89237f0da06adea2efe57" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-13511.ic1" merge="mpr-13511.ic1" size="1048576" crc="f8f15b11" sha1="da6c2b8c3a94c4c263583f046823eaea818aff7c" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-13512.ic5" merge="mpr-13512.ic5" size="1048576" crc="d0be34a6" sha1="b42a63e30f0f7a94de8a825ca93cf8efdb7a7648" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-13513.ic10" merge="mpr-13513.ic10" size="1048576" crc="feef1982" sha1="bdf906317079a12c48ef4fca5bef0d437e9bf050" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-13514.ic16" merge="mpr-13514.ic16" size="1048576" crc="d0f9ebd1" sha1="510ebd3d7a52bcab2debea61591770d1dff172a1" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-13515.ic2" merge="mpr-13515.ic2" size="1048576" crc="77bf2387" sha1="7215dde5618e238edbe16b3007ede790785fe25f" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-13516.ic6" merge="mpr-13516.ic6" size="1048576" crc="8c4bc62d" sha1="3206f623ec0b7558413d063404103b183f26b488" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-13517.ic11" merge="mpr-13517.ic11" size="1048576" crc="1d7d84a7" sha1="954cfccfc7250a5bead2eeba42e655d5ac82955f" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-13518.ic17" merge="mpr-13518.ic17" size="1048576" crc="9ea4b15d" sha1="7dcfd6d42bb945beca8344cf92e7bd53903a824b" region="mainpcb:sprites" offset="7" />
    <rom name="epr-14084.17" merge="epr-14084.17" size="32768" crc="f14ed074" sha1="e1bb23eac85e3236046527c5c7688f6f23d43aef" region="user2" offset="0" />
    <rom name="eeprom-radr.ic76" merge="eeprom-radr.ic76" size="128" crc="602032c6" sha1="fecf14017e537fe870457d2a8d4f86ec6d442b90" region="mainpcb:eeprom" offset="0" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="1" coins="2" service="yes">
      <control type="paddle" buttons="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Transmission" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Manual" value="8" default="yes" />
      <dipvalue name="Automatic" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="scross" sourcefile="segas32.cpp">
    <description>Stadium Cross (World)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15093.ic37" size="262144" crc="2adc7a4b" sha1="dca71f00d94898c0758394704d819e13482bf120" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15094.ic40" size="262144" crc="bbb0ae73" sha1="0d8837706405f301adf8fa85c8d4813d7600af98" region="mainpcb:maincpu" offset="2" />
    <rom name="mpr-15018.ic36" size="524288" crc="3a98385e" sha1="8088d337655030c28e290da4bbf44cb647dab66c" region="mainpcb:maincpu" offset="100000" />
    <rom name="mpr-15019.ic39" size="524288" crc="8bf4ac83" sha1="e594d9d9b42d0765ed8a20a40b7dd92b75124d34" region="mainpcb:maincpu" offset="100002" />
    <rom name="epr-15192.ic31" size="131072" crc="7524290b" sha1="ee58be2c0c4293ee19622b96ca493f4ce4da0038" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15020.ic3" size="1048576" crc="de47006a" sha1="dbef7b9ff8c39992b8596d38985e65c627d6fa79" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15021.ic11" size="1048576" crc="3677db02" sha1="7aeeb85f1632253fcdc8f7881512066e97837e5e" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15022.ic14" size="1048576" crc="baee6fd5" sha1="ddf022c61f0805af45a84c65eb5d01006c153c07" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15024.ic15" size="1048576" crc="b9f339e2" sha1="4b9a392459132a19d62928ef3939e1f2356e3994" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15026.ic10" size="1048576" crc="b72e8df6" sha1="a7a87f79814b022985121e163c7f88244c50e427" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15028.ic38" size="1048576" crc="183f6eb0" sha1="5a2172d5afd696af361ff9f8a92f5911e05c578d" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15023.ic22" size="1048576" crc="230735ed" sha1="36075504e27b8a32d63fa3b8abd7037d17440ebf" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15025.ic23" size="1048576" crc="da4315cb" sha1="3910c5654e34b17851d6d93615e3404b3b397fea" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15027.ic18" size="1048576" crc="b765efb8" sha1="61f3865f92b36ca4b3cd20c0716a7121755eea73" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15029.ic41" size="1048576" crc="cf8e3b2b" sha1="c158810d9d82b10a753bc739d1f56572042dac0b" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-15031.ic1" size="1048576" crc="6af139dc" sha1="2378c2ad0c52c114eb93206a6fbee723c038d030" region="mainpcb:sega" offset="0" />
    <rom name="mpr-15032.ic2" size="1048576" crc="915d6096" sha1="e1f670949b1254f5a3c3131993ca9b3baa4d9f6b" region="mainpcb:sega" offset="200000" />
    <rom name="epr-15033.ic17" size="131072" crc="dc19ac00" sha1="16bbb5af034e5419673e637be30283b73ab7b290" region="user2" offset="0" />
    <device_ref name="segas32_pcb_multi_analog" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="paddle" player="1" buttons="3" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
      <control type="pedal" player="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="joy" player="2" buttons="3" ways="8" />
      <control type="paddle" player="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
      <control type="pedal" player="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="scrossa" sourcefile="segas32.cpp" cloneof="scross" romof="scross">
    <description>Stadium Cross (World, alt)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="ic37" size="262144" crc="240a7655" sha1="7cfdce002fb4783e8c1debf206922d88647c106e" region="mainpcb:maincpu" offset="0" />
    <rom name="ic40" size="262144" crc="3a073060" sha1="c92c8d8921d94d85c8484c103cbf9cd6ad651333" region="mainpcb:maincpu" offset="2" />
    <rom name="mpr-15018.ic36" merge="mpr-15018.ic36" size="524288" crc="3a98385e" sha1="8088d337655030c28e290da4bbf44cb647dab66c" region="mainpcb:maincpu" offset="100000" />
    <rom name="mpr-15019.ic39" merge="mpr-15019.ic39" size="524288" crc="8bf4ac83" sha1="e594d9d9b42d0765ed8a20a40b7dd92b75124d34" region="mainpcb:maincpu" offset="100002" />
    <rom name="epr-15192.ic31" merge="epr-15192.ic31" size="131072" crc="7524290b" sha1="ee58be2c0c4293ee19622b96ca493f4ce4da0038" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15020.ic3" merge="mpr-15020.ic3" size="1048576" crc="de47006a" sha1="dbef7b9ff8c39992b8596d38985e65c627d6fa79" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15021.ic11" merge="mpr-15021.ic11" size="1048576" crc="3677db02" sha1="7aeeb85f1632253fcdc8f7881512066e97837e5e" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15022.ic14" merge="mpr-15022.ic14" size="1048576" crc="baee6fd5" sha1="ddf022c61f0805af45a84c65eb5d01006c153c07" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15024.ic15" merge="mpr-15024.ic15" size="1048576" crc="b9f339e2" sha1="4b9a392459132a19d62928ef3939e1f2356e3994" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15026.ic10" merge="mpr-15026.ic10" size="1048576" crc="b72e8df6" sha1="a7a87f79814b022985121e163c7f88244c50e427" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15028.ic38" merge="mpr-15028.ic38" size="1048576" crc="183f6eb0" sha1="5a2172d5afd696af361ff9f8a92f5911e05c578d" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15023.ic22" merge="mpr-15023.ic22" size="1048576" crc="230735ed" sha1="36075504e27b8a32d63fa3b8abd7037d17440ebf" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15025.ic23" merge="mpr-15025.ic23" size="1048576" crc="da4315cb" sha1="3910c5654e34b17851d6d93615e3404b3b397fea" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15027.ic18" merge="mpr-15027.ic18" size="1048576" crc="b765efb8" sha1="61f3865f92b36ca4b3cd20c0716a7121755eea73" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15029.ic41" merge="mpr-15029.ic41" size="1048576" crc="cf8e3b2b" sha1="c158810d9d82b10a753bc739d1f56572042dac0b" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-15031.ic1" merge="mpr-15031.ic1" size="1048576" crc="6af139dc" sha1="2378c2ad0c52c114eb93206a6fbee723c038d030" region="mainpcb:sega" offset="0" />
    <rom name="mpr-15032.ic2" merge="mpr-15032.ic2" size="1048576" crc="915d6096" sha1="e1f670949b1254f5a3c3131993ca9b3baa4d9f6b" region="mainpcb:sega" offset="200000" />
    <rom name="epr-15033.ic17" merge="epr-15033.ic17" size="131072" crc="dc19ac00" sha1="16bbb5af034e5419673e637be30283b73ab7b290" region="user2" offset="0" />
    <device_ref name="segas32_pcb_multi_analog" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="paddle" player="1" buttons="3" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
      <control type="pedal" player="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="joy" player="2" buttons="3" ways="8" />
      <control type="paddle" player="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
      <control type="pedal" player="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="scrossu" sourcefile="segas32.cpp" cloneof="scross" romof="scross">
    <description>Stadium Cross (US)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15091.ic37" size="262144" crc="2c572293" sha1="6377a6eb6084f7332ce6eeaaf0c37200da792d0c" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15092.ic40" size="262144" crc="6e3e175a" sha1="feaca0720646e2a4b78b376e99dc86788adb98e7" region="mainpcb:maincpu" offset="2" />
    <rom name="epr-15018.ic36" merge="mpr-15018.ic36" size="524288" crc="3a98385e" sha1="8088d337655030c28e290da4bbf44cb647dab66c" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15019.ic39" merge="mpr-15019.ic39" size="524288" crc="8bf4ac83" sha1="e594d9d9b42d0765ed8a20a40b7dd92b75124d34" region="mainpcb:maincpu" offset="100002" />
    <rom name="epr-15192.ic31" merge="epr-15192.ic31" size="131072" crc="7524290b" sha1="ee58be2c0c4293ee19622b96ca493f4ce4da0038" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15020.ic3" merge="mpr-15020.ic3" size="1048576" crc="de47006a" sha1="dbef7b9ff8c39992b8596d38985e65c627d6fa79" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15021.ic11" merge="mpr-15021.ic11" size="1048576" crc="3677db02" sha1="7aeeb85f1632253fcdc8f7881512066e97837e5e" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15022.ic14" merge="mpr-15022.ic14" size="1048576" crc="baee6fd5" sha1="ddf022c61f0805af45a84c65eb5d01006c153c07" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15024.ic15" merge="mpr-15024.ic15" size="1048576" crc="b9f339e2" sha1="4b9a392459132a19d62928ef3939e1f2356e3994" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15026.ic10" merge="mpr-15026.ic10" size="1048576" crc="b72e8df6" sha1="a7a87f79814b022985121e163c7f88244c50e427" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15028.ic38" merge="mpr-15028.ic38" size="1048576" crc="183f6eb0" sha1="5a2172d5afd696af361ff9f8a92f5911e05c578d" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15023.ic22" merge="mpr-15023.ic22" size="1048576" crc="230735ed" sha1="36075504e27b8a32d63fa3b8abd7037d17440ebf" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15025.ic23" merge="mpr-15025.ic23" size="1048576" crc="da4315cb" sha1="3910c5654e34b17851d6d93615e3404b3b397fea" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15027.ic18" merge="mpr-15027.ic18" size="1048576" crc="b765efb8" sha1="61f3865f92b36ca4b3cd20c0716a7121755eea73" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15029.ic41" merge="mpr-15029.ic41" size="1048576" crc="cf8e3b2b" sha1="c158810d9d82b10a753bc739d1f56572042dac0b" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-15031.ic1" merge="mpr-15031.ic1" size="1048576" crc="6af139dc" sha1="2378c2ad0c52c114eb93206a6fbee723c038d030" region="mainpcb:sega" offset="0" />
    <rom name="mpr-15032.ic2" merge="mpr-15032.ic2" size="1048576" crc="915d6096" sha1="e1f670949b1254f5a3c3131993ca9b3baa4d9f6b" region="mainpcb:sega" offset="200000" />
    <device_ref name="segas32_pcb_multi_analog" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="paddle" player="1" buttons="3" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
      <control type="pedal" player="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="joy" player="2" buttons="3" ways="8" />
      <control type="paddle" player="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" reverse="yes" />
      <control type="pedal" player="2" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG4">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="slipstrm" sourcefile="segas32.cpp">
    <description>Slip Stream (Brazil 950515)</description>
    <year>1995</year>
    <manufacturer>Capcom</manufacturer>
    <rom name="s32b_prg01.ic6" size="524288" crc="7d066307" sha1="d87e04167263b435b77830db02ed58651ccc020c" region="mainpcb:maincpu" offset="0" />
    <rom name="s32_dat00.ic14" size="524288" crc="c3ff6309" sha1="dcc857736fe0f15aa7909c3ee88a7e239c8f0228" region="mainpcb:maincpu" offset="100000" />
    <rom name="s32_dat01.ic7" size="524288" crc="0e605c81" sha1="47c64195cab9a07b234d5a375d26168e53ffaa17" region="mainpcb:maincpu" offset="100001" />
    <rom name="s32_snd00.ic35" size="131072" crc="0fee2278" sha1="7533a03c3fc46d65dfdd07bddf1e6e0bbc368752" region="mainpcb:soundcpu" offset="0" />
    <rom name="s32_snd01.ic31" size="524288" crc="ae7be5f2" sha1="ba089355e64864435bcc3b0c208e4bce1ea66295" region="mainpcb:soundcpu" offset="100000" />
    <rom name="s32_scr00.ic38" size="524288" crc="3cbb2d0b" sha1="b94006347b72cd60a889b0e279f62f677cedfd2e" region="mainpcb:gfx1" offset="0" />
    <rom name="s32_scr01.ic34" size="524288" crc="4167be55" sha1="96b34d311b318c00c3fad917e341589a70ba0a15" region="mainpcb:gfx1" offset="2" />
    <rom name="s32_scr02.ic29" size="524288" crc="52c4bb85" sha1="4fbee1072a19c75c25b5fd269acc75640923d69c" region="mainpcb:gfx1" offset="1" />
    <rom name="s32_scr03.ic25" size="524288" crc="4948604a" sha1="d5a1b9781fef7976a59a0af9b755a04fcacf9381" region="mainpcb:gfx1" offset="3" />
    <rom name="s32_obj00.ic36" size="524288" crc="cffe9e0d" sha1="5272d54ff142de927a9abd61f3646e963c7d22c4" region="mainpcb:sprites" offset="0" />
    <rom name="s32_obj01.ic32" size="524288" crc="4ebd1383" sha1="ce35f4d15e7904bfde55e58cdde925cba8002763" region="mainpcb:sprites" offset="1" />
    <rom name="s32_obj02.ic27" size="524288" crc="b3cf4fe2" sha1="e13199522e1e3e8b9cfe72cc29b33f25dad542ef" region="mainpcb:sprites" offset="2" />
    <rom name="s32_obj03.ic23" size="524288" crc="c6345391" sha1="155758097911ffca0c5c0b2a24a8033339dcfcbb" region="mainpcb:sprites" offset="3" />
    <rom name="s32_obj04.ic37" size="524288" crc="2de4288e" sha1="8e794f79f506293edb7609187a7908516ce76849" region="mainpcb:sprites" offset="4" />
    <rom name="s32_obj05.ic33" size="524288" crc="6cfb74fb" sha1="b74c886959910cd069427418525b23300a9b7b18" region="mainpcb:sprites" offset="5" />
    <rom name="s32_obj06.ic28" size="524288" crc="53234bf4" sha1="1eca538dcb86e44c31310ab1ab42a2b66b69c8fe" region="mainpcb:sprites" offset="6" />
    <rom name="s32_obj07.ic24" size="524288" crc="22c129cf" sha1="0f64680511a357038f6a556253c13fbb5417dd1a" region="mainpcb:sprites" offset="7" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="1" coins="2" service="yes">
      <control type="paddle" buttons="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="slipstrmh" sourcefile="segas32.cpp" cloneof="slipstrm" romof="slipstrm">
    <description>Slip Stream (Hispanic 950515)</description>
    <year>1995</year>
    <manufacturer>Capcom</manufacturer>
    <rom name="s32h_prg01.ic6" size="524288" crc="ab778297" sha1="e440d44b20f2f7478ef7d86af90af5eb7b9a545a" region="mainpcb:maincpu" offset="0" />
    <rom name="s32_dat00.ic14" merge="s32_dat00.ic14" size="524288" crc="c3ff6309" sha1="dcc857736fe0f15aa7909c3ee88a7e239c8f0228" region="mainpcb:maincpu" offset="100000" />
    <rom name="s32_dat01.ic7" merge="s32_dat01.ic7" size="524288" crc="0e605c81" sha1="47c64195cab9a07b234d5a375d26168e53ffaa17" region="mainpcb:maincpu" offset="100001" />
    <rom name="s32_snd00.ic35" merge="s32_snd00.ic35" size="131072" crc="0fee2278" sha1="7533a03c3fc46d65dfdd07bddf1e6e0bbc368752" region="mainpcb:soundcpu" offset="0" />
    <rom name="s32_snd01.ic31" merge="s32_snd01.ic31" size="524288" crc="ae7be5f2" sha1="ba089355e64864435bcc3b0c208e4bce1ea66295" region="mainpcb:soundcpu" offset="100000" />
    <rom name="s32_scr00.ic38" merge="s32_scr00.ic38" size="524288" crc="3cbb2d0b" sha1="b94006347b72cd60a889b0e279f62f677cedfd2e" region="mainpcb:gfx1" offset="0" />
    <rom name="s32_scr01.ic34" merge="s32_scr01.ic34" size="524288" crc="4167be55" sha1="96b34d311b318c00c3fad917e341589a70ba0a15" region="mainpcb:gfx1" offset="2" />
    <rom name="s32_scr02.ic29" merge="s32_scr02.ic29" size="524288" crc="52c4bb85" sha1="4fbee1072a19c75c25b5fd269acc75640923d69c" region="mainpcb:gfx1" offset="1" />
    <rom name="s32_scr03.ic25" merge="s32_scr03.ic25" size="524288" crc="4948604a" sha1="d5a1b9781fef7976a59a0af9b755a04fcacf9381" region="mainpcb:gfx1" offset="3" />
    <rom name="s32_obj00.ic36" merge="s32_obj00.ic36" size="524288" crc="cffe9e0d" sha1="5272d54ff142de927a9abd61f3646e963c7d22c4" region="mainpcb:sprites" offset="0" />
    <rom name="s32_obj01.ic32" merge="s32_obj01.ic32" size="524288" crc="4ebd1383" sha1="ce35f4d15e7904bfde55e58cdde925cba8002763" region="mainpcb:sprites" offset="1" />
    <rom name="s32_obj02.ic27" merge="s32_obj02.ic27" size="524288" crc="b3cf4fe2" sha1="e13199522e1e3e8b9cfe72cc29b33f25dad542ef" region="mainpcb:sprites" offset="2" />
    <rom name="s32_obj03.ic23" merge="s32_obj03.ic23" size="524288" crc="c6345391" sha1="155758097911ffca0c5c0b2a24a8033339dcfcbb" region="mainpcb:sprites" offset="3" />
    <rom name="s32_obj04.ic37" merge="s32_obj04.ic37" size="524288" crc="2de4288e" sha1="8e794f79f506293edb7609187a7908516ce76849" region="mainpcb:sprites" offset="4" />
    <rom name="s32_obj05.ic33" merge="s32_obj05.ic33" size="524288" crc="6cfb74fb" sha1="b74c886959910cd069427418525b23300a9b7b18" region="mainpcb:sprites" offset="5" />
    <rom name="s32_obj06.ic28" merge="s32_obj06.ic28" size="524288" crc="53234bf4" sha1="1eca538dcb86e44c31310ab1ab42a2b66b69c8fe" region="mainpcb:sprites" offset="6" />
    <rom name="s32_obj07.ic24" merge="s32_obj07.ic24" size="524288" crc="22c129cf" sha1="0f64680511a357038f6a556253c13fbb5417dd1a" region="mainpcb:sprites" offset="7" />
    <device_ref name="segas32_pcb_analog" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="msm6253" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="1" coins="2" service="yes">
      <control type="paddle" buttons="1" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
      <control type="pedal" minimum="0" maximum="255" sensitivity="30" keydelta="10" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:ANALOG1">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG2">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:ANALOG3">
      <analog mask="255" />
    </port>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="sonic" sourcefile="segas32.cpp">
    <description>SegaSonic The Hedgehog (Japan, rev. C)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15787c.ic17" size="131072" crc="25e3c27e" sha1="8f173cd5c7c817dcccdcad9be5781cfaa081d73e" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15786c.ic8" size="131072" crc="efe9524c" sha1="8020e734704a8f989919ee5ad92f70035de717f0" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-15781c.ic18" size="262144" crc="65b06c25" sha1="9f524012a7adbc71737f90fc556f0ce9adc2bcf8" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-15780c.ic9" size="262144" crc="2db66fd2" sha1="54582c0d5977649a38fc3a2c0fe4d7b1959abc76" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-15785.ic36" size="262144" crc="0fe7422e" sha1="b7eaf4736ba155965317bb4ef3b33fc122635151" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15784.ic35" size="1048576" crc="42f06714" sha1="30e45bb2d9b492f0c1acc4fbe1e5869f0559300b" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-15783.ic34" size="1048576" crc="e4220eea" sha1="a546c8bfc24e0695cf79c49e1a867d2595a1ed7f" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-15782.ic33" size="1048576" crc="cf56b5a0" sha1="5786228aab120c3361524ba93b418b24fd5b8ffb" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-15789.ic14" size="1048576" crc="4378f12b" sha1="826e0550a3c5f2b6e59c6531ac03658a4f826651" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15788.ic5" size="1048576" crc="a6ed5d7a" sha1="d30f26b452d380e7657e044e144f7dbbc4dc13e5" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15790.ic32" size="2097152" crc="c69d51b1" sha1="7644fb64457855f9ed87ca25ddc28c21bcb61fd9" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15792.ic30" size="2097152" crc="1006bb67" sha1="38c752e634aa94b1a23c09c4dba6388b7d0358af" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15794.ic28" size="2097152" crc="8672b480" sha1="61659e3856cdff0b2bca190a7e60c81b86ea2089" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15796.ic26" size="2097152" crc="95b8011c" sha1="ebc56ae49a76d04de60b0f81506769219a9885a7" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15791.ic31" size="1048576" crc="42217066" sha1="46d14c632da1bed02bc0a637e34ab9cbf356c5de" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15793.ic29" size="1048576" crc="75bafe55" sha1="ad33dae062c4bdf8d17d3f6f7c333aa2e7da260e" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15795.ic27" size="1048576" crc="7f3dad30" sha1="84be1c31df35e1c7fef77e83d6d135378789a1ef" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15797.ic25" size="1048576" crc="013c6cab" sha1="eb9b77d28815d2e225b0882706084a52b11c48ea" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_trackball" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="upd4701a" />
    <device_ref name="upd4701a" />
    <device_ref name="upd4701a" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="3" coins="3" service="yes">
      <control type="trackball" player="1" buttons="1" minimum="0" maximum="4095" sensitivity="100" keydelta="30" reverse="yes" />
      <control type="trackball" player="2" buttons="1" minimum="0" maximum="4095" sensitivity="100" keydelta="30" reverse="yes" />
      <control type="trackball" player="3" buttons="1" minimum="0" maximum="4095" sensitivity="100" keydelta="30" reverse="yes" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:TRACKX1">
      <analog mask="4095" />
    </port>
    <port tag=":mainpcb:TRACKX2">
      <analog mask="4095" />
    </port>
    <port tag=":mainpcb:TRACKX3">
      <analog mask="4095" />
    </port>
    <port tag=":mainpcb:TRACKY1">
      <analog mask="4095" />
    </port>
    <port tag=":mainpcb:TRACKY2">
      <analog mask="4095" />
    </port>
    <port tag=":mainpcb:TRACKY3">
      <analog mask="4095" />
    </port>
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="sonicp" sourcefile="segas32.cpp" cloneof="sonic" romof="sonic">
    <description>SegaSonic The Hedgehog (Japan, prototype)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="sonpg0.bin" size="131072" crc="da05dcbb" sha1="c2ced1f3aee92b0e531d5cd7611d4811f2ae95e7" region="mainpcb:maincpu" offset="0" />
    <rom name="sonpg1.bin" size="131072" crc="c57dc5c5" sha1="5741bdd52ee7181d883129885838b36f4af8a04c" region="mainpcb:maincpu" offset="80000" />
    <rom name="sonpd0.bin" size="262144" crc="a7da7546" sha1="0a10573b21cd38d58380698bc18b0256dbb24044" region="mainpcb:maincpu" offset="100000" />
    <rom name="sonpd1.bin" size="262144" crc="c30e4c70" sha1="897b6f62921694fe3c63677908f76eaf38b7b92f" region="mainpcb:maincpu" offset="100001" />
    <rom name="sonsnd0.bin" size="262144" crc="569c8d4b" sha1="9f1f6da6adbea043cc5ad853806fcb7bf683c832" region="mainpcb:soundcpu" offset="0" />
    <rom name="sonsnd1.bin" size="1048576" crc="f4fa5a21" sha1="14a364ba7744ff0b44423d8d6bab990fe534ff29" region="mainpcb:soundcpu" offset="100000" />
    <rom name="sonsnd2.bin" size="1048576" crc="e1bd45a5" sha1="b411757853d61588e5223b48b5124cc00b3d65dd" region="mainpcb:soundcpu" offset="200000" />
    <rom name="sonsnd3.bin" merge="mpr-15782.ic33" size="1048576" crc="cf56b5a0" sha1="5786228aab120c3361524ba93b418b24fd5b8ffb" region="mainpcb:soundcpu" offset="300000" />
    <rom name="sonscl0.bin" size="524288" crc="445e31b9" sha1="5678dfda74a09b5ac673448b222d11df4ca23aff" region="mainpcb:gfx1" offset="0" />
    <rom name="sonscl1.bin" size="524288" crc="3d234181" sha1="2e8c14ad36be76f5f5fc6a3ee152f1abc8bf0ddd" region="mainpcb:gfx1" offset="2" />
    <rom name="sonscl2.bin" size="524288" crc="a5de28b2" sha1="49a16ac10cf01b5b8802b8b015a2e403086c206a" region="mainpcb:gfx1" offset="1" />
    <rom name="sonscl3.bin" size="524288" crc="7ce7554b" sha1="8def3acae6baafbe9e350f18e245a9a833df5cc4" region="mainpcb:gfx1" offset="3" />
    <rom name="sonobj0.bin" size="1048576" crc="ceea18e3" sha1="f902a7e2f8e126fd7a7862c55de32ce6352a7716" region="mainpcb:sprites" offset="0" />
    <rom name="sonobj1.bin" size="1048576" crc="6bbc226b" sha1="5ef4256b6a93891daf1349def6db3bc428e5f4f3" region="mainpcb:sprites" offset="1" />
    <rom name="sonobj2.bin" size="1048576" crc="fcd5ef0e" sha1="e3e50d4838ac3cce41d69ee6cd31981fbe422a4b" region="mainpcb:sprites" offset="2" />
    <rom name="sonobj3.bin" size="1048576" crc="b99b42ab" sha1="60d91dc4e8e0adc62809cd2e71833c658124fbfc" region="mainpcb:sprites" offset="3" />
    <rom name="sonobj4.bin" size="1048576" crc="c7ec1456" sha1="d866b9dff546bd6feb43e317328ac0a2324303b9" region="mainpcb:sprites" offset="4" />
    <rom name="sonobj5.bin" size="1048576" crc="bd5da27f" sha1="ab3043190a32b555513a29a70e01547daf698cf8" region="mainpcb:sprites" offset="5" />
    <rom name="sonobj6.bin" size="1048576" crc="313c92d1" sha1="a5134750667502811fd755cc0974a744cdb785e1" region="mainpcb:sprites" offset="6" />
    <rom name="sonobj7.bin" size="1048576" crc="3784c507" sha1="8ea58c52b09b84643218e26f1ec1fa0ea864346e" region="mainpcb:sprites" offset="7" />
    <device_ref name="segas32_pcb_trackball" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="upd4701a" />
    <device_ref name="upd4701a" />
    <device_ref name="upd4701a" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="3" coins="3" service="yes">
      <control type="trackball" player="1" buttons="1" minimum="0" maximum="4095" sensitivity="100" keydelta="30" reverse="yes" />
      <control type="trackball" player="2" buttons="1" minimum="0" maximum="4095" sensitivity="100" keydelta="30" reverse="yes" />
      <control type="trackball" player="3" buttons="1" minimum="0" maximum="4095" sensitivity="100" keydelta="30" reverse="yes" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:TRACKX1">
      <analog mask="4095" />
    </port>
    <port tag=":mainpcb:TRACKX2">
      <analog mask="4095" />
    </port>
    <port tag=":mainpcb:TRACKX3">
      <analog mask="4095" />
    </port>
    <port tag=":mainpcb:TRACKY1">
      <analog mask="4095" />
    </port>
    <port tag=":mainpcb:TRACKY2">
      <analog mask="4095" />
    </port>
    <port tag=":mainpcb:TRACKY3">
      <analog mask="4095" />
    </port>
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="spidman" sourcefile="segas32.cpp">
    <description>Spider-Man: The Videogame (World)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14307.ic13" size="131072" crc="d900219c" sha1="d59654db1fc0ec4d5f8cda9000ab4bd3bb36cdfc" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14306.ic7" size="131072" crc="64379dc6" sha1="7efc7175351186c54f141161a395e63b1cc7e7a5" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-14281.ic14" size="131072" crc="8a746c42" sha1="fa3729ec3aa4b3c59322408146ce2cfbf5a11b98" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14280.ic6" size="131072" crc="3c8148f7" sha1="072b7982bb95e7a9ab77844b59020146c262488d" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14285.ic35" size="262144" crc="25aefad6" sha1="10153f4e773a0f55378f869eb1d85156e85f893f" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14284.ic31" size="524288" crc="760542d4" sha1="dcac73869c02fefd328bd6bdbcbdb3b68b0647da" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14283.ic26" size="524288" crc="c863a91c" sha1="afdc76bbb9b207cfcb47d437248a757d03212f4e" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14282.ic22" size="524288" crc="ea20979e" sha1="9b70ef055da8c7c56da54b7edef2379678e7c50f" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14291-s.ic38" size="1048576" crc="490f95a1" sha1="f220788670b76164ac414ed9b16a422f719be267" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14290-s.ic34" size="1048576" crc="a144162d" sha1="d43f12dd9f690cdfcebb6c7b515ff7dc7dcaa377" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-14289-s.ic29" size="1048576" crc="38570582" sha1="a9d810a02a1f5a6849c79d65fbebff21a4b82b59" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14288-s.ic25" size="1048576" crc="3188b636" sha1="bc0adeeca5040caa563ee1e0eded9c323ca23446" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-14299-h.ic36" size="1048576" crc="ce59231b" sha1="bcb1f11b74935694d0617ec8df66db2cc57b6219" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14298-h.ic32" size="1048576" crc="2745c84c" sha1="5a0528c921cba7a1047d3a2ece79925103d719a1" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-14297-h.ic27" size="1048576" crc="29cb9450" sha1="7dc38d23a2f0cee2f4edde05c1a6f0dc83f331db" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14296-h.ic23" size="1048576" crc="9d8cbd31" sha1="55a9f9ec9029157da033e69664b58e694a28db47" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-14295-h.ic37" size="1048576" crc="29591f50" sha1="1ac4ceaf74892e30f210ad77024eb441c5e4a959" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14294-h.ic33" size="1048576" crc="fa86b794" sha1="7b6907e5734fbf2fba7bcc213a8551fec5e9f3d5" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-14293-s.ic28" size="1048576" crc="52899269" sha1="ff809ff88701109e0ca79e785a61402d97335cec" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14292-s.ic24" size="1048576" crc="41f71443" sha1="351d40d6159cb5b792519bce5d16490965800cfb" region="mainpcb:sprites" offset="7" />
    <device_ref name="segas32_pcb_4player" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="2" service="yes">
      <control type="joy" player="1" buttons="2" ways="8" />
      <control type="joy" player="2" buttons="2" ways="8" />
      <control type="joy" player="3" buttons="2" ways="8" />
      <control type="joy" player="4" buttons="2" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="spidmanj" sourcefile="segas32.cpp" cloneof="spidman" romof="spidman">
    <description>Spider-Man: The Videogame (Japan)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14287.ic13" size="131072" crc="403ccdc9" sha1="4e240c749e362dfa5c579ccbdff18ae3fab58dff" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14286.ic7" size="131072" crc="5c2b4e2c" sha1="79229594710416510f85e6e53ea578789afd4091" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-14281.ic14" merge="epr-14281.ic14" size="131072" crc="8a746c42" sha1="fa3729ec3aa4b3c59322408146ce2cfbf5a11b98" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14280.ic6" merge="epr-14280.ic6" size="131072" crc="3c8148f7" sha1="072b7982bb95e7a9ab77844b59020146c262488d" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14285.ic35" merge="epr-14285.ic35" size="262144" crc="25aefad6" sha1="10153f4e773a0f55378f869eb1d85156e85f893f" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14284.ic31" merge="mpr-14284.ic31" size="524288" crc="760542d4" sha1="dcac73869c02fefd328bd6bdbcbdb3b68b0647da" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14283.ic26" merge="mpr-14283.ic26" size="524288" crc="c863a91c" sha1="afdc76bbb9b207cfcb47d437248a757d03212f4e" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14282.ic22" merge="mpr-14282.ic22" size="524288" crc="ea20979e" sha1="9b70ef055da8c7c56da54b7edef2379678e7c50f" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14291-s.ic38" merge="mpr-14291-s.ic38" size="1048576" crc="490f95a1" sha1="f220788670b76164ac414ed9b16a422f719be267" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14290-s.ic34" merge="mpr-14290-s.ic34" size="1048576" crc="a144162d" sha1="d43f12dd9f690cdfcebb6c7b515ff7dc7dcaa377" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-14289-s.ic29" merge="mpr-14289-s.ic29" size="1048576" crc="38570582" sha1="a9d810a02a1f5a6849c79d65fbebff21a4b82b59" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14288-s.ic25" merge="mpr-14288-s.ic25" size="1048576" crc="3188b636" sha1="bc0adeeca5040caa563ee1e0eded9c323ca23446" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-14299-h.ic36" merge="mpr-14299-h.ic36" size="1048576" crc="ce59231b" sha1="bcb1f11b74935694d0617ec8df66db2cc57b6219" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14298-h.ic32" merge="mpr-14298-h.ic32" size="1048576" crc="2745c84c" sha1="5a0528c921cba7a1047d3a2ece79925103d719a1" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-14297-h.ic27" merge="mpr-14297-h.ic27" size="1048576" crc="29cb9450" sha1="7dc38d23a2f0cee2f4edde05c1a6f0dc83f331db" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14296-h.ic23" merge="mpr-14296-h.ic23" size="1048576" crc="9d8cbd31" sha1="55a9f9ec9029157da033e69664b58e694a28db47" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-14295-h.ic37" merge="mpr-14295-h.ic37" size="1048576" crc="29591f50" sha1="1ac4ceaf74892e30f210ad77024eb441c5e4a959" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14294-h.ic33" merge="mpr-14294-h.ic33" size="1048576" crc="fa86b794" sha1="7b6907e5734fbf2fba7bcc213a8551fec5e9f3d5" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-14293-s.ic28" merge="mpr-14293-s.ic28" size="1048576" crc="52899269" sha1="ff809ff88701109e0ca79e785a61402d97335cec" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14292-s.ic24" merge="mpr-14292-s.ic24" size="1048576" crc="41f71443" sha1="351d40d6159cb5b792519bce5d16490965800cfb" region="mainpcb:sprites" offset="7" />
    <device_ref name="segas32_pcb_4player" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="2" service="yes">
      <control type="joy" player="1" buttons="2" ways="8" />
      <control type="joy" player="2" buttons="2" ways="8" />
      <control type="joy" player="3" buttons="2" ways="8" />
      <control type="joy" player="4" buttons="2" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="spidmanu" sourcefile="segas32.cpp" cloneof="spidman" romof="spidman">
    <description>Spider-Man: The Videogame (US, Rev A)</description>
    <year>1991</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-14303a.ic13" size="131072" crc="7f1bd28f" sha1="cff57e66d09682baf44aace99d698ad305f6a3d5" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-14302a.ic7" size="131072" crc="d954c40a" sha1="436c81779274861de79dc6ce2c0fcc65bfd52098" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-14281.ic14" merge="epr-14281.ic14" size="131072" crc="8a746c42" sha1="fa3729ec3aa4b3c59322408146ce2cfbf5a11b98" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-14280.ic6" merge="epr-14280.ic6" size="131072" crc="3c8148f7" sha1="072b7982bb95e7a9ab77844b59020146c262488d" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-14285.ic35" merge="epr-14285.ic35" size="262144" crc="25aefad6" sha1="10153f4e773a0f55378f869eb1d85156e85f893f" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-14284.ic31" merge="mpr-14284.ic31" size="524288" crc="760542d4" sha1="dcac73869c02fefd328bd6bdbcbdb3b68b0647da" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-14283.ic26" merge="mpr-14283.ic26" size="524288" crc="c863a91c" sha1="afdc76bbb9b207cfcb47d437248a757d03212f4e" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-14282.ic22" merge="mpr-14282.ic22" size="524288" crc="ea20979e" sha1="9b70ef055da8c7c56da54b7edef2379678e7c50f" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-14291-s.ic38" merge="mpr-14291-s.ic38" size="1048576" crc="490f95a1" sha1="f220788670b76164ac414ed9b16a422f719be267" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-14290-s.ic34" merge="mpr-14290-s.ic34" size="1048576" crc="a144162d" sha1="d43f12dd9f690cdfcebb6c7b515ff7dc7dcaa377" region="mainpcb:gfx1" offset="2" />
    <rom name="mpr-14289-s.ic29" merge="mpr-14289-s.ic29" size="1048576" crc="38570582" sha1="a9d810a02a1f5a6849c79d65fbebff21a4b82b59" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-14288-s.ic25" merge="mpr-14288-s.ic25" size="1048576" crc="3188b636" sha1="bc0adeeca5040caa563ee1e0eded9c323ca23446" region="mainpcb:gfx1" offset="3" />
    <rom name="mpr-14299-h.ic36" merge="mpr-14299-h.ic36" size="1048576" crc="ce59231b" sha1="bcb1f11b74935694d0617ec8df66db2cc57b6219" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-14298-h.ic32" merge="mpr-14298-h.ic32" size="1048576" crc="2745c84c" sha1="5a0528c921cba7a1047d3a2ece79925103d719a1" region="mainpcb:sprites" offset="1" />
    <rom name="mpr-14297-h.ic27" merge="mpr-14297-h.ic27" size="1048576" crc="29cb9450" sha1="7dc38d23a2f0cee2f4edde05c1a6f0dc83f331db" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-14296-h.ic23" merge="mpr-14296-h.ic23" size="1048576" crc="9d8cbd31" sha1="55a9f9ec9029157da033e69664b58e694a28db47" region="mainpcb:sprites" offset="3" />
    <rom name="mpr-14295-h.ic37" merge="mpr-14295-h.ic37" size="1048576" crc="29591f50" sha1="1ac4ceaf74892e30f210ad77024eb441c5e4a959" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-14294-h.ic33" merge="mpr-14294-h.ic33" size="1048576" crc="fa86b794" sha1="7b6907e5734fbf2fba7bcc213a8551fec5e9f3d5" region="mainpcb:sprites" offset="5" />
    <rom name="mpr-14293-s.ic28" merge="mpr-14293-s.ic28" size="1048576" crc="52899269" sha1="ff809ff88701109e0ca79e785a61402d97335cec" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-14292-s.ic24" merge="mpr-14292-s.ic24" size="1048576" crc="41f71443" sha1="351d40d6159cb5b792519bce5d16490965800cfb" region="mainpcb:sprites" offset="7" />
    <device_ref name="segas32_pcb_4player" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <device_ref name="i8255" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="4" coins="4" service="yes">
      <control type="joy" player="1" buttons="2" ways="8" />
      <control type="joy" player="2" buttons="2" ways="8" />
      <control type="joy" player="3" buttons="2" ways="8" />
      <control type="joy" player="4" buttons="2" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:EXTRA1" />
    <port tag=":mainpcb:EXTRA2" />
    <port tag=":mainpcb:EXTRA3" />
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="svf" sourcefile="segas32.cpp">
    <description>Super Visual Football: European Sega Cup (Rev A)</description>
    <year>1994</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16872a.ic17" size="131072" crc="1f383b00" sha1="c3af01743de5ff09ada19879902842efdbceb595" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16871a.ic8" size="131072" crc="f7061bd7" sha1="b46f4f2ecda8f521c0a91f2f2c2445b72cbc2874" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-16865.ic18" size="524288" crc="9198ca9f" sha1="0f6271ce8a07e4ab7fdce38964055510f2ebfd4e" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-16864.ic9" size="524288" crc="201a940e" sha1="e19d76141844dbdedee0698ea50edbb898ab55e9" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-16866.ic36" size="131072" crc="74431350" sha1="d3208b595423b5b0f25ee90db213112a09906f8f" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16779.ic35" size="1048576" crc="7055e859" sha1="cde27fa4aaf0ee54063ee68794e9a6075581fff5" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16778.ic34" size="1048576" crc="feedaecf" sha1="25c14ccb85c467dc0c8e85b61f8f86f4396c0cc7" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-16777.ic24" size="1048576" crc="14b5d5df" sha1="1b0b0a31294b1bbc16d2046b374d584a1b00a78c" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-16784.ic14" size="1048576" crc="4608efe2" sha1="9b41aa28f50af770e854ef9fdff1a55da7b7b131" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16783.ic5" size="1048576" crc="042eabe7" sha1="a11df5c21d85f0c96dbdcaf57be37a79658ad648" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16785.ic32" size="2097152" crc="51f775ce" sha1="125b40bf47304d37b92e81df5081c81d9af6c8a2" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16787.ic30" size="2097152" crc="dee7a204" sha1="29acff4d5dd68609ac46853860788206d18262ab" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16789.ic28" size="2097152" crc="6b6c8ad3" sha1="97b0078c851845c31dcf0fe4b2a88393dcdf8988" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16791.ic26" size="2097152" crc="4f7236da" sha1="d1c29f6aa82d60a626217f1430bc8a76ef012007" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16860.ic31" size="2097152" crc="578a7325" sha1="75a066841fa24952d8ed5ac2d988609295f437a8" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16861.ic29" size="2097152" crc="d79c3f73" sha1="e4360efb0964a92cfad8c458a5568709fcc81339" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16862.ic27" size="2097152" crc="00793354" sha1="3b37a89c5100d5f92a3567fc8d2003bc9d6fe0cd" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16863.ic25" size="2097152" crc="42338226" sha1="106636408d5648fb95fbaee06074c57f6a535a82" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_regular" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="3" ways="8" />
      <control type="joy" player="2" buttons="3" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="svfo" sourcefile="segas32.cpp" cloneof="svf" romof="svf">
    <description>Super Visual Football: European Sega Cup</description>
    <year>1994</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16872.ic17" size="131072" crc="654d8c95" sha1="0d28d6d8814c07e98fb9c50bd3ecbe17a9dee70a" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16871.ic8" size="131072" crc="e0d0cac0" sha1="e9a7d0878a38b93681497489a2366f7337a1abf5" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-16865.ic18" merge="epr-16865.ic18" size="524288" crc="9198ca9f" sha1="0f6271ce8a07e4ab7fdce38964055510f2ebfd4e" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-16864.ic9" merge="epr-16864.ic9" size="524288" crc="201a940e" sha1="e19d76141844dbdedee0698ea50edbb898ab55e9" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-16866.ic36" merge="epr-16866.ic36" size="131072" crc="74431350" sha1="d3208b595423b5b0f25ee90db213112a09906f8f" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16779.ic35" merge="mpr-16779.ic35" size="1048576" crc="7055e859" sha1="cde27fa4aaf0ee54063ee68794e9a6075581fff5" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16778.ic34" merge="mpr-16778.ic34" size="1048576" crc="feedaecf" sha1="25c14ccb85c467dc0c8e85b61f8f86f4396c0cc7" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-16777.ic24" merge="mpr-16777.ic24" size="1048576" crc="14b5d5df" sha1="1b0b0a31294b1bbc16d2046b374d584a1b00a78c" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-16784.ic14" merge="mpr-16784.ic14" size="1048576" crc="4608efe2" sha1="9b41aa28f50af770e854ef9fdff1a55da7b7b131" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16783.ic5" merge="mpr-16783.ic5" size="1048576" crc="042eabe7" sha1="a11df5c21d85f0c96dbdcaf57be37a79658ad648" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16785.ic32" merge="mpr-16785.ic32" size="2097152" crc="51f775ce" sha1="125b40bf47304d37b92e81df5081c81d9af6c8a2" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16787.ic30" merge="mpr-16787.ic30" size="2097152" crc="dee7a204" sha1="29acff4d5dd68609ac46853860788206d18262ab" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16789.ic28" merge="mpr-16789.ic28" size="2097152" crc="6b6c8ad3" sha1="97b0078c851845c31dcf0fe4b2a88393dcdf8988" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16791.ic26" merge="mpr-16791.ic26" size="2097152" crc="4f7236da" sha1="d1c29f6aa82d60a626217f1430bc8a76ef012007" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16860.ic31" merge="mpr-16860.ic31" size="2097152" crc="578a7325" sha1="75a066841fa24952d8ed5ac2d988609295f437a8" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16861.ic29" merge="mpr-16861.ic29" size="2097152" crc="d79c3f73" sha1="e4360efb0964a92cfad8c458a5568709fcc81339" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16862.ic27" merge="mpr-16862.ic27" size="2097152" crc="00793354" sha1="3b37a89c5100d5f92a3567fc8d2003bc9d6fe0cd" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16863.ic25" merge="mpr-16863.ic25" size="2097152" crc="42338226" sha1="106636408d5648fb95fbaee06074c57f6a535a82" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_regular" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="3" ways="8" />
      <control type="joy" player="2" buttons="3" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="svs" sourcefile="segas32.cpp" cloneof="svf" romof="svf">
    <description>Super Visual Soccer: Sega Cup (US, Rev A)</description>
    <year>1994</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-16883a.ic17" size="131072" crc="e1c0c3ce" sha1="12dd8d9d1a2c2c7bf1ab652a6a6f947384d79577" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-16882a.ic8" size="131072" crc="1161bbbe" sha1="3cfeed9ea947eed79aeb5674d54de45d15fb6e1f" region="mainpcb:maincpu" offset="80000" />
    <rom name="epr-16865.ic18" merge="epr-16865.ic18" size="524288" crc="9198ca9f" sha1="0f6271ce8a07e4ab7fdce38964055510f2ebfd4e" region="mainpcb:maincpu" offset="100000" />
    <rom name="epr-16864.ic9" merge="epr-16864.ic9" size="524288" crc="201a940e" sha1="e19d76141844dbdedee0698ea50edbb898ab55e9" region="mainpcb:maincpu" offset="100001" />
    <rom name="epr-16868.ic36" size="262144" crc="47aa4ec7" sha1="baea18aaac0314f769f1e36fdbe8aedf62862544" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-16779.ic35" merge="mpr-16779.ic35" size="1048576" crc="7055e859" sha1="cde27fa4aaf0ee54063ee68794e9a6075581fff5" region="mainpcb:soundcpu" offset="100000" />
    <rom name="mpr-16778.ic34" merge="mpr-16778.ic34" size="1048576" crc="feedaecf" sha1="25c14ccb85c467dc0c8e85b61f8f86f4396c0cc7" region="mainpcb:soundcpu" offset="200000" />
    <rom name="mpr-16777.ic24" merge="mpr-16777.ic24" size="1048576" crc="14b5d5df" sha1="1b0b0a31294b1bbc16d2046b374d584a1b00a78c" region="mainpcb:soundcpu" offset="300000" />
    <rom name="mpr-16784.ic14" merge="mpr-16784.ic14" size="1048576" crc="4608efe2" sha1="9b41aa28f50af770e854ef9fdff1a55da7b7b131" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-16783.ic5" merge="mpr-16783.ic5" size="1048576" crc="042eabe7" sha1="a11df5c21d85f0c96dbdcaf57be37a79658ad648" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-16785.ic32" merge="mpr-16785.ic32" size="2097152" crc="51f775ce" sha1="125b40bf47304d37b92e81df5081c81d9af6c8a2" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-16787.ic30" merge="mpr-16787.ic30" size="2097152" crc="dee7a204" sha1="29acff4d5dd68609ac46853860788206d18262ab" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-16789.ic28" merge="mpr-16789.ic28" size="2097152" crc="6b6c8ad3" sha1="97b0078c851845c31dcf0fe4b2a88393dcdf8988" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-16791.ic26" merge="mpr-16791.ic26" size="2097152" crc="4f7236da" sha1="d1c29f6aa82d60a626217f1430bc8a76ef012007" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-16860.ic31" merge="mpr-16860.ic31" size="2097152" crc="578a7325" sha1="75a066841fa24952d8ed5ac2d988609295f437a8" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-16861.ic29" merge="mpr-16861.ic29" size="2097152" crc="d79c3f73" sha1="e4360efb0964a92cfad8c458a5568709fcc81339" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-16862.ic27" merge="mpr-16862.ic27" size="2097152" crc="00793354" sha1="3b37a89c5100d5f92a3567fc8d2003bc9d6fe0cd" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-16863.ic25" merge="mpr-16863.ic25" size="2097152" crc="42338226" sha1="106636408d5648fb95fbaee06074c57f6a535a82" region="mainpcb:sprites" offset="800006" />
    <device_ref name="segas32_pcb_regular" />
    <device_ref name="v60" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ym3438" />
    <device_ref name="rf5c68" />
    <device_ref name="s32comm" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V60" clock="16107950" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ym1" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:ym2" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:rfsnd" name="Ricoh RF5C68" clock="12500000" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="joy" player="1" buttons="3" ways="8" />
      <control type="joy" player="2" buttons="3" ways="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE34_A" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="titlef" sourcefile="segas32.cpp">
    <description>Title Fight (World)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15388.ic37" size="262144" crc="db1eefbd" sha1="7059a1d5c9364d836c1d922071a108cbde661e0a" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15389.ic40" size="262144" crc="da9f60a3" sha1="87a7bea04e51e3c241871e83ff7322c6a07bd106" region="mainpcb:maincpu" offset="2" />
    <rom name="epr-15384.ic31" size="131072" crc="0f7d208d" sha1="5425120480f813210fae28951e8bfd5acb08ca53" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15381.ic3" size="2097152" crc="162cc4d6" sha1="2369d3d76ab5ef8f033aa45530ab957f0e5ff028" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15382.ic11" size="2097152" crc="fd03a130" sha1="040c36383ef5d8298af714958cd5b0a4c7556ae7" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15379.ic14" size="2097152" crc="e5c74b11" sha1="67e4460efe5dcd88ffc12024b255efc843e6a8b5" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15375.ic15" size="2097152" crc="046a9b50" sha1="2b4c53f2a0264835cb7197daa9b3461c212541e8" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15371.ic10" size="2097152" crc="999046c6" sha1="37ce4e8aaf537b5366eacabaf36e4477b5624121" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15373.ic38" size="2097152" crc="9b3294d9" sha1="19542f14ce09753385a44098dfd1aaf331e7af0e" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15380.ic22" size="2097152" crc="6ea0e58d" sha1="1c4b761522157b0b9d086181ba6f6994879d8fdf" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15376.ic23" size="2097152" crc="de3e05c5" sha1="cac0d04ecd37e5836d246c0809bcfc11430df591" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15372.ic18" size="2097152" crc="c187c36a" sha1="bb55c2a768a43ef19a7847a4aa113523fee26c20" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15374.ic41" size="2097152" crc="e026aab0" sha1="75dfaef6d50c3d1d7f27aa5e44fcbc0ff2173c6f" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-15385.ic1" size="2097152" crc="5a9b0aa0" sha1="d208aa165f9eea05e3b8c3f406ff44374e4f6887" region="mainpcb:sega" offset="0" />
    <device_ref name="segas32_pcb_multi" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="doublejoy" player="1" ways="8" ways2="8" />
      <control type="doublejoy" player="2" ways="8" ways2="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="titlefj" sourcefile="segas32.cpp" cloneof="titlef" romof="titlef">
    <description>Title Fight (Japan)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15377.ic37" size="262144" crc="1868403c" sha1="d34a3a05e5a3bb2e6159f95d1e22d264bf553cda" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15378.ic40" size="262144" crc="44487b0a" sha1="4aefd063bf148334d5f43d69f497766d50ffca30" region="mainpcb:maincpu" offset="2" />
    <rom name="epr-15384.ic31" merge="epr-15384.ic31" size="131072" crc="0f7d208d" sha1="5425120480f813210fae28951e8bfd5acb08ca53" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15381.ic3" merge="mpr-15381.ic3" size="2097152" crc="162cc4d6" sha1="2369d3d76ab5ef8f033aa45530ab957f0e5ff028" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15382.ic11" merge="mpr-15382.ic11" size="2097152" crc="fd03a130" sha1="040c36383ef5d8298af714958cd5b0a4c7556ae7" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15379.ic14" merge="mpr-15379.ic14" size="2097152" crc="e5c74b11" sha1="67e4460efe5dcd88ffc12024b255efc843e6a8b5" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15375.ic15" merge="mpr-15375.ic15" size="2097152" crc="046a9b50" sha1="2b4c53f2a0264835cb7197daa9b3461c212541e8" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15371.ic10" merge="mpr-15371.ic10" size="2097152" crc="999046c6" sha1="37ce4e8aaf537b5366eacabaf36e4477b5624121" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15373.ic38" merge="mpr-15373.ic38" size="2097152" crc="9b3294d9" sha1="19542f14ce09753385a44098dfd1aaf331e7af0e" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15380.ic22" merge="mpr-15380.ic22" size="2097152" crc="6ea0e58d" sha1="1c4b761522157b0b9d086181ba6f6994879d8fdf" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15376.ic23" merge="mpr-15376.ic23" size="2097152" crc="de3e05c5" sha1="cac0d04ecd37e5836d246c0809bcfc11430df591" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15372.ic18" merge="mpr-15372.ic18" size="2097152" crc="c187c36a" sha1="bb55c2a768a43ef19a7847a4aa113523fee26c20" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15374.ic41" merge="mpr-15374.ic41" size="2097152" crc="e026aab0" sha1="75dfaef6d50c3d1d7f27aa5e44fcbc0ff2173c6f" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-15385.ic1" merge="mpr-15385.ic1" size="2097152" crc="5a9b0aa0" sha1="d208aa165f9eea05e3b8c3f406ff44374e4f6887" region="mainpcb:sega" offset="0" />
    <device_ref name="segas32_pcb_multi" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="doublejoy" player="1" ways="8" ways2="8" />
      <control type="doublejoy" player="2" ways="8" ways2="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
  <machine name="titlefu" sourcefile="segas32.cpp" cloneof="titlef" romof="titlef">
    <description>Title Fight (US)</description>
    <year>1992</year>
    <manufacturer>Sega</manufacturer>
    <rom name="epr-15386.ic37" size="262144" crc="e36e2516" sha1="b6a73d6136ff8a13831b6db0fbc8a585f2acf254" region="mainpcb:maincpu" offset="0" />
    <rom name="epr-15387.ic40" size="262144" crc="e63406d3" sha1="cd105862b2267d1d3af588cda70e6e4c1cca1da2" region="mainpcb:maincpu" offset="2" />
    <rom name="epr-15384.ic31" merge="epr-15384.ic31" size="131072" crc="0f7d208d" sha1="5425120480f813210fae28951e8bfd5acb08ca53" region="mainpcb:soundcpu" offset="0" />
    <rom name="mpr-15381.ic3" merge="mpr-15381.ic3" size="2097152" crc="162cc4d6" sha1="2369d3d76ab5ef8f033aa45530ab957f0e5ff028" region="mainpcb:gfx1" offset="0" />
    <rom name="mpr-15382.ic11" merge="mpr-15382.ic11" size="2097152" crc="fd03a130" sha1="040c36383ef5d8298af714958cd5b0a4c7556ae7" region="mainpcb:gfx1" offset="1" />
    <rom name="mpr-15379.ic14" merge="mpr-15379.ic14" size="2097152" crc="e5c74b11" sha1="67e4460efe5dcd88ffc12024b255efc843e6a8b5" region="mainpcb:sprites" offset="0" />
    <rom name="mpr-15375.ic15" merge="mpr-15375.ic15" size="2097152" crc="046a9b50" sha1="2b4c53f2a0264835cb7197daa9b3461c212541e8" region="mainpcb:sprites" offset="2" />
    <rom name="mpr-15371.ic10" merge="mpr-15371.ic10" size="2097152" crc="999046c6" sha1="37ce4e8aaf537b5366eacabaf36e4477b5624121" region="mainpcb:sprites" offset="4" />
    <rom name="mpr-15373.ic38" merge="mpr-15373.ic38" size="2097152" crc="9b3294d9" sha1="19542f14ce09753385a44098dfd1aaf331e7af0e" region="mainpcb:sprites" offset="6" />
    <rom name="mpr-15380.ic22" merge="mpr-15380.ic22" size="2097152" crc="6ea0e58d" sha1="1c4b761522157b0b9d086181ba6f6994879d8fdf" region="mainpcb:sprites" offset="800000" />
    <rom name="mpr-15376.ic23" merge="mpr-15376.ic23" size="2097152" crc="de3e05c5" sha1="cac0d04ecd37e5836d246c0809bcfc11430df591" region="mainpcb:sprites" offset="800002" />
    <rom name="mpr-15372.ic18" merge="mpr-15372.ic18" size="2097152" crc="c187c36a" sha1="bb55c2a768a43ef19a7847a4aa113523fee26c20" region="mainpcb:sprites" offset="800004" />
    <rom name="mpr-15374.ic41" merge="mpr-15374.ic41" size="2097152" crc="e026aab0" sha1="75dfaef6d50c3d1d7f27aa5e44fcbc0ff2173c6f" region="mainpcb:sprites" offset="800006" />
    <rom name="mpr-15385.ic1" merge="mpr-15385.ic1" size="2097152" crc="5a9b0aa0" sha1="d208aa165f9eea05e3b8c3f406ff44374e4f6887" region="mainpcb:sega" offset="0" />
    <device_ref name="segas32_pcb_multi" />
    <device_ref name="v70" />
    <device_ref name="z80" />
    <device_ref name="315_5296" />
    <device_ref name="315_5296" />
    <device_ref name="93c46_16" />
    <device_ref name="timer" />
    <device_ref name="timer" />
    <device_ref name="gfxdecode" />
    <device_ref name="palette" />
    <device_ref name="screen" />
    <device_ref name="screen" />
    <device_ref name="speaker" />
    <device_ref name="speaker" />
    <device_ref name="ym3438" />
    <device_ref name="ymw258f" />
    <device_ref name="s32comm" />
    <chip type="cpu" tag="mainpcb:maincpu" name="NEC V70" clock="20000000" />
    <chip type="cpu" tag="mainpcb:soundcpu" name="Zilog Z80" clock="8053975" />
    <chip type="audio" tag="mainpcb:lspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:rspeaker" name="Speaker" />
    <chip type="audio" tag="mainpcb:ymsnd" name="YM3438 OPN2C" clock="8053975" />
    <chip type="audio" tag="mainpcb:sega" name="Yamaha YMW-258-F" clock="8053975" />
    <display tag="mainpcb:screen" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <display tag="mainpcb:screen2" type="raster" rotate="0" width="416" height="224" refresh="60.000000" pixclock="6539520" htotal="416" hbend="0" hbstart="416" vtotal="262" vbend="0" vbstart="224" />
    <sound channels="2" />
    <input players="2" coins="2" service="yes">
      <control type="doublejoy" player="1" ways="8" ways2="8" />
      <control type="doublejoy" player="2" ways="8" ways2="8" />
    </input>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="1">
      <diplocation name="SW1" number="1" />
      <dipvalue name="Off" value="1" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="2">
      <diplocation name="SW1" number="2" />
      <dipvalue name="Off" value="2" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="4">
      <diplocation name="SW1" number="3" />
      <dipvalue name="Off" value="4" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <dipswitch name="Unknown" tag="mainpcb:SERVICE34_A" mask="8">
      <diplocation name="SW1" number="4" />
      <dipvalue name="Off" value="8" default="yes" />
      <dipvalue name="On" value="0" />
    </dipswitch>
    <port tag=":mainpcb:P1_A" />
    <port tag=":mainpcb:P1_B" />
    <port tag=":mainpcb:P2_A" />
    <port tag=":mainpcb:P2_B" />
    <port tag=":mainpcb:PORTC_A" />
    <port tag=":mainpcb:PORTC_B" />
    <port tag=":mainpcb:SERVICE12_A" />
    <port tag=":mainpcb:SERVICE12_B" />
    <port tag=":mainpcb:SERVICE34_A" />
    <port tag=":mainpcb:SERVICE34_B" />
    <driver status="imperfect" emulation="good" savestate="unsupported" />
    <feature type="graphics" status="imperfect" />
  </machine>
</datafile>